Package pygeodesy :: Module mgrs :: Class Mgrs |
[frames] | no frames]

# Class Mgrs

      object --+
               |
    named._Named --+
                   |
    named._NamedBase --+
                       |
                      Mgrs

Military Grid Reference System (MGRS/NATO) references, with method to convert to UTM coordinates.

Instance Methods
__init__(self, zone, en100k, easting, northing, band=`'````'`, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Tran`...`, name=`'````'`) New Mgrs Military grid reference. |
parse(self, strMGRS, name=`'````'`) Parse a string to a similar Mgrs instance. |
toRepr(self, prec=10, fmt=`'``[%s]``'`, sep=`'``,` `'`) Return a string representation of this MGRS grid reference. |
toStr(self, prec=10, sep=`'``` `'`) Return a string representation of this MGRS grid reference. |
toUtm(self, Utm=<class 'pygeodesy.utm.Utm'>) Convert this MGRS grid reference to a UTM coordinate. |
Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others` Inherited from `named._Named`: `_dot_`, `attrs`, `classof`, `copy`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
| band Get the latitudinal band (`str, 'A'|'B'..'Y'|'Z'`).
| bandLatitude Get the band latitude (`degrees90` or `None`).
| datum Get the datum (Datum).
| en100k Get the 2-character grid EN digraph (`str`).
| digraph Get the 2-character grid EN digraph (`str`).
| easting Gets the easting (`meter`).
| northing Get the northing (`meter`).
| zone Get the longitudal zone (`int`, 1..60).
Inherited from `named._Named`: `classname`, `classnaming`, `name`, `named`, `named2` Inherited from `object`: `__class__`

Method Details

### __init__ (self, zone, en100k, easting, northing, band=`'````'`, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Tran`...`, name=`'````'`) (Constructor) |
New Mgrs Military grid reference. Arguments: `zone` - 6° longitudinal zone (`int`), 1..60 covering 180°W..180°E. `en100k` - Two-letter EN digraph (`str`), 100 km grid square. `easting` - Easting (`meter`), within 100 km grid square. `northing` - Northing (`meter`), within 100 km grid square. `band` - Optional 8° latitudinal band (`str`), C..X covering 80°S..84°N. `datum` - Optional this reference's datum (Datum). `name` - Optional name (`str`). Raises: `MGRSError` - Invalid MGRS grid reference, `zone`, `en100k`, `easting`, `northing` or `band`. Overrides: object.__init__ Example:
    >>> from pygeodesy import Mgrs
    >>> m = Mgrs('31U', 'DQ', 48251, 11932)  # 31U DQ 48251 11932

### parse (self, strMGRS, name=`'````'`) |
Parse a string to a similar Mgrs instance. Arguments: `strMGRS` - The MGRS reference (`str`), see function parseMGRS. `name` - Optional instance name (`str`), overriding this name. Returns: The similar instance (Mgrs). Raises: `MGRSError` - Invalid `strMGRS`.

### toRepr (self, prec=10, fmt=`'``[%s]``'`, sep=`'``,` `'`) |
Return a string representation of this MGRS grid reference. Arguments: `prec` - Optional number of digits (`int`), 4:km, 10:m. `fmt` - Optional enclosing backets format (`str`). `sep` - Optional separator between name:values (`str`). Returns: This Mgrs as "[Z:00B, G:EN, E:meter, N:meter]" (`str`). Overrides: named._Named.toRepr

### toStr (self, prec=10, sep=`'``` `'`) |
Return a string representation of this MGRS grid reference. Note that MGRS grid references are truncated, not rounded (unlike UTM coordinates). Arguments: `prec` - Optional number of digits (`int`), 4:km, 10:m. `sep` - Optional separator to join (`str`) or `None` to return an unjoined `tuple` of `str`s. Returns: This Mgrs as "00B EN easting northing" (`str`). Raises: `ValueError` - Invalid `prec`. Overrides: named._Named.toStr Example:
    >>> m = Mgrs(31, 'DQ', 48251, 11932, band='U')
    >>> m.toStr()  # '31U DQ 48251 11932'

### toUtm (self, Utm=<class 'pygeodesy.utm.Utm'>) |
Convert this MGRS grid reference to a UTM coordinate. Arguments: `Utm` - Optional class to return the UTM coordinate (Utm) or `None`. Returns: The UTM coordinate (Utm) or a UtmUps5Tuple`(zone, hemipole, easting, northing, band)` if `Utm` is `None`. Example:
    >>> m = Mgrs('31U', 'DQ', 448251, 11932)
    >>> u = m.toUtm()  # 31 N 448251 5411932
    >>> u = m.toUtm(None)  # 31 N 448251 5411932 U

Property Details

### band Get the latitudinal band (`str, 'A'|'B'..'Y'|'Z'`). Get method: band(self) - Get the latitudinal band (`str, 'A'|'B'..'Y'|'Z'`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### bandLatitude Get the band latitude (`degrees90` or `None`). Get method: bandLatitude(self) - Get the band latitude (`degrees90` or `None`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### datum Get the datum (Datum). Get method: datum(self) - Get the datum (Datum). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### en100k Get the 2-character grid EN digraph (`str`). Get method: en100k(self) - Get the 2-character grid EN digraph (`str`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### digraph Get the 2-character grid EN digraph (`str`). Get method: en100k(self) - Get the 2-character grid EN digraph (`str`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### easting Gets the easting (`meter`). Get method: easting(self) - Gets the easting (`meter`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### northing Get the northing (`meter`). Get method: northing(self) - Get the northing (`meter`). Set method: immutable(inst, value) - Throws an `AttributeError`, always.

### zone Get the longitudal zone (`int`, 1..60). Get method: zone(self) - Get the longitudal zone (`int`, 1..60). Set method: immutable(inst, value) - Throws an `AttributeError`, always.