# Coverage for pygeodesy/dms.py : 92%

## 201 statements 184 run 17 missing 12 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 | # -*- coding: utf-8 -*- u'''Functions to parse and format bearing, compass, lat- and longitudes in various forms of degrees, minutes and seconds. After I{(C) Chris Veness 2011-2015} published under the same MIT Licence**, see U{Latitude/Longitude<https://www.Movable-Type.co.UK/scripts/latlong.html>} and U{Vector-based geodesy<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}. @newfield example: Example, Examples ''' from pygeodesy.fmath import fStr, fStrzs, isint from pygeodesy.lazily import _ALL_LAZY from pygeodesy.named import LatLon2Tuple, LatLon3Tuple from math import copysign, radians try: from string import letters as _LETTERS except ImportError: # Python 3+ from string import ascii_letters as _LETTERS # all public contants, classes and functions __all__ = _ALL_LAZY.dms __version__ = '19.09.07' F_D = 'd' #: Format degrees as unsigned "deg°" plus suffix (C{str}). F_DM = 'dm' #: Format degrees as unsigned "deg°min′" plus suffix (C{str}). F_DMS = 'dms' #: Format degrees as unsigned "deg°min′sec″" plus suffix (C{str}). F_DEG = 'deg' #: Format degrees as unsigned "[D]DD" plus suffix without symbol (C{str}). F_MIN = 'min' #: Format degrees as unsigned "[D]DDMM" plus suffix without symbols (C{str}). F_SEC = 'sec' #: Format degrees as unsigned "[D]DDMMSS" plus suffix without symbols (C{str}). F_RAD = 'rad' #: Convert degrees to radians and format as unsigned "RR" plus suffix (C{str}). F_D_ = '-d' #: Format degrees as signed "-/deg°" without suffix (C{str}). F_DM_ = '-dm' #: Format degrees as signed "-/deg°min′" without suffix (C{str}). F_DMS_ = '-dms' #: Format degrees as signed "-/deg°min′sec″" without suffix (C{str}). F_DEG_ = '-deg' #: Format degrees as signed "-/[D]DD" without suffix and symbol (C{str}). F_MIN_ = '-min' #: Format degrees as signed "-/[D]DDMM" without suffix and symbols (C{str}). F_SEC_ = '-sec' #: Format degrees as signed "-/[D]DDMMSS" without suffix and symbols (C{str}). F_RAD_ = '-rad' #: Convert degrees to radians and format as signed "-/RR" without suffix (C{str}). F_D__ = '+d' #: Format degrees as signed "-/+deg°" without suffix (C{str}). F_DM__ = '+dm' #: Format degrees as signed "-/+deg°min′" without suffix (C{str}). F_DMS__ = '+dms' #: Format degrees as signed "-/+deg°min′sec″" without suffix (C{str}). F_DEG__ = '+deg' #: Format degrees as signed "-/+[D]DD" without suffix and symbol (C{str}). F_MIN__ = '+min' #: Format degrees as signed "-/+[D]DDMM" without suffix and symbols (C{str}). F_SEC__ = '+sec' #: Format degrees as signed "-/+[D]DDMMSS" without suffix and symbols (C{str}). F_RAD__ = '+rad' #: Convert degrees to radians and format as signed "-/+RR" without suffix (C{str}). S_DEG = '°' #: Degrees "°" symbol (C{str}). S_MIN = '′' #: Minutes "′" symbol (C{str}). S_SEC = '″' #: Seconds "″" symbol (C{str}). S_RAD = '' #: Radians symbol "" (C{str}). S_SEP = '' #: Separator between deg, min and sec "" (C{str}). _F_prec = {F_D: 6, F_DM: 4, F_DMS: 2, #: (INTERNAL) default precs. F_DEG: 6, F_MIN: 4, F_SEC: 2, F_RAD: 5} _S_norm = {'^': S_DEG, '˚': S_DEG, #: (INTERNAL) normalized DMS. "'": S_MIN, '’': S_MIN, '′': S_MIN, '"': S_SEC, '″': S_SEC, '”': S_SEC} _S_ALL = (S_DEG, S_MIN, S_SEC) + tuple(_S_norm.keys()) #: (INTERNAL) alternates. _rangerrors = True class RangeError(ValueError): '''Error raised for lat- or longitude values outside the B{C{clip}}, B{C{clipLat}}, B{C{clipLon}} or B{C{limit}} range in function L{clipDMS}, L{parse3llh}, L{parseDMS} or L{parseDMS2}. @see: Function L{rangerrors}. ''' pass def _toDMS(deg, form, prec, sep, ddd, suff): # MCCABE 14 '''(INTERNAL) Convert degrees to C{str}, with/-out sign and/or suffix. ''' try: d = abs(float(deg)) except ValueError: raise ValueError('%s invalid: %r' % ('deg', deg)) form = form.lower() sign = form[:1] if sign in '-+': form = form[1:] else: sign = '' if prec is None: z = p = _F_prec.get(form, 6) else: z = int(prec) p = abs(z) w = p + (1 if p else 0) if form in (F_DEG, F_MIN, F_SEC): s_deg = s_min = s_sec = '' # no symbols else: s_deg, s_min, s_sec = S_DEG, S_MIN, S_SEC if form in (F_D, F_DEG, 'degrees'): # deg°, degrees t = '%0*.*f' % (ddd+w,p,d) s = s_deg elif form in (F_RAD, 'radians'): t = '%.*f' % (p,radians(d)) s = S_RAD elif form in (F_DM, F_MIN, 'deg+min'): d, m = divmod(d * 60, 60) t = "%0*d%s%s%0*.*f" % (ddd,int(d),s_deg, sep, w+2,p,m) s = s_min else: # F_DMS, F_SEC, 'deg+min+sec' d, s = divmod(d * 3600, 3600) m, s = divmod(s, 60) t = "%0*d%s%s%02d%s%s%0*.*f" % (ddd,int(d),s_deg, sep, int(m),s_min, sep, w+2,p,s) s = s_sec if z > 1: t = fStrzs(t) if sign: if deg < 0: t = '-' + t elif deg > 0 and sign == '+': t = '+' + t elif suff: s += sep + suff return t + s def bearingDMS(bearing, form=F_D, prec=None, sep=S_SEP): '''Convert bearing to a string. @param bearing: Bearing from North (compass C{degrees360}). @keyword form: Optional B{C{bearing}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__} or L{F_RAD__}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword sep: Optional separator (C{str}). @return: Compass degrees per the specified B{C{form}} (C{str}). @JSname: I{toBrng}. ''' return _toDMS(bearing % 360, form, prec, sep, 1, '') def clipDMS(deg, limit): '''Clip a lat- or longitude to the given range. @param deg: Unclipped lat- or longitude (C{degrees}). @param limit: Valid B{C{-limit..+limit}} range (C{degrees}). @return: Clipped value (C{degrees}). @raise RangeError: If B{C{abs(deg)}} beyond B{C{limit}} and L{rangerrors} set to C{True}. ''' if limit > 0: c = min(limit, max(-limit, deg)) if _rangerrors and deg != c: raise RangeError('%s beyond %s degrees' % (fStr(deg, prec=6), fStr(copysign(limit, deg), prec=3, ints=True))) deg = c return deg def compassDMS(bearing, form=F_D, prec=None, sep=S_SEP): '''Convert bearing to a string suffixed with compass point. @param bearing: Bearing from North (compass C{degrees360}). @keyword form: Optional B{C{bearing}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__} or L{F_RAD__}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword sep: Optional separator (C{str}). @return: Compass degrees and point in the specified form (C{str}). ''' return _toDMS(bearing % 360, form, prec, sep, 1, compassPoint(bearing)) def compassPoint(bearing, prec=3): '''Convert bearing to a compass point. @param bearing: Bearing from North (compass C{degrees360}). @keyword prec: Optional precision (1 for cardinal or basic winds, 2 for intercardinal or ordinal or principal winds, 3 for secondary-intercardinal or half-winds or 4 for quarter-winds). @return: Compass point (1-, 2-, 3- or 4-letter C{str}). @raise ValueError: Invalid B{C{prec}}. @see: U{Dms.compassPoint <https://GitHub.com/chrisveness/geodesy/blob/master/dms.js>} and U{Compass rose<https://WikiPedia.org/wiki/Compass_rose>}. @example: >>> p = compassPoint(24, 1) # 'N' >>> p = compassPoint(24, 2) # 'NE' >>> p = compassPoint(24, 3) # 'NNE' >>> p = compassPoint(24) # 'NNE' >>> p = compassPoint(11, 4) # 'NbE' >>> p = compassPoint(30, 4) # 'NEbN' >>> p = compassPoint(11.249) # 'N' >>> p = compassPoint(11.25) # 'NNE' >>> p = compassPoint(-11.25) # 'N' >>> p = compassPoint(348.749) # 'NNW' ''' try: # m = 2 << prec; x = 32 // m m, x = _MOD_X[prec] except KeyError: raise ValueError('%s invalid: %r' % ('prec', prec)) # not round(), i.e. half-even rounding in Python 3, # but round-away-from-zero as int(b + 0.5) iff b is # non-negative, otherwise int(b + copysign(0.5, b)) q = int((bearing % 360) * m / 360.0 + 0.5) % m return _WINDS[q * x] _MOD_X = {1: (4, 8), 2: (8, 4), 3: (16, 2), 4: (32, 1)} #: (INTERNAL) [prec] _WINDS = ('N', 'NbE', 'NNE', 'NEbN', 'NE', 'NEbE', 'ENE', 'EbN', 'E', 'EbS', 'ESE', 'SEbE', 'SE', 'SEbS', 'SSE', 'SbE', 'S', 'SbW', 'SSW', 'SWbS', 'SW', 'SWbW', 'WSW', 'WbS', 'W', 'WbN', 'WNW', 'NWbW', 'NW', 'NWbN', 'NNW', 'NbW') #: (INTERNAL) cardinals def degDMS(deg, prec=6, s_D=S_DEG, s_M=S_MIN, s_S=S_SEC, neg='-', pos=''): '''Convert degrees to a string in degrees, minutes I{or} seconds. @param deg: Value in degrees (C{scalar}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword s_D: Symbol for degrees (C{str}). @keyword s_M: Symbol for minutes (C{str}) or C{""}. @keyword s_S: Symbol for seconds (C{str}) or C{""}. @keyword neg: Optional sign for negative ('-'). @keyword pos: Optional sign for positive (''). @return: I{Either} degrees, minutes I{or} seconds (C{str}). ''' d, s = abs(deg), s_D if d < 1: if s_M: d *= 60 if d < 1 and s_S: d *= 60 s = s_S else: s = s_M elif s_S: d *= 3600 s = s_S n = neg if deg < 0 else pos z = int(prec) t = '%s%.*f' % (n, abs(z),d) if z > 1: t = fStrzs(t) return t + s def latDMS(deg, form=F_DMS, prec=2, sep=S_SEP): '''Convert latitude to a string, optionally suffixed with N or S. @param deg: Latitude to be formatted (C{degrees}). @keyword form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__} or L{F_RAD__}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword sep: Optional separator (C{str}). @return: Degrees in the specified form (C{str}). @JSname: I{toLat}. ''' return _toDMS(deg, form, prec, sep, 2, 'S' if deg < 0 else 'N') def lonDMS(deg, form=F_DMS, prec=2, sep=S_SEP): '''Convert longitude to a string, optionally suffixed with E or W. @param deg: Longitude to be formatted (C{degrees}). @keyword form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__} or L{F_RAD__}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword sep: Optional separator (C{str}). @return: Degrees in the specified form (C{str}). @JSname: I{toLon}. ''' return _toDMS(deg, form, prec, sep, 3, 'W' if deg < 0 else 'E') def normDMS(strDMS, norm=''): '''Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols %s, %s and %s. @param strDMS: DMS (C{str}). @keyword norm: Optional replacement symbol, default symbol otherwise (C{str}). @return: Normalized DMS (C{str}). ''' if norm: for s in _S_ALL: strDMS = strDMS.replace(s, norm) strDMS = strDMS.rstrip(norm) else: for s, S in _S_norm.items(): strDMS = strDMS.replace(s, S) return strDMS if __debug__: # no __doc__ at -O and -OO normDMS.__doc__ %= (S_DEG, S_MIN, S_SEC) def parse3llh(strll, height=0, sep=',', clipLat=90, clipLon=180): '''Parse a string representing lat-, longitude and height point. The lat- and longitude value must be separated by a separator character. If height is present it must follow, separated by another separator. The lat- and longitude values may be swapped, provided at least one ends with the proper compass point. @param strll: Latitude, longitude[, height] (C{str}, ...). @keyword height: Optional, default height (C{meter}). @keyword sep: Optional separator (C{str}). @keyword clipLat: Keep latitude in B{C{-clipLat..+clipLat}} (C{degrees}). @keyword clipLon: Keep longitude in B{C{-clipLon..+clipLon}} range (C{degrees}). @return: A L{LatLon3Tuple}C{(lat, lon, height)} in C{degrees}, C{degrees} and C{float}. @raise RangeError: Lat- or longitude value of B{C{strll}} outside valid range and L{rangerrors} set to C{True}. @raise ValueError: Invalid B{C{strll}}. @see: Functions L{parseDMS} and L{parseDMS2} for more details on the forms and symbols accepted. @example: >>> parse3llh('000°00′05.31″W, 51° 28′ 40.12″ N') (51.4778°N, 000.0015°W, 0) ''' try: ll = strll.strip().split(sep) if len(ll) > 2: # XXX interpret height unit h = float(ll.pop(2).strip().rstrip(_LETTERS).rstrip()) else: h = height if len(ll) != 2: raise ValueError except (AttributeError, TypeError, ValueError): return ValueError('parsing %r failed' % (strll,)) a, b = [_.strip() for _ in ll] if a[-1:] in 'EW' or b[-1:] in 'NS': a, b = b, a a, b = parseDMS2(a, b, clipLat=clipLat, clipLon=clipLon) # PYCHOK LatLon2Tuple return LatLon3Tuple(a, b, h) def parseDMS(strDMS, suffix='NSEW', sep=S_SEP, clip=0): '''Parse a string representing deg°min′sec″ to degrees. This is very flexible on formats, allowing signed decimal degrees, degrees and minutes or degrees minutes and seconds optionally suffixed by compass direction NSEW. A variety of symbols, separators and suffixes are accepted, for example 3° 37′ 09″W. Minutes and seconds may be omitted. @param strDMS: Degrees in any of several forms (C{str} or C{degrees}). @keyword suffix: Optional, valid compass directions (NSEW). @keyword sep: Optional separator between deg°, min′ and sec″ (''). @keyword clip: Optionally, limit value to -clip..+clip (C{degrees}). @return: Degrees (C{float}). @raise RangeError: Value of B{C{strDMS}} outside the valid range and L{rangerrors} set to C{True}. @raise ValueError: Invalid B{C{strDMS}}. @see: Function L{parse3llh} to parse a string with lat-, longitude and height values. ''' try: # signed decimal degrees without NSEW d = float(strDMS) except (TypeError, ValueError): try: strDMS = strDMS.strip() t = strDMS.lstrip('-+').rstrip(suffix.upper()) if sep: t = t.replace(sep, ' ') for s in _S_ALL: t = t.replace(s, '') else: for s in _S_ALL: t = t.replace(s, ' ') t = list(map(float, t.strip().split())) + [0, 0] d = t[0] + (t[1] + t[2] / 60.0) / 60.0 if strDMS[:1] == '-' or strDMS[-1:] in 'SW': d = -d except (AttributeError, IndexError, TypeError, ValueError): raise ValueError('parsing %r failed' % (strDMS,)) return clipDMS(d, clip) def parseDMS2(strLat, strLon, sep=S_SEP, clipLat=90, clipLon=180): '''Parse lat- and longitude representions. @param strLat: Latitude in any of several forms (C{str} or C{degrees}). @param strLon: Longitude in any of several forms (C{str} or C{degrees}). @keyword sep: Optional separator between deg°, min′ and sec″ (''). @keyword clipLat: Keep latitude in B{C{-clipLat..+clipLat}} range (C{degrees}). @keyword clipLon: Keep longitude in B{C{-clipLon..+clipLon}} range (C{degrees}). @return: A L{LatLon2Tuple}C{(lat, lon)} in C{degrees}. @raise RangeError: Value of B{C{strLat}} or B{C{strLon}} outside the valid range and L{rangerrors} set to C{True}. @raise ValueError: Invalid B{C{strLat}} or B{C{strLon}}. @see: Function L{parse3llh} to parse a string with lat-, longitude and height values and function L{parseDMS} to parse individual lat- or longitudes. ''' return LatLon2Tuple(parseDMS(strLat, suffix='NS', sep=sep, clip=clipLat), parseDMS(strLon, suffix='EW', sep=sep, clip=clipLon)) def _parseUTMUPS(strUTMUPS, band=''): # see .utm.py '''(INTERNAL) Parse a string representing a UTM or UPS coordinate consisting of C{"zone[band] hemisphere/pole easting northing"}. @param strUTMUPS: A UTM or UPS coordinate (C{str}). @keyword band: Optional, default Band letter (C{str}). @return: 5-Tuple (C{zone, hemisphere/pole, easting, northing, band}). @raise Value: Invalid B{C{strUTMUPS}}. ''' try: u = strUTMUPS.strip().replace(',', ' ').split() if len(u) < 4: raise ValueError z, h = u[:2] if h[:1] not in 'NnSs': raise ValueError if z.isdigit(): z, B = int(z), band else: for i in range(len(z)): if not z[i].isdigit(): # int('') raises ValueError z, B = int(z[:i]), z[i:] break else: raise ValueError e, n = map(float, u[2:4]) except (AttributeError, TypeError, ValueError): raise ValueError('%s invalid: %r' % ('strUTMUPS', strUTMUPS)) return z, h.upper(), e, n, B.upper() def precision(form, prec=None): '''Set the default precison for a given F_ form. @param form: L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC} or L{F_RAD} (C{str}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @return: Previous precision (C{int}). @raise ValueError: Invalid B{C{form}} or B{C{prec}} or beyond valid range. ''' try: p = _F_prec[form] except KeyError: raise ValueError('%s invalid: %s' % ('form', form)) if isint(prec): if not -10 < prec < 10: raise ValueError('%s invalid: %s' % ('prec', prec)) _F_prec[form] = prec return p def rangerrors(raiser=None): '''Gert/set raising of range errors. @keyword raiser: Choose C{True} to raise or C{False} to ignore L{RangeError} exceptions. Use C{None} to leave the setting unchanged. @return: Previous setting (C{bool}). @note: Out-of-range lat- and longitude values are always clipped to the nearest range limit. ''' global _rangerrors t = _rangerrors if raiser in (True, False): _rangerrors = raiser return t def toDMS(deg, form=F_DMS, prec=2, sep=S_SEP, ddd=2, neg='-', pos=''): '''Convert signed degrees to string, without suffix. @param deg: Degrees to be formatted (C{degrees}). @keyword form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_RAD} without suffix, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__} or L{F_RAD__}). @keyword prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @keyword sep: Optional separator (C{str}). @keyword ddd: Optional number of digits for deg° (2 or 3). @keyword neg: Optional sign for negative degrees ('-'). @keyword pos: Optional sign for positive degrees (''). @return: Degrees in the specified form (C{str}). ''' t = _toDMS(deg, form, prec, sep, ddd, '') if form[:1] not in '-+': t = (neg if deg < 0 else pos) + t return t # **) MIT License # # Copyright (C) 2016-2020 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.