Package pygeodesy :: Module dms |
[frames] | no frames]

# Module dms

Functions to parse and format bearing, compass, lat- and longitudes in various forms of degrees, minutes and seconds.

After (C) Chris Veness 2011-2015 published under the same MIT Licence**, see Latitude/Longitude and Vector-based geodesy.

Version: 20.04.11

Functions
bearingDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) Convert bearing to a string. |
clipDMS(deg, limit) Clip a lat- or longitude to the given range. |
compassDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) Convert bearing to a string suffixed with compass point. |
compassPoint(bearing, prec=3) Convert bearing to a compass point. |
degDMS(deg, prec=6, s_D=`'``°``'`, s_M=`'``\xe2\x80\xb2``'`, s_S=`'``″``'`, neg=`'``-``'`, pos=`'````'`) Convert degrees to a string in degrees, minutes or seconds. |
latDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) Convert latitude to a string, optionally suffixed with N or S. |
lonDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) Convert longitude to a string, optionally suffixed with E or W. |
normDMS(strDMS, norm=`'````'`) Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols °, ′ and ″. |
parse3llh(strll, height=0, sep=`'``,``'`, clipLat=90, clipLon=180) Parse a string representing lat-, longitude and height point. |
parseDMS(strDMS, suffix=`'``NSEW``'`, sep=`'````'`, clip=0) Parse a string representing deg°min′sec″ to degrees. |
parseDMS2(strLat, strLon, sep=`'````'`, clipLat=90, clipLon=180) Parse lat- and longitude representions. |
precision(form, prec=None) Set the default precison for a given F_ form. |
toDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`, ddd=2, neg=`'``-``'`, pos=`'````'`) Convert signed degrees to string, without suffix. |

Variables
| __all__ = `_ALL_LAZY.dms`
| F_D = ``'``d``'`` Format degrees as unsigned "deg°" plus suffix (`str`).
| F_DM = ``'``dm``'`` Format degrees as unsigned "deg°min′" plus suffix (`str`).
| F_DMS = ``'``dms``'`` Format degrees as unsigned "deg°min′sec″" plus suffix (`str`).
| F_DEG = ``'``deg``'`` Format degrees as unsigned "[D]DD" plus suffix without symbol (`str`).
| F_MIN = ``'``min``'`` Format degrees as unsigned "[D]DDMM" plus suffix without symbols (`str`).
| F_SEC = ``'``sec``'`` Format degrees as unsigned "[D]DDMMSS" plus suffix without symbols (`str`).
| F_RAD = ``'``rad``'`` Convert degrees to radians and format as unsigned "RR" plus suffix (`str`).
| F_D_ = ``'``-d``'`` Format degrees as signed "-/deg°" without suffix (`str`).
| F_DM_ = ``'``-dm``'`` Format degrees as signed "-/deg°min′" without suffix (`str`).
| F_DMS_ = ``'``-dms``'`` Format degrees as signed "-/deg°min′sec″" without suffix (`str`).
| F_DEG_ = ``'``-deg``'`` Format degrees as signed "-/[D]DD" without suffix and symbol (`str`).
| F_MIN_ = ``'``-min``'`` Format degrees as signed "-/[D]DDMM" without suffix and symbols (`str`).
| F_SEC_ = ``'``-sec``'`` Format degrees as signed "-/[D]DDMMSS" without suffix and symbols (`str`).
| F_RAD_ = ``'``-rad``'`` Convert degrees to radians and format as signed "-/RR" without suffix (`str`).
| F_D__ = ``'``+d``'`` Format degrees as signed "-/+deg°" without suffix (`str`).
| F_DM__ = ``'``+dm``'`` Format degrees as signed "-/+deg°min′" without suffix (`str`).
| F_DMS__ = ``'``+dms``'`` Format degrees as signed "-/+deg°min′sec″" without suffix (`str`).
| F_DEG__ = ``'``+deg``'`` Format degrees as signed "-/+[D]DD" without suffix and symbol (`str`).
| F_MIN__ = ``'``+min``'`` Format degrees as signed "-/+[D]DDMM" without suffix and symbols (`str`).
| F_SEC__ = ``'``+sec``'`` Format degrees as signed "-/+[D]DDMMSS" without suffix and symbols (`str`).
| F_RAD__ = ``'``+rad``'`` Convert degrees to radians and format as signed "-/+RR" without suffix (`str`).
| S_DEG = ``'``°``'`` Degrees "°" symbol (`str`).
| S_MIN = ``'``\xe2\x80\xb2``'`` Minutes "′" symbol (`str`).
| S_SEC = ``'``″``'`` Seconds "″" symbol (`str`).
| S_RAD = ``'````'`` Radians symbol "" (`str`).
| S_SEP = ``'````'`` Separator between deg, min and sec "" (`str`).

Function Details

### bearingDMS (bearing, form=`'``d``'`, prec=None, sep=`'````'`) |
Convert bearing to a string. Arguments: `bearing` - Bearing from North (compass `degrees360`). `form` - Optional `bearing` format (`str` or F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_RAD, F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_RAD_, F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__ or F_RAD__). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `sep` - Optional separator (`str`). Returns: Compass degrees per the specified `form` (`str`). JS name: toBrng.

### clipDMS (deg, limit) |
Clip a lat- or longitude to the given range. Arguments: `deg` - Unclipped lat- or longitude (`degrees`). `limit` - Valid `-limit..+limit` range (`degrees`). Returns: Clipped value (`degrees`). Raises: `RangeError` - If `abs(deg)` beyond `limit` and rangerrors set to `True`.

### compassDMS (bearing, form=`'``d``'`, prec=None, sep=`'````'`) |
Convert bearing to a string suffixed with compass point. Arguments: `bearing` - Bearing from North (compass `degrees360`). `form` - Optional `bearing` format (`str` or F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_RAD, F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_RAD_, F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__ or F_RAD__). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `sep` - Optional separator (`str`). Returns: Compass degrees and point in the specified form (`str`).

### compassPoint (bearing, prec=3) |
Convert bearing to a compass point. Arguments: `bearing` - Bearing from North (compass `degrees360`). `prec` - Optional precision (1 for cardinal or basic winds, 2 for intercardinal or ordinal or principal winds, 3 for secondary-intercardinal or half-winds or 4 for quarter-winds). Returns: Compass point (1-, 2-, 3- or 4-letter `str`). Raises: `ValueError` - Invalid `prec`. See Also: Dms.compassPoint and Compass rose. Example:
    >>> p = compassPoint(24, 1)  # 'N'
    >>> p = compassPoint(24, 2)  # 'NE'
    >>> p = compassPoint(24, 3)  # 'NNE'
    >>> p = compassPoint(24)     # 'NNE'
    >>> p = compassPoint(11, 4)  # 'NbE'
    >>> p = compassPoint(30, 4)  # 'NEbN'
    >>> p = compassPoint(11.249)  # 'N'
    >>> p = compassPoint(11.25)   # 'NNE'
    >>> p = compassPoint(-11.25)  # 'N'
    >>> p = compassPoint(348.749) # 'NNW'

### degDMS (deg, prec=6, s_D=`'``°``'`, s_M=`'``\xe2\x80\xb2``'`, s_S=`'``″``'`, neg=`'``-``'`, pos=`'````'`) |
Convert degrees to a string in degrees, minutes or seconds. Arguments: `deg` - Value in degrees (`scalar`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `s_D` - Symbol for degrees (`str`). `s_M` - Symbol for minutes (`str`) or `""`. `s_S` - Symbol for seconds (`str`) or `""`. `neg` - Optional sign for negative (`'-'`). `pos` - Optional sign for positive (`''`). Returns: Either degrees, minutes or seconds (`str`).

### latDMS (deg, form=`'``dms``'`, prec=2, sep=`'````'`) |
Convert latitude to a string, optionally suffixed with N or S. Arguments: `deg` - Latitude to be formatted (`degrees`). `form` - Optional `deg` format (`str` or F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_RAD, F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_RAD_, F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__ or F_RAD__). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `sep` - Optional separator (`str`). Returns: Degrees in the specified form (`str`). JS name: toLat.

### lonDMS (deg, form=`'``dms``'`, prec=2, sep=`'````'`) |
Convert longitude to a string, optionally suffixed with E or W. Arguments: `deg` - Longitude to be formatted (`degrees`). `form` - Optional `deg` format (`str` or F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_RAD, F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_RAD_, F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__ or F_RAD__). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `sep` - Optional separator (`str`). Returns: Degrees in the specified form (`str`). JS name: toLon.

### normDMS (strDMS, norm=`'````'`) |
Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols °, ′ and ″. Arguments: `strDMS` - DMS (`str`). `norm` - Optional replacement symbol, default symbol otherwise (`str`). Returns: Normalized DMS (`str`).

### parse3llh (strll, height=0, sep=`'``,``'`, clipLat=90, clipLon=180) |
Parse a string representing lat-, longitude and height point. The lat- and longitude value must be separated by a separator character. If height is present it must follow, separated by another separator. The lat- and longitude values may be swapped, provided at least one ends with the proper compass point. Arguments: `strll` - Latitude, longitude[, height] (`str`, ...). `height` - Optional, default height (`meter`) or `None`. `sep` - Optional separator (`str`). `clipLat` - Keep latitude in `-clipLat..+clipLat` (`degrees`). `clipLon` - Keep longitude in `-clipLon..+clipLon` range (`degrees`). Returns: A LatLon3Tuple`(lat, lon, height)` in `degrees`, `degrees` and `float`. Raises: `RangeError` - Lat- or longitude value of `strll` outside valid range and rangerrors set to `True`. `ValueError` - Invalid `strll` or `height`. See Also: Functions parseDMS and parseDMS2 for more details on the forms and symbols accepted. Example:
    >>> parse3llh('000°00′05.31″W, 51° 28′ 40.12″ N')
    (51.4778°N, 000.0015°W, 0)

### parseDMS (strDMS, suffix=`'``NSEW``'`, sep=`'````'`, clip=0) |
Parse a string representing deg°min′sec″ to degrees. This is very flexible on formats, allowing signed decimal degrees, degrees and minutes or degrees minutes and seconds optionally suffixed by compass direction NSEW. A variety of symbols, separators and suffixes are accepted, for example 3° 37′ 09″W. Minutes and seconds may be omitted. Arguments: `strDMS` - Degrees in any of several forms (`str` or `degrees`). `suffix` - Optional, valid compass directions (NSEW). `sep` - Optional separator between deg°, min′ and sec″ (''). `clip` - Optionally, limit value to -clip..+clip (`degrees`). Returns: Degrees (`float`). Raises: `RangeError` - Value of `strDMS` outside the valid range and rangerrors set to `True`. `ValueError` - Invalid `strDMS` or `clip`. See Also: Function parse3llh to parse a string with lat-, longitude and height values.

### parseDMS2 (strLat, strLon, sep=`'````'`, clipLat=90, clipLon=180) |
Parse lat- and longitude representions. Arguments: `strLat` - Latitude in any of several forms (`str` or `degrees`). `strLon` - Longitude in any of several forms (`str` or `degrees`). `sep` - Optional separator between deg°, min′ and sec″ (''). `clipLat` - Keep latitude in `-clipLat..+clipLat` range (`degrees`). `clipLon` - Keep longitude in `-clipLon..+clipLon` range (`degrees`). Returns: A LatLon2Tuple`(lat, lon)` in `degrees`. Raises: `RangeError` - Value of `strLat` or `strLon` outside the valid range and rangerrors set to `True`. `ValueError` - Invalid `strLat` or `strLon`. See Also: Function parse3llh to parse a string with lat-, longitude and height values and function parseDMS to parse individual lat- or longitudes.

### precision (form, prec=None) |
Set the default precison for a given F_ form. Arguments: `form` - F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. Returns: Previous precision (`int`). Raises: `ValueError` - Invalid `form` or `prec` or beyond valid range.

### toDMS (deg, form=`'``dms``'`, prec=2, sep=`'````'`, ddd=2, neg=`'``-``'`, pos=`'````'`) |
Convert signed degrees to string, without suffix. Arguments: `deg` - Degrees to be formatted (`degrees`). `form` - Optional `deg` format (`str` or F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_RAD without suffix, F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_RAD_, F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__ or F_RAD__). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for `prec` values of 1 and above, but kept for negative `prec`. `sep` - Optional separator (`str`). `ddd` - Optional number of digits for deg° (2 or 3). `neg` - Optional sign for negative degrees ('-'). `pos` - Optional sign for positive degrees (''). Returns: Degrees in the specified form (`str`).