Package pygeodesy :: Module dms |
[frames] | no frames]

# Module dms

Functions to parse and format bearing, compass, lat- and longitudes in various forms of degrees, minutes and seconds.

After (C) Chris Veness 2011-2015 published under the same MIT Licence**, see Latitude/Longitude and Vector-based geodesy.

Version: 19.01.05

Classes
| RangeError Error raised for lat- or longitude values outside the clip, clipLat, clipLon or limit range in function clipDMS, parse3llh, parseDMS or parseDMS2.

Functions
bearingDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) Convert bearing to a string. |
clipDMS(deg, limit) Clip a lat- or longitude to the given range. |
compassDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) Convert bearing to a string suffixed with compass point. |
compassPoint(bearing, prec=3) Convert bearing to a compass point. |
latDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) Convert latitude to a string suffixed with N or S. |
lonDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) Convert longitude to a string suffixed with E or W. |
normDMS(strDMS, norm=`'````'`) Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols °, ′ and ″. |
parse3llh(strll, height=0, sep=`'``,``'`, clipLat=90, clipLon=180) Parse a string representing lat-, longitude and height point. |
parseDMS(strDMS, suffix=`'``NSEW``'`, sep=`'````'`, clip=0) Parse a string representing deg°min′sec″ to degrees. |
parseDMS2(strLat, strLon, sep=`'````'`, clipLat=90, clipLon=180) Parse lat- and longitude representions. |
precision(form, prec=None) Set the default precison for a given F_ form. |
rangerrors(raiser=None) Gert/set raising of range errors. |
toDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`, ddd=2, neg=`'``-``'`, pos=`'````'`) Convert signed degrees to string, without suffix. |

Variables
| __all__ = `_ALL_LAZY.dms`
| F_D = ``'``d``'`` Format degrees as deg° (`str`).
| F_DM = ``'``dm``'`` Format degrees as deg°min′ (`str`).
| F_DMS = ``'``dms``'`` Format degrees as deg°min′sec″ (`str`).
| F_DEG = ``'``deg``'`` Format degrees as [D]DD without symbol (`str`).
| F_MIN = ``'``min``'`` Format degrees as [D]DDMM without symbols (`str`).
| F_SEC = ``'``sec``'`` Format degrees as [D]DDMMSS without symbols (`str`).
| F_RAD = ``'``rad``'`` Convert degrees to radians and format as RR.r (`str`).
| S_DEG = ``'``\xc2\xb0``'`` Degrees "°" symbol (`str`).
| S_MIN = ``'``\xe2\x80\xb2``'`` Minutes "′" symbol (`str`).
| S_SEC = ``'``\xe2\x80\xb3``'`` Seconds "″" symbol (`str`).
| S_RAD = ``'````'`` Radians symbol "" (`str`).
| S_SEP = ``'````'`` Separator between deg, min and sec "" (`str`).

Function Details

### bearingDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) |
Convert bearing to a string. Parameters: `bearing` - Bearing from North (compass `degrees360`). `form` - Optional format, F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD for deg°, deg°min′, deg°min′sec″, [D]DD, [D]DDMM, [D]DDMMSS or radians (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. `sep` - Optional separator (`str`). Returns: Compass degrees per the specified form (`str`). JS name: toBrng.

### clipDMS(deg, limit) |
Clip a lat- or longitude to the given range. Parameters: `deg` - Unclipped lat- or longitude (`degrees`). `limit` - Valid -limit..+limit range (`degrees`). Returns: Clipped value (`degrees`). Raises: `RangeError` - If deg beyond limit and rangerrors set to `True`.

### compassDMS(bearing, form=`'``d``'`, prec=None, sep=`'````'`) |
Convert bearing to a string suffixed with compass point. Parameters: `bearing` - Bearing from North (compass `degrees360`). `form` - Optional format, F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD for deg°, deg°min′, deg°min′sec″, [D]DD, [D]DDMM, [D]DDMMSS or radians (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. `sep` - Optional separator (`str`). Returns: Compass degrees and point in the specified form (`str`).

### compassPoint(bearing, prec=3) |
Convert bearing to a compass point. Parameters: `bearing` - Bearing from North (compass `degrees360`). `prec` - Optional precision (1 for cardinal or basic winds, 2 for intercardinal or ordinal or principal winds, 3 for secondary-intercardinal or half-winds or 4 for quarter-winds). Returns: Compass point (1-, 2-, 3- or 4-letter `str`). Raises: `ValueError` - Invalid prec. See Also: Dms.compassPoint and Compass rose. Example:
    >>> p = compassPoint(24, 1)  # 'N'
    >>> p = compassPoint(24, 2)  # 'NE'
    >>> p = compassPoint(24, 3)  # 'NNE'
    >>> p = compassPoint(24)     # 'NNE'
    >>> p = compassPoint(11, 4)  # 'NbE'
    >>> p = compassPoint(30, 4)  # 'NEbN'
    >>> p = compassPoint(11.249)  # 'N'
    >>> p = compassPoint(11.25)   # 'NNE'
    >>> p = compassPoint(-11.25)  # 'N'
    >>> p = compassPoint(348.749) # 'NNW'

### latDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) |
Convert latitude to a string suffixed with N or S. Parameters: `deg` - Latitude to be formatted (`degrees`). `form` - Optional format, F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD for deg°, deg°min′, deg°min′sec″, DD, DDMM, DDMMSS or radians (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. `sep` - Optional separator (`str`). Returns: Degrees in the specified form (`str`). JS name: toLat.

### lonDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`) |
Convert longitude to a string suffixed with E or W. Parameters: `deg` - Longitude to be formatted (`degrees`). `form` - Optional format, F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD for deg°, deg°min′, deg°min′sec″, DDD, DDDMM, DDDMMSS or radians (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. `sep` - Optional separator (`str`). Returns: Degrees in the specified form (`str`). JS name: toLon.

### normDMS(strDMS, norm=`'````'`) |
Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols °, ′ and ″. Parameters: `strDMS` - DMS (`str`). `norm` - Optional replacement symbol, default symbol otherwise (`str`). Returns: Normalized DMS (`str`).

### parse3llh(strll, height=0, sep=`'``,``'`, clipLat=90, clipLon=180) |
Parse a string representing lat-, longitude and height point. The lat- and longitude value must be separated by a separator character. If height is present it must follow, separated by another separator. The lat- and longitude values may be swapped, provided at least one ends with the proper compass point. Parameters: `strll` - Latitude, longitude[, height] (`str`, ...). `height` - Optional, default height (`meter`). `sep` - Optional separator (`str`). `clipLat` - Keep latitude in -clipLat..+clipLat (`degrees`). `clipLon` - Keep longitude in -clipLon..+clipLon range (`degrees`). Returns: 3-Tuple (lat, lon, height) as (`degrees90`, `degrees180`, `float`). Raises: `RangeError` - Lat- or longitude value of strll outside valid range and rangerrrors set to `True`. `ValueError` - Invalid strll. See Also: Functions parseDMS and parseDMS2 for more details on the forms and symbols accepted. Example:
    >>> parse3llh('000°00′05.31″W, 51° 28′ 40.12″ N')
    (51.4778°N, 000.0015°W, 0)

### parseDMS(strDMS, suffix=`'``NSEW``'`, sep=`'````'`, clip=0) |
Parse a string representing deg°min′sec″ to degrees. This is very flexible on formats, allowing signed decimal degrees, degrees and minutes or degrees minutes and seconds optionally suffixed by compass direction NSEW. A variety of symbols, separators and suffixes are accepted, for example 3° 37′ 09″W. Minutes and seconds may be omitted. Parameters: `strDMS` - Degrees in any of several forms (`str` or `degrees`). `suffix` - Optional, valid compass directions (NSEW). `sep` - Optional separator between deg°, min′ and sec″ (''). `clip` - Optionally, limit value to -clip..+clip (`degrees`). Returns: Degrees (`float`). Raises: `RangeError` - Value of strDMS outside the valid range and rangerrrors set to `True`. `ValueError` - Invalid strDMS. See Also: Function parse3llh to parse a string with lat-, longitude and height values.

### parseDMS2(strLat, strLon, sep=`'````'`, clipLat=90, clipLon=180) |
Parse lat- and longitude representions. Parameters: `strLat` - Latitude in any of several forms (`str` or `degrees`). `strLon` - Longitude in any of several forms (`str` or `degrees`). `sep` - Optional separator between deg°, min′ and sec″ (''). `clipLat` - Keep latitude in -clipLat..+clipLat range (`degrees`). `clipLon` - Keep longitude in -clipLon..+clipLon range (`degrees`). Returns: 2-Tuple (lat, lon) in (`degrees`, `degrees`). Raises: `RangeError` - Value of strLat or strLon outside the valid range and rangerrrors set to `True`. `ValueError` - Invalid strLat or strLon. See Also: Function parse3llh to parse a string with lat-, longitude and height values and function parseDMS to parse individual lat- or longitudes.

### precision(form, prec=None) |
Set the default precison for a given F_ form. Parameters: `form` - F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. Returns: Previous precision (`int`). Raises: `ValueError` - Invalid form or prec or beyond valid range.

### rangerrors(raiser=None) |
Gert/set raising of range errors. Parameters: `raiser` - Choose `True` to raise or `False` to ignore RangeError exceptions. Use `None` to leave the setting unchanged. Returns: Previous setting (`bool`). Note: Out-of-range lat- and longitude values are always clipped to the nearest range limit.

### toDMS(deg, form=`'``dms``'`, prec=2, sep=`'````'`, ddd=2, neg=`'``-``'`, pos=`'````'`) |
Convert signed degrees to string, without suffix. Parameters: `deg` - Degrees to be formatted (`degrees`). `form` - Optional format, F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC or F_RAD for deg°, deg°min′, deg°min′sec″, [D]DD, [D]DDMM, [D]DDMMSS or radians (`str`). `prec` - Optional number of decimal digits (0..9 or `None` for default). Trailing zero decimals are stripped for prec values of 1 and above, but kept for negative prec values. `sep` - Optional separator (`str`). `ddd` - Optional number of digits for deg° (2 or 3). `neg` - Optional sign for negative degrees ('-'). `pos` - Optional sign for positive degrees (''). Returns: Degrees in the specified form (`str`).