# Coverage for pygeodesy/ups.py : 97%

## 175 statements 169 run 6 missing 9 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 | # -*- coding: utf-8 -*- u'''I{Karney}'s Universal Polar Stereographic (UPS) projection. Classes L{Ups} and L{UPSError} and functions L{parseUPS5}, L{toUps8} and L{upsZoneBand5}. A pure Python implementation, partially transcoded from C++ class U{PolarStereographic <https://GeographicLib.SourceForge.io/html/classGeographicLib_1_1PolarStereographic.html>} by I{Charles Karney}. The U{UPS<https://WikiPedia.org/wiki/Universal_polar_stereographic_coordinate_system>} system is used in conjuction with U{UTM <https://WikiPedia.org/wiki/Universal_Transverse_Mercator_coordinate_system>} for locations on the polar regions of the earth. UPS covers areas south of 79.5°S and north of 83.5°N (slightly overlapping the UTM range from 80°S to 84°N by 30' at each end). ''' from pygeodesy.basics import neg from pygeodesy.datums import _ellipsoidal_datum, _WGS84 from pygeodesy.dms import degDMS, parseDMS2 from pygeodesy.errors import RangeError, _ValueError from pygeodesy.fmath import hypot, hypot1, sqrt0 from pygeodesy.interns import EPS, EPS0, NN, _A_, _B_, _COMMASPACE_, \ _EPSmin as _Tol90, _N_, _inside_, \ _pole_, _range_, _S_, _SPACE_, _to_, \ _UTM_, _0_0, _0_5, _1_0, _2_0, _90_0 from pygeodesy.lazily import _ALL_LAZY from pygeodesy.named import nameof, _xnamed from pygeodesy.namedTuples import EasNor2Tuple, UtmUps5Tuple, \ UtmUps8Tuple, UtmUpsLatLon5Tuple from pygeodesy.props import deprecated_method, Property_RO, _update_all from pygeodesy.streprs import Fmt from pygeodesy.units import Meter, Lat, Scalar, Scalar_ from pygeodesy.utily import degrees90, degrees180, sincos2d from pygeodesy.utmupsBase import _LLEB, _hemi, _parseUTMUPS5, \ _to4lldn, _to3zBhp, _to3zll, \ _UPS_LAT_MAX, _UPS_LAT_MIN, _UPS_ZONE, \ _UPS_ZONE_STR, UtmUpsBase from math import atan, atan2, radians, tan __all__ = _ALL_LAZY.ups __version__ = '21.10.05' _Bands = _A_, _B_, 'Y', 'Z' # polar bands _Falsing = Meter(2000e3) # false easting and northing (C{meter}) _K0_UPS = Scalar(0.994) # central UPS scale factor _K1_UPS = Scalar(_1_0) # rescale point scale factor def _Band(a, b): # determine the polar band letter return _Bands[(0 if a < 0 else 2) + (0 if b < 0 else 1)] def _scale(E, rho, tau): # compute the point scale factor, ala Karney t = hypot1(tau) return Scalar((rho / E.a) * t * sqrt0(E.e12 + E.e2 / t**2)) class UPSError(_ValueError): '''Universal Polar Stereographic (UPS) parse or other L{Ups} issue. ''' pass class Ups(UtmUpsBase): '''Universal Polar Stereographic (UPS) coordinate. ''' # _band = NN # polar band ('A', 'B', 'Y' or 'Z') _Error = UPSError # Error class _latlon_args = True # unfalse from _latlon (C{bool}) _pole = NN # UPS projection top/center ('N' or 'S') # _scale = None # point scale factor (C{scalar}) _scale0 = _K0_UPS # central scale factor (C{scalar}) def __init__(self, zone, pole, easting, northing, band=NN, # PYCHOK expected datum=_WGS84, falsed=True, convergence=None, scale=None, name=NN): '''New L{Ups} UPS coordinate. @arg zone: UPS zone (C{int}, zero) or zone with/-out Band letter (C{str}, '00', '00A', '00B', '00Y' or '00Z'). @arg pole: Top/center of (stereographic) projection (C{str}, C{'N[orth]'} or C{'S[outh]'}). @arg easting: Easting, see B{C{falsed}} (C{meter}). @arg northing: Northing, see B{C{falsed}} (C{meter}). @kwarg band: Optional, polar Band (C{str}, 'A'|'B'|'Y'|'Z'). @kwarg datum: Optional, this coordinate's datum (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg falsed: Both B{C{easting}} and B{C{northing}} are falsed (C{bool}). @kwarg convergence: Optional, meridian convergence gamma to save (C{degrees}). @kwarg scale: Optional, computed scale factor k to save (C{scalar}). @kwarg name: Optional name (C{str}). @raise TypeError: Invalid B{C{datum}}. @raise UPSError: Invalid B{C{zone}}, B{C{pole}}, B{C{easting}}, B{C{northing}}, B{C{band}}, B{C{convergence}} or B{C{scale}}. ''' if name: self.name = name try: z, B, p = _to3zBhp(zone, band, hemipole=pole) if z != _UPS_ZONE or (B and B not in _Bands): raise ValueError except (TypeError, ValueError) as x: raise UPSError(zone=zone, pole=pole, band=band, txt=str(x)) self._pole = p UtmUpsBase.__init__(self, easting, northing, band=B, datum=datum, falsed=falsed, convergence=convergence, scale=scale) def __eq__(self, other): return isinstance(other, Ups) and other.zone == self.zone \ and other.pole == self.pole \ and other.easting == self.easting \ and other.northing == self.northing \ and other.band == self.band \ and other.datum == self.datum @Property_RO def band(self): '''Get the polar band letter (C{'A'|'B'|'Y'|'Z'}). ''' self.toLatLon(unfalse=True) return self._band @Property_RO def falsed2(self): '''Get the easting and northing falsing (L{EasNor2Tuple}C{(easting, northing)}). ''' f = _Falsing if self.falsed else 0 return EasNor2Tuple(f, f) @Property_RO def hemisphere(self): '''Get the hemisphere (C{'N'|'S'}). ''' self.toLatLon(unfalse=True) return self._hemisphere @Property_RO def _mgrs(self): '''(INTERNAL) Cache for L{toMgrs}. ''' return self.toUtm(None).toMgrs() def parse(self, strUPS, name=NN): '''Parse a string to a similar L{Ups} instance. @arg strUPS: The UPS coordinate (C{str}), see function L{parseUPS5}. @kwarg name: Optional instance name (C{str}), overriding this name. @return: The similar instance (L{Ups}). @raise UTMError: Invalid B{C{strUPS}}. @see: Functions L{parseUTM5} and L{pygeodesy.parseUTMUPS5}. ''' return parseUPS5(strUPS, datum=self.datum, Ups=self.classof, name=name or self.name) @deprecated_method def parseUPS(self, strUPS): # PYCHOK no cover '''DEPRECATED, use method L{parse}.''' return self.parse(strUPS) @Property_RO def pole(self): '''Get the top/center of (stereographic) projection (C{'N'|'S'} or C{""}). ''' return self._pole def rescale0(self, lat, scale0=_K0_UPS): '''Set the central scale factor for this UPS projection. @arg lat: Northern latitude (C{degrees}). @arg scale0: UPS k0 scale at B{C{lat}} latitude (C{scalar}). @raise RangeError: If B{C{lat}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @raise UPSError: Invalid B{C{scale}}. ''' s0 = Scalar_(scale0=scale0, Error=UPSError, low=EPS) # <= 1.003 or 1.0016? u = toUps8(abs(Lat(lat)), _0_0, datum=self.datum, Ups=_Ups_K1) k = s0 / u.scale if self.scale0 != k: _update_all(self) self._band = NN # force re-compute self._latlon = self._utm = None self._scale0 = Scalar(scale0=k) def toLatLon(self, LatLon=None, unfalse=True, **LatLon_kwds): '''Convert this UPS coordinate to an (ellipsoidal) geodetic point. @kwarg LatLon: Optional, ellipsoidal class to return the geodetic point (C{LatLon}) or C{None}. @kwarg unfalse: Unfalse B{C{easting}} and B{C{northing}} if falsed (C{bool}). @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: This UPS coordinate (B{C{LatLon}}) or if B{C{LatLon}} is C{None}, a L{LatLonDatum5Tuple}C{(lat, lon, datum, convergence, scale)}. @raise TypeError: If B{C{LatLon}} is not ellipsoidal. @raise UPSError: Invalid meridional radius or H-value. ''' if self._latlon and self._latlon_args == unfalse: return self._latlon5(LatLon) E = self.datum.ellipsoid # XXX vs LatLon.datum.ellipsoid x, y = self.eastingnorthing2(falsed=not unfalse) r = hypot(x, y) t = (r / (_2_0 * self.scale0 * E.a / E.es_c)) if r > 0 else EPS0 t = E.es_tauf((1 / t - t) * _0_5) if self._pole == _N_: a, b, c = atan(t), atan2(x, -y), 1 else: a, b, c = neg(atan(t)), atan2(x, y), -1 a, b = degrees90(a), degrees180(b) if not self._band: self._band = _Band(a, b) if not self._hemisphere: self._hemisphere = _hemi(a) ll = _LLEB(a, b, datum=self._datum, name=self.name) ll._convergence = b * c # gamma ll._scale = _scale(E, r, t) if r > 0 else self.scale0 self._latlon_to(ll, unfalse) return self._latlon5(LatLon, **LatLon_kwds) def _latlon_to(self, ll, unfalse): '''(INTERNAL) See method C{.toLatLon}, function C{toUps8}. ''' self._latlon, self._latlon_args = ll, unfalse def toMgrs(self): '''Convert this UPS coordinate to an MGRS grid reference. @return: The MGRS grid reference (L{Mgrs}). @see: Methods L{Ups.toUtm} and L{Utm.toMgrs}. ''' return self._mgrs def toRepr(self, prec=0, fmt=Fmt.SQUARE, sep=_COMMASPACE_, B=False, cs=False, **unused): # PYCHOK expected '''Return a string representation of this UPS coordinate. Note that UPS coordinates are rounded, not truncated (unlike MGRS grid references). @kwarg prec: Optional number of decimals, unstripped (C{int}). @kwarg fmt: Optional, enclosing backets format (C{str}). @kwarg sep: Optional separator between name:value pairs (C{str}). @kwarg B: Optionally, include polar band letter (C{bool}). @kwarg cs: Optionally, include gamma meridian convergence and point scale factor (C{bool} or non-zero C{int} to specify the precison like B{C{prec}}). @return: This UPS as a string with C{00[Band] pole, easting, northing, [convergence, scale]} as C{"[Z:00[Band], P:N|S, E:meter, N:meter]"} plus C{", C:DMS, S:float"} if B{C{cs}} is C{True}, where C{[Band]} is present and C{'A'|'B'|'Y'|'Z'} only if B{C{B}} is C{True} and convergence C{DMS} is in I{either} degrees, minutes I{or} seconds (C{str}). @note: Pseudo zone zero (C{"00"}) for UPS follows I{Karney}'s U{zone UPS <https://GeographicLib.SourceForge.io/html/classGeographicLib_1_1UTMUPS.html>}. ''' return self._toRepr(fmt, B, cs, prec, sep) def toStr(self, prec=0, sep=_SPACE_, B=False, cs=False): # PYCHOK expected '''Return a string representation of this UPS coordinate. Note that UPS coordinates are rounded, not truncated (unlike MGRS grid references). @kwarg prec: Optional number of decimals, unstripped (C{int}). @kwarg sep: Optional separator to join (C{str}) or C{None} to return an unjoined C{tuple} of C{str}s. @kwarg B: Optionally, include and polar band letter (C{bool}). @kwarg cs: Optionally, include gamma meridian convergence and point scale factor (C{bool} or non-zero C{int} to specify the precison like B{C{prec}}). @return: This UPS as a string with C{00[Band] pole, easting, northing, [convergence, scale]} as C{"00[B] N|S meter meter"} plus C{" DMS float"} if B{C{cs}} is C{True}, where C{[Band]} is present and C{'A'|'B'|'Y'|'Z'} only if B{C{B}} is C{True} and convergence C{DMS} is in I{either} degrees, minutes I{or} seconds (C{str}). @note: Zone zero (C{"00"}) for UPS follows I{Karney}'s U{zone UPS <https://GeographicLib.SourceForge.io/html/classGeographicLib_1_1UTMUPS.html>}. ''' return self._toStr(self.pole, B, cs, prec, sep) # PYCHOK pole def toUps(self, pole=NN, **unused): '''Duplicate this UPS coordinate. @kwarg pole: Optional top/center of the UPS projection, (C{str}, 'N[orth]'|'S[outh]'). @return: A copy of this UPS coordinate (L{Ups}). @raise UPSError: Invalid B{C{pole}} or attempt to transfer the projection top/center. ''' if self.pole == pole or not pole: return self.copy() t = _SPACE_(_pole_, repr(self.pole), _to_, repr(pole)) raise UPSError('no transfer', txt=t) def toUtm(self, zone, falsed=True, **unused): '''Convert this UPS coordinate to a UTM coordinate. @arg zone: The UTM zone (C{int}). @kwarg falsed: False both easting and northing (C{bool}). @return: The UTM coordinate (L{Utm}). ''' u = self._utm if u is None or u.zone != zone or falsed != u.falsed: from pygeodesy.utm import toUtm8, Utm ll = self.toLatLon(LatLon=None, unfalse=True) self._utm = toUtm8(ll, Utm=Utm, falsed=falsed, name=self.name, zone=zone) return self._utm @Property_RO def zone(self): '''Get the polar pseudo zone (C{0}), like I{Karney}'s U{zone UPS<https:// GeographicLib.SourceForge.io/html/classGeographicLib_1_1UTMUPS.html>}. ''' return _UPS_ZONE class _Ups_K1(Ups): '''(INTERNAL) For method L{Ups.rescale0}. ''' _scale0 = _K1_UPS def parseUPS5(strUPS, datum=_WGS84, Ups=Ups, falsed=True, name=NN): '''Parse a string representing a UPS coordinate, consisting of C{"[zone][band] pole easting northing"} where B{C{zone}} is pseudo zone C{"00"|"0"|""} and C{band} is C{'A'|'B'|'Y'|'Z'|''}. @arg strUPS: A UPS coordinate (C{str}). @kwarg datum: Optional datum to use (L{Datum}). @kwarg Ups: Optional class to return the UPS coordinate (L{Ups}) or C{None}. @kwarg falsed: Both B{C{easting}} and B{C{northing}} are falsed (C{bool}). @kwarg name: Optional B{C{Ups}} name (C{str}). @return: The UPS coordinate (B{C{Ups}}) or a L{UtmUps5Tuple}C{(zone, hemipole, easting, northing, band)} if B{C{Ups}} is C{None}. The C{hemipole} is the C{'N'|'S'} pole, the UPS projection top/center. @raise UPSError: Invalid B{C{strUPS}}. ''' z, p, e, n, B = _parseUTMUPS5(strUPS, _UPS_ZONE_STR, Error=UPSError) if z != _UPS_ZONE or (B and B not in _Bands): raise UPSError(strUPS=strUPS, zone=z, band=B) if Ups is None: r = UtmUps5Tuple(z, p, e, n, B, Error=UPSError, name=name) else: r = Ups(z, p, e, n, band=B, falsed=falsed, datum=datum) r = _xnamed(r, name) return r def toUps8(latlon, lon=None, datum=None, Ups=Ups, pole=NN, falsed=True, strict=True, name=NN): '''Convert a lat-/longitude point to a UPS coordinate. @arg latlon: Latitude (C{degrees}) or an (ellipsoidal) geodetic C{LatLon} point. @kwarg lon: Optional longitude (C{degrees}) or C{None} if B{C{latlon}} is a C{LatLon}. @kwarg datum: Optional datum for this UPS coordinate, overriding B{C{latlon}}'s datum (C{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg Ups: Optional class to return the UPS coordinate (L{Ups}) or C{None}. @kwarg pole: Optional top/center of (stereographic) projection (C{str}, C{'N[orth]'} or C{'S[outh]'}). @kwarg falsed: False both easting and northing (C{bool}). @kwarg strict: Restrict B{C{lat}} to UPS ranges (C{bool}). @kwarg name: Optional B{C{Ups}} name (C{str}). @return: The UPS coordinate (B{C{Ups}}) or a L{UtmUps8Tuple}C{(zone, hemipole, easting, northing, band, datum, convergence, scale)} if B{C{Ups}} is C{None}. The C{hemipole} is the C{'N'|'S'} pole, the UPS projection top/center. @raise RangeError: If B{C{strict}} and B{C{lat}} outside the valid UPS bands or if B{C{lat}} or B{C{lon}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @raise TypeError: If B{C{latlon}} is not ellipsoidal or B{C{datum}} invalid. @raise ValueError: If B{C{lon}} value is missing or if B{C{latlon}} is invalid. @see: I{Karney}'s C++ class U{UPS <https://GeographicLib.SourceForge.io/html/classGeographicLib_1_1UPS.html>}. ''' lat, lon, d, name = _to4lldn(latlon, lon, datum, name) z, B, p, lat, lon = upsZoneBand5(lat, lon, strict=strict) # PYCHOK UtmUpsLatLon5Tuple d = _ellipsoidal_datum(d, name=name) E = d.ellipsoid p = str(pole or p)[:1].upper() N = p == _N_ # is north a = lat if N else -lat A = abs(a - _90_0) < _Tol90 # at pole t = tan(radians(a)) T = E.es_taupf(t) r = hypot1(T) + abs(T) if T >= _0_0: r = _0_0 if A else _1_0 / r k0 = getattr(Ups, '_scale0', _K0_UPS) # Ups is class or None r *= 2 * k0 * E.a / E.es_c k = k0 if A else _scale(E, r, t) c = lon # [-180, 180) from .upsZoneBand5 x, y = sincos2d(c) x *= r y *= r if N: y = neg(y) else: c = neg(c) if falsed: x += _Falsing y += _Falsing n = name or nameof(latlon) if Ups is None: r = UtmUps8Tuple(z, p, x, y, B, d, c, k, Error=UPSError, name=n) else: if z != _UPS_ZONE and not strict: z = _UPS_ZONE # ignore UTM zone r = _xnamed(Ups(z, p, x, y, band=B, datum=d, falsed=falsed, convergence=c, scale=k), n) r._hemisphere = _hemi(lat) if isinstance(latlon, _LLEB) and d is latlon.datum: r._latlon_to(latlon, falsed) # XXX weakref(latlon)? return r def upsZoneBand5(lat, lon, strict=True, name=NN): '''Return the UTM/UPS zone number, (polar) Band letter, pole and clipped lat- and longitude for a given location. @arg lat: Latitude in degrees (C{scalar} or C{str}). @arg lon: Longitude in degrees (C{scalar} or C{str}). @kwarg strict: Restrict B{C{lat}} to UPS ranges (C{bool}). @kwarg name: Optional name (C{str}). @return: A L{UtmUpsLatLon5Tuple}C{(zone, band, hemipole, lat, lon)} where C{hemipole} is the C{'N'|'S'} pole, the UPS projection top/center. @raise RangeError: If B{C{strict}} and B{C{lat}} in the UTM and not the UPS range or if B{C{lat}} or B{C{lon}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @raise ValueError: Invalid B{C{lat}} or B{C{lon}}. ''' z, lat, lon = _to3zll(*parseDMS2(lat, lon)) if lat < _UPS_LAT_MIN: # includes 30' overlap z, B, p = _UPS_ZONE, _Band(lat, lon), _S_ elif lat > _UPS_LAT_MAX: # includes 30' overlap z, B, p = _UPS_ZONE, _Band(lat, lon), _N_ elif strict: r = _range_(_UPS_LAT_MIN, _UPS_LAT_MAX) t = _SPACE_(_inside_, _UTM_, _range_, r) raise RangeError(lat=degDMS(lat), txt=t) else: B, p = NN, _hemi(lat) return UtmUpsLatLon5Tuple(z, B, p, lat, lon, Error=UPSError, name=name) # **) MIT License # # Copyright (C) 2016-2021 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.