Package VisionEgg :: Module DaqLPT :: Class LPTDevice |
[frames] | no frames]

# Class LPTDevice

source code

    Daq.Device --+
                 |
                LPTDevice

    A single parallel port. (Line PrinTer port.)

    Typically, LPT1 has a base address of 0x0378, and LPT2 has a base
    address of 0x0278.

Instance Methods
__init__(self, base_address=0x378, **kw) | source code
add_channel(self, channel) | source code

Method Details

### __init__(self, base_address=0x378, **kw) (Constructor) | source code
Overrides: Daq.Device.__init__

### add_channel(self, channel) | source code
Overrides: Daq.Device.add_channel