# Coverage for pygeodesy/ellipsoidalNvector.py : 99%

## 117 statements 116 run 1 missing 3 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 616 617 618 619 620 621 622 623 624 625 626 627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 657 658 659 660 661 662 663 664 665 666 667 668 669 670 671 672 673 674 675 676 677 678 679 680 681 682 683 684 685 686 687 688 689 690 691 692 693 694 695 696 697 698 699 700 701 702 703 704 705 706 707 708 709 710 711 712 713 714 715 716 717 718 719 720 721 722 723 724 725 726 727 728 729 730 731 732 733 734 735 736 737 738 739 740 741 742 743 744 | # -*- coding: utf-8 -*- u'''Ellipsoidal, C{N-vector}-based geodesy. Ellipsoidal classes geodetic (lat-/longitude) L{LatLon}, geocentric (ECEF) L{Cartesian}, L{Ned} and L{Nvector} and functions L{meanOf}, L{sumOf} and L{toNed}. Pure Python implementation of n-vector-based geodetic (lat-/longitude) methods by I{(C) Chris Veness 2011-2016} published under the same MIT Licence**, see U{Vector-based geodesy <https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}. These classes and functions work with: (a) geodesic (polar) lat-/longitude points on the earth's surface and (b) 3-D vectors used as n-vectors representing points on the earth's surface or vectors normal to the plane of a great circle. See also Kenneth Gade U{'A Non-singular Horizontal Position Representation' <https://www.NavLab.net/Publications/A_Nonsingular_Horizontal_Position_Representation.pdf>}, The Journal of Navigation (2010), vol 63, nr 3, pp 395-417. ''' # make sure int/int division yields float quotient, see .basics from __future__ import division as _; del _ # PYCHOK semicolon # from pygeodesy.basics import _xinstanceof # from .ltpTuples from pygeodesy.datums import _ellipsoidal_datum, _spherical_datum, _WGS84 from pygeodesy.ellipsoidalBase import CartesianEllipsoidalBase, _TOL_M, \ LatLonEllipsoidalBase, _nearestOn # from pygeodesy.errors import _xkwds # from .ltpTuples # from pygeodesy.fmath import fdot # from .nvectorBase from pygeodesy.interns import NN, _Nv00_, _COMMASPACE_ from pygeodesy.interns import _down_, _east_, _north_, _pole_ # PYCHOK used! from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS, _ALL_OTHER from pygeodesy.ltpTuples import Aer as _Aer, Ned as _Ned, sincos2d_, \ _xinstanceof, _xkwds, _xnamed # from pygeodesy.named import _xnamed # from .ltpTuples from pygeodesy.nvectorBase import fdot, NorthPole, LatLonNvectorBase, \ NvectorBase, sumOf as _sumOf from pygeodesy.props import deprecated_class, deprecated_function, \ deprecated_method, Property_RO from pygeodesy.streprs import Fmt, fstr, _xzipairs from pygeodesy.units import Bearing, Distance, Height, Scalar # from pygeodesy.utily import sincos2d_ # from .ltpTuples __all__ = _ALL_LAZY.ellipsoidalNvector __version__ = '22.08.07' class Cartesian(CartesianEllipsoidalBase): '''Extended to convert geocentric, L{Cartesian} points to L{Nvector} and n-vector-based, geodetic L{LatLon}. ''' @Property_RO def Ecef(self): '''Get the ECEF I{class} (L{EcefVeness}), I{lazily}. ''' return _MODS.ecef.EcefVeness def toLatLon(self, **LatLon_and_kwds): # PYCHOK LatLon=LatLon, datum=None '''Convert this cartesian to an C{Nvector}-based geodetic point. @kwarg LatLon_and_kwds: Optional L{LatLon}, B{C{datum}} and other keyword arguments. Use C{B{LatLon}=...} to override this L{LatLon} class or specify C{B{LatLon} is None}. @return: The geodetic point (L{LatLon}) or if B{C{LatLon}} is set to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with C{C} and C{M} if available. @raise TypeError: Invalid B{C{LatLon_and_kwds}}. ''' kwds = _xkwds(LatLon_and_kwds, LatLon=LatLon, datum=self.datum) return CartesianEllipsoidalBase.toLatLon(self, **kwds) def toNvector(self, **Nvector_and_kwds): # PYCHOK Datums.WGS84 '''Convert this cartesian to L{Nvector} components, I{including height}. @kwarg Nvector_and_kwds: Optional L{Nvector}, B{C{datum}} and other keyword arguments. Use C{B{Nvector}=...} to override this L{Nvector} class or specify C{B{Nvector} is None}. @return: The C{n-vector} components (L{Nvector}) or if B{C{Nvector}} is set to C{None}, a L{Vector4Tuple}C{(x, y, z, h)} @raise TypeError: Invalid B{C{Nvector_and_kwds}}. @example: >>> from ellipsoidalNvector import LatLon >>> c = Cartesian(3980581, 97, 4966825) >>> n = c.toNvector() # (0.62282, 0.000002, 0.78237, +0.24) ''' kwds = _xkwds(Nvector_and_kwds, Nvector=Nvector, datum=self.datum) return CartesianEllipsoidalBase.toNvector(self, **kwds) class LatLon(LatLonNvectorBase, LatLonEllipsoidalBase): '''An n-vector-based, ellipsoidal L{LatLon} point. @example: >>> from ellipsoidalNvector import LatLon >>> p = LatLon(52.205, 0.119) # height=0, datum=Datums.WGS84 ''' _Nv = None # cached toNvector (L{Nvector}) def _update(self, updated, *attrs): # PYCHOK args '''(INTERNAL) Zap cached attributes if updated. ''' if updated: LatLonNvectorBase._update(self, updated, _Nv=self._Nv) # special case LatLonEllipsoidalBase._update(self, updated, *attrs) # def crossTrackDistanceTo(self, start, end, radius=R_M): # '''Return the (signed) distance from this point to the great # circle defined by a start point and an end point or bearing. # # @arg start: Start point of great circle path (L{LatLon}). # @arg end: End point of great circle path (L{LatLon}) or # initial bearing (compass C{degrees360}) at the # start point. # @kwarg radius: Mean earth radius (C{meter}). # # @return: Distance to great circle, negative if to left or # positive if to right of path (C{meter}, same units # as B{C{radius}}). # # @raise TypeError: If B{C{start}} or B{C{end}} point is not L{LatLon}. # # @example: # # >>> p = LatLon(53.2611, -0.7972) # # >>> s = LatLon(53.3206, -1.7297) # >>> b = 96.0 # >>> d = p.crossTrackDistanceTo(s, b) # -305.7 # # >>> e = LatLon(53.1887, 0.1334) # >>> d = p.crossTrackDistanceTo(s, e) # -307.5 # ''' # self.others(start=start) # # if isscalar(end): # gc from point and bearing # gc = start.greatCircle(end) # else: # gc by two points # gc = start.toNvector().cross(end.toNvector()) # # # (signed) angle between point and gc normal vector # v = self.toNvector() # a = gc.angleTo(v, vSign=v.cross(gc)) # a = (-PI_2 - a) if a < 0 else (PI_2 - a) # return a * float(radius) def deltaTo(self, other): '''Calculate the local delta from this to an other point. The delta is returned as a North-East-Down (NED) vector. Note, this is a linear delta, unrelated to a geodesic on the ellipsoid. The points need not be defined on the same datum. @arg other: The other point (L{LatLon}). @return: Delta of this point (L{Ned}). @raise TypeError: The B{C{other}} point is not L{LatLon}. @raise ValueError: If ellipsoids are incompatible. @example: >>> a = LatLon(49.66618, 3.45063) >>> b = LatLon(48.88667, 2.37472) >>> delta = a.deltaTo(b) # [N:-86126, E:-78900, D:1069] >>> d = delta.length # 116807.681 m >>> b = delta.bearing # 222.493° >>> e = delta.elevation # -0.5245° ''' self.ellipsoids(other) # throws TypeError and ValueError # get delta in cartesian frame dc = other.toCartesian().minus(self.toCartesian()) # rotate dc to get delta in n-vector reference # frame using the rotation matrix row vectors nv, ev, dv = self._rotation3 return Ned(dc.dot(nv), dc.dot(ev), dc.dot(dv), name=self.name) # def destination(self, distance, bearing, radius=R_M, height=None): # '''Return the destination point after traveling from this # point the given distance on the given initial bearing. # # @arg distance: Distance traveled (C{meter}, same units as # given earth B{C{radius}}). # @arg bearing: Initial bearing (compass C{degrees360}). # @kwarg radius: Mean earth radius (C{meter}). # @kwarg height: Optional height at destination point, # overriding default (C{meter}, same units # as B{C{radius}}). # # @return: Destination point (L{LatLon}). # # @example: # # >>> p = LatLon(51.4778, -0.0015) # >>> q = p.destination(7794, 300.7) # >>> q.toStr() # '51.5135°N, 000.0983°W' ? # ''' # r = _angular(distance, radius) # angular distance in radians # # great circle by starting from this point on given bearing # gc = self.greatCircle(bearing) # # v1 = self.toNvector() # x = v1.times(cos(r)) # component of v2 parallel to v1 # y = gc.cross(v1).times(sin(r)) # component of v2 perpendicular to v1 # # v2 = x.plus(y).unit() # return v2.toLatLon(height=self.height if height is C{None} else height) def destinationNed(self, delta): '''Calculate the destination point using the supplied NED delta from this point. @arg delta: Delta from this to the other point in the local tangent plane (LTP) of this point (L{Ned}). @return: Destination point (L{LatLon}). @raise TypeError: If B{C{delta}} is not L{Ned}. @example: >>> a = LatLon(49.66618, 3.45063) >>> delta = Ned(-86126, -78900, 1069) # from Aer(222.493, -0.5245, 116807.681) >>> b = a.destinationNed(delta) # 48.886669°N, 002.374721°E or 48°53′12.01″N, 002°22′29.0″E +0.20m ''' _xinstanceof(Ned, delta=delta) nv, ev, dv = self._rotation3 # convert NED delta to standard coordinate frame of n-vector dn = delta.ned # rotate dn to get delta in cartesian (ECEF) coordinate # reference frame using the rotation matrix column vectors dc = Cartesian(fdot(dn, nv.x, ev.x, dv.x), fdot(dn, nv.y, ev.y, dv.y), fdot(dn, nv.z, ev.z, dv.z)) # apply (cartesian) delta to this Cartesian to obtain destination as cartesian v = self.toCartesian().plus(dc) return v.toLatLon(datum=self.datum, LatLon=self.classof) # Cartesian(v.x, v.y, v.z).toLatLon(...) def distanceTo(self, other, radius=None, wrap=False): '''I{Approximate} the distance from this to an other point. @arg other: The other point (L{LatLon}). @kwarg radius: Mean earth radius, ellipsoid or datum (C{meter}, L{Ellipsoid}, L{Ellipsoid2}, L{Datum} or L{a_f2Tuple}), overriding the mean radius C{R1} of this point's datum.. @kwarg wrap: Wrap/unroll the angular distance (C{bool}). @return: Distance (C{meter}, same units as B{C{radius}}). @raise TypeError: The B{C{other}} point is not L{LatLon}. @raise ValueError: Invalid B{C{radius}}. @example: >>> p = LatLon(52.205, 0.119) >>> q = LatLon(48.857, 2.351); >>> d = p.distanceTo(q) # 404300 ''' self.others(other) a = self._N_vector.angleTo(other._N_vector, wrap=wrap) d = self.datum if radius is None else _spherical_datum(radius) return abs(a) * d.ellipsoid.R1 # see .utily.radians2m @Property_RO def Ecef(self): '''Get the ECEF I{class} (L{EcefVeness}), I{lazily}. ''' return _MODS.ecef.EcefVeness @deprecated_method def equals(self, other, eps=None): # PYCHOK no cover '''DEPRECATED, use method L{isequalTo}. ''' return self.isequalTo(other, eps=eps) def isequalTo(self, other, eps=None): '''Compare this point with an other point. @arg other: The other point (L{LatLon}). @kwarg eps: Optional margin (C{float}). @return: C{True} if points are identical, including datum, I{ignoring height}, C{False} otherwise. @raise TypeError: The B{C{other}} point is not L{LatLon}. @raise ValueError: Invalid B{C{eps}}. @see: Method C{isequalTo3} to include I{height}. @example: >>> p = LatLon(52.205, 0.119) >>> q = LatLon(52.205, 0.119) >>> e = p.isequalTo(q) # True ''' return LatLonEllipsoidalBase.isequalTo(self, other, eps=eps) \ if self.datum == other.datum else False # def greatCircle(self, bearing): # '''Return the great circle heading on the given bearing # from this point. # # Direction of vector is such that initial bearing vector # b = c × p, where p is representing this point. # # @arg bearing: Bearing from this point (compass C{degrees360}). # # @return: N-vector representing great circle (L{Nvector}). # # @example: # # >>> p = LatLon(53.3206, -1.7297) # >>> g = p.greatCircle(96.0) # >>> g.toStr() # '(-0.794, 0.129, 0.594)' # ''' # a, b, _ = self.philamheight # t = radians(bearing) # # sa, ca, sb, cb, st, ct = sincos2_(a, b, t) # return self._xnamed(Nvector(sb * ct - sa * cb * st, # -cb * ct - sa * sb * st, # ca * st) # def initialBearingTo(self, other): # '''Return the initial bearing (forward azimuth) from this # to an other point. # # @arg other: The other point (L{LatLon}). # # @return: Initial bearing (compass C{degrees360}). # # @raise TypeError: The B{C{other}} point is not L{LatLon}. # # @example: # # >>> p1 = LatLon(52.205, 0.119) # >>> p2 = LatLon(48.857, 2.351) # >>> b = p1.bearingTo(p2) # 156.2 # ''' # self.others(other) # # v1 = self.toNvector() # v2 = other.toNvector() # # gc1 = v1.cross(v2) # gc through v1 & v2 # gc2 = v1.cross(_NP3) # gc through v1 & North pole # # # bearing is (signed) angle between gc1 & gc2 # return degrees360(gc1.angleTo(gc2, vSign=v1)) def intermediateTo(self, other, fraction, height=None, **unused): # PYCHOK wrap=False '''Return the point at given fraction between this and an other point. @arg other: The other point (L{LatLon}). @arg fraction: Fraction between both points (C{scalar}, 0.0 at this to 1.0 at the other point. @kwarg height: Optional height, overriding the fractional height (C{meter}). @return: Intermediate point (L{LatLon}). @raise TypeError: The B{C{other}} point is not L{LatLon}. @example: >>> p = LatLon(52.205, 0.119) >>> q = LatLon(48.857, 2.351) >>> p = p.intermediateTo(q, 0.25) # 51.3721°N, 000.7073°E ''' self.others(other) f = Scalar(fraction=fraction) i = self.toNvector().intermediateTo(other.toNvector(), f) h = self._havg(other, f=f) if height is None else Height(height) return i.toLatLon(height=h, LatLon=self.classof) # Nvector(i.x, i.y, i.z).toLatLon(...) @Property_RO def _rotation3(self): '''(INTERNAL) Get the rotation matrix from n-vector coordinate frame axes. ''' nv = self.toNvector() # local (n-vector) coordinate frame dv = nv.negate() # down, opposite to n-vector ev = NorthPole.cross(nv, raiser=_pole_).unit() # east, pointing perpendicular to the plane nv = ev.cross(dv) # north, by right hand rule return nv, ev, dv # matrix rows def toCartesian(self, **Cartesian_and_kwds): # PYCHOK Cartesian=Cartesian, datum=None '''Convert this point to an C{Nvector}-based geodetic point. @kwarg Cartesian_and_kwds: Optional L{Cartesian}, B{C{datum}} and other keyword arguments. Use C{B{Cartesian}=...} to override this L{Cartesian} class or specify C{B{Cartesian} is None}. @return: The geodetic point (L{Cartesian}) or if B{C{Cartesian}} is set to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with C{C} and C{M} if available. @raise TypeError: Invalid B{C{Cartesian}} or other B{C{Cartesian_and_kwds}}. ''' kwds = _xkwds(Cartesian_and_kwds, Cartesian=Cartesian, datum=self.datum) return LatLonEllipsoidalBase.toCartesian(self, **kwds) def toNvector(self, **Nvector_and_kwds): # PYCHOK signature '''Convert this point to L{Nvector} components, I{including height}. @kwarg Nvector_and_kwds: Optional L{Nvector}, B{C{datum}} and other keyword arguments. Use C{B{Nvector}=...} to override this L{Nvector} class or specify C{B{Nvector} is None}. @return: The C{n-vector} components (L{Nvector}) or if B{C{Nvector}} is set to C{None}, a L{Vector4Tuple}C{(x, y, z, h)}. @raise TypeError: Invalid B{C{Nvector}} or other B{C{Nvector_and_kwds}}. @example: >>> p = LatLon(45, 45) >>> n = p.toNvector() >>> n.toStr() # [0.50, 0.50, 0.70710] ''' kwds = _xkwds(Nvector_and_kwds, Nvector=Nvector, datum=self.datum) return LatLonNvectorBase.toNvector(self, **kwds) class Ned(_Ned): '''DEPRECATED, use class L{pygeodesy.Ned}.''' def __init__(self, north, east, down, name=NN): deprecated_class(self.__class__) _Ned.__init__(self, north, east, down, name=name) @deprecated_method # PYCHOK expected def toRepr(self, prec=None, fmt=Fmt.SQUARE, sep=_COMMASPACE_, **unused): '''DEPRECATED, use class L{pygeodesy.Ned}. Return a string representation of this NED vector as length, bearing and elevation. @kwarg prec: Number of (decimal) digits, unstripped (C{int}). @kwarg fmt: Enclosing backets format (C{str}). @kwarg sep: Separator between NEDs (C{str}). @return: This Ned as "[L:f, B:degrees360, E:degrees90]" (C{str}). ''' dms = _MODS.dms t = (fstr(self.slantrange, prec=3 if prec is None else prec), dms.toDMS(self.azimuth, form=dms.F_D, prec=prec, ddd=0), dms.toDMS(self.elevation, form=dms.F_D, prec=prec, ddd=0)) return _xzipairs('LBE', t, sep=sep, fmt=fmt) _Nvll = LatLon(0, 0, name=_Nv00_) # reference instance (L{LatLon}) class Nvector(NvectorBase): '''An n-vector is a position representation using a (unit) vector normal to the earth ellipsoid. Unlike lat-/longitude points, n-vectors have no singularities or discontinuities. For many applications, n-vectors are more convenient to work with than other position representations like lat-/longitude, earth-centred earth-fixed (ECEF) vectors, UTM coordinates, etc. Note commonality with L{sphericalNvector.Nvector}. ''' _datum = _WGS84 # default datum (L{Datum}) def __init__(self, x_xyz, y=None, z=None, h=0, datum=None, ll=None, name=NN): '''New n-vector normal to the earth's surface. @arg x_xyz: X component of vector (C{scalar}) or (3-D) vector (C{Nvector}, L{Vector3d}, L{Vector3Tuple} or L{Vector4Tuple}). @kwarg y: Y component of vector (C{scalar}), ignored if B{C{x_xyz}} is not C{scalar}, otherwise same units as B{C{x_xyz}}. @kwarg z: Z component of vector (C{scalar}), ignored if B{C{x_xyz}} is not C{scalar}, otherwise same units as B{C{x_xyz}}. @kwarg h: Optional height above model surface (C{meter}). @kwarg datum: Optional datum this n-vector is defined in (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg ll: Optional, original latlon (C{LatLon}). @kwarg name: Optional name (C{str}). @raise TypeError: If B{C{datum}} is not a L{Datum}. @example: >>> from ellipsoidalNvector import Nvector >>> v = Nvector(0.5, 0.5, 0.7071, 1) >>> v.toLatLon() # 45.0°N, 045.0°E, +1.00m ''' NvectorBase.__init__(self, x_xyz, y=y, z=z, h=h, ll=ll, name=name) if datum not in (None, self._datum): self._datum = _ellipsoidal_datum(datum, name=name) @Property_RO def datum(self): '''Get this n-vector's datum (L{Datum}). ''' return self._datum def toCartesian(self, **Cartesian_and_kwds): # PYCHOK Cartesian=Cartesian '''Convert this n-vector to C{Nvector}-based cartesian (ECEF) coordinates. @kwarg Cartesian_and_kwds: Optional L{Cartesian}, B{C{h}}, B{C{datum}} and other keyword arguments. Use C{B{Cartesian}=...} to override this L{Cartesian} class or specify C{B{Cartesian} is None}. @return: The cartesian point (L{Cartesian}) or if B{C{Cartesian}} is set to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with C{C} and C{M} if available. @raise TypeError: Invalid B{C{Cartesian_and_kwds}}. @example: >>> v = Nvector(0.5, 0.5, 0.7071) >>> c = v.toCartesian() # [3194434, 3194434, 4487327] >>> p = c.toLatLon() # 45.0°N, 45.0°E ''' kwds = _xkwds(Cartesian_and_kwds, h=self.h, Cartesian=Cartesian, datum=self.datum) return NvectorBase.toCartesian(self, **kwds) # class or .classof def toLatLon(self, **LatLon_and_kwds): # PYCHOK height=None, LatLon=LatLon '''Convert this n-vector to an C{Nvector}-based geodetic point. @kwarg LatLon_and_kwds: Optional L{LatLon}, B{C{height}}, B{C{datum}} and other keyword arguments. Use C{B{LatLon}=...} to override this L{LatLon} class or specify C{B{LatLon} is None}. @return: The geodetic point (L{LatLon}) or if B{C{LatLon}} is set to C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with C{C} and C{M} if available. @raise TypeError: Invalid B{C{LatLon_and_kwds}}. @example: >>> v = Nvector(0.5, 0.5, 0.7071) >>> p = v.toLatLon() # 45.0°N, 45.0°E ''' kwds = _xkwds(LatLon_and_kwds, height=self.h, datum=self.datum, LatLon=LatLon) return NvectorBase.toLatLon(self, **kwds) # class or .classof def unit(self, ll=None): '''Normalize this vector to unit length. @kwarg ll: Optional, original latlon (C{LatLon}). @return: Normalised vector (L{Nvector}). ''' u = NvectorBase.unit(self, ll=ll) if u.datum != self.datum: u._update(False, datum=self.datum) return u def meanOf(points, datum=_WGS84, height=None, LatLon=LatLon, **LatLon_kwds): '''Compute the geographic mean of several points. @arg points: Points to be averaged (L{LatLon}[]). @kwarg datum: Optional datum to use (L{Datum}). @kwarg height: Optional height at mean point, overriding the mean height (C{meter}). @kwarg LatLon: Optional class to return the mean point (L{LatLon}) or C{None}. @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: Geographic mean point and mean height (B{C{LatLon}}) or if B{C{LatLon}} is C{None}, an L{Ecef9Tuple}C{(x, y, z, lat, lon, height, C, M, datum)} with C{C} and C{M} if available. @raise ValueError: Insufficient number of B{C{points}}. ''' Ps = _Nvll.PointsIter(points) # geographic mean m = sumOf(p._N_vector for p in Ps.iterate(closed=False)) kwds = _xkwds(LatLon_kwds, height=height, datum=datum, LatLon=LatLon, name=meanOf.__name__) return m.toLatLon(**kwds) def nearestOn(point, point1, point2, within=True, height=None, wrap=False, equidistant=None, tol=_TOL_M, LatLon=LatLon, **LatLon_kwds): '''Iteratively locate the closest point on the geodesic between two other (ellipsoidal) points. @arg point: Reference point (C{LatLon}). @arg point1: Start point of the geodesic (C{LatLon}). @arg point2: End point of the geodesic (C{LatLon}). @kwarg within: If C{True} return the closest point I{between} B{C{point1}} and B{C{point2}}, otherwise the closest point elsewhere on the geodesic (C{bool}). @kwarg height: Optional height for the closest point (C{meter}, conventionally) or C{None} or C{False} for the interpolated height. If C{False}, the closest takes the heights of the points into account. @kwarg wrap: Wrap and unroll longitudes (C{bool}). @kwarg equidistant: An azimuthal equidistant projection (I{class} or function L{pygeodesy.equidistant}) or C{None} for the preferred C{B{point}.Equidistant}. @kwarg tol: Convergence tolerance (C{meter}). @kwarg LatLon: Optional class to return the closest point (L{LatLon}) or C{None}. @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: Closest point, a B{C{LatLon}} instance or if C{B{LatLon} is None}, a L{LatLon4Tuple}C{(lat, lon, height, datum)}. @raise ImportError: Package U{geographiclib <https://PyPI.org/project/geographiclib>} not installed or not found. @raise TypeError: Invalid or non-ellipsoidal B{C{point}}, B{C{point1}} or B{C{point2}} or invalid B{C{equidistant}}. @raise ValueError: No convergence for the B{C{tol}}. @see: U{The B{ellipsoidal} case<https://GIS.StackExchange.com/questions/48937/ calculating-intersection-of-two-circles>} and U{Karney's paper <https://ArXiv.org/pdf/1102.1215.pdf>}, pp 20-21, section B{14. MARITIME BOUNDARIES} for more details about the iteration algorithm. ''' return _nearestOn(point, point1, point2, within=within, height=height, wrap=wrap, equidistant=equidistant, tol=tol, LatLon=LatLon, **LatLon_kwds) def sumOf(nvectors, Vector=Nvector, h=None, **Vector_kwds): '''Return the vectorial sum of two or more n-vectors. @arg nvectors: Vectors to be added (L{Nvector}[]). @kwarg Vector: Optional class for the vectorial sum (L{Nvector}). @kwarg h: Optional height, overriding the mean height (C{meter}). @kwarg Vector_kwds: Optional, additional B{C{Vector}} keyword arguments, ignored if C{B{Vector} is None}. @return: Vectorial sum (B{C{Vector}}). @raise VectorError: No B{C{nvectors}}. ''' return _sumOf(nvectors, Vector=Vector, h=h, **Vector_kwds) @deprecated_function def toNed(distance, bearing, elevation, Ned=Ned, name=NN): '''DEPRECATED, use L{pygeodesy.Aer}C{(bearing, elevation, distance).xyzLocal.toNed(B{Ned}, name=B{name})} or L{XyzLocal}C{(pygeodesy.Aer(bearing, elevation, distance)).toNed(B{Ned}, name=B{name})}. Create an NED vector from distance, bearing and elevation (in local coordinate system). @arg distance: NED vector length (C{meter}). @arg bearing: NED vector bearing (compass C{degrees360}). @arg elevation: NED vector elevation from local coordinate frame horizontal (C{degrees}). @kwarg Ned: Optional class to return the NED (C{Ned}) or C{None}. @kwarg name: Optional name (C{str}). @return: An NED vector equivalent to this B{C{distance}}, B{C{bearing}} and B{C{elevation}} (DEPRECATED L{Ned}) or a DEPRECATED L{Ned3Tuple}C{(north, east, down)} if C{B{Ned} is None}. @raise ValueError: Invalid B{C{distance}}, B{C{bearing}} or B{C{elevation}}. ''' if True: # use new Aer class n, e, d, _ = _Aer(bearing, elevation, distance).xyz4 else: # DEPRECATED d = Distance(distance) sb, cb, se, ce = sincos2d_(Bearing(bearing), Height(elevation=elevation)) n = cb * d * ce e = sb * d * ce d *= se r = _MODS.deprecated.Ned3Tuple(n, e, -d) if Ned is None else \ Ned(n, e, -d) return _xnamed(r, name) __all__ += _ALL_OTHER(Cartesian, LatLon, Ned, Nvector, # classes meanOf, sumOf, toNed) # **) MIT License # # Copyright (C) 2016-2022 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.