# Coverage for pygeodesy/dms.py : 99%

## 241 statements 240 run 1 missing 31 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 616 617 618 619 620 621 622 623 624 625 626 627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 657 658 659 660 661 662 663 664 665 666 667 668 669 670 671 672 673 674 675 676 677 678 679 680 681 682 683 684 685 686 687 688 689 690 691 692 693 694 695 696 697 698 699 700 701 702 703 704 705 706 707 708 709 710 711 712 713 714 715 716 717 718 719 720 721 722 723 724 725 726 727 728 729 730 731 732 733 734 735 736 737 738 739 740 741 742 743 744 745 746 747 748 749 750 751 752 753 754 755 756 757 758 759 760 761 762 763 764 765 766 767 768 769 770 771 772 773 774 775 776 777 778 779 780 781 782 783 784 785 786 787 788 | # -*- coding: utf-8 -*- u'''Parsers and formatters of degrees, minutes and seconds. Functions to parse and format bearing, compass, lat- and longitudes in various forms of degrees, minutes and seconds. After I{(C) Chris Veness 2011-2015} published under the same MIT Licence**, see U{Latitude/Longitude<https://www.Movable-Type.co.UK/scripts/latlong.html>} and U{Vector-based geodesy<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}. ''' from pygeodesy.basics import copysign0, isodd, issequence, isstr, map2, neg from pygeodesy.errors import ParseError, _parseX, RangeError, \ _rangerrors, _ValueError from pygeodesy.interns import _COMMA_, _NE_, _NSEW_, _NW_, _SE_ # PYCHOK used! from pygeodesy.interns import NN, _deg_, _degrees_, _DOT_, _e_, _E_, \ _f_, _g_, _MINUS_, _PLUSMINUS_, _EW_, \ _N_, _NS_, _PERCENTDOTSTAR_, _PLUS_, \ _radians_, _S_, _SPACE_, _SW_, _W_, _0_, \ _0_5, _60_0, _360_0, _3600_0 from pygeodesy.lazily import _ALL_LAZY from pygeodesy.streprs import Fmt, fstr, fstrzs, _0wpF from math import modf, radians try: from string import letters as _LETTERS except ImportError: # Python 3+ from string import ascii_letters as _LETTERS __all__ = _ALL_LAZY.dms __version__ = '21.10.05' F_D = 'd' # unsigned format "deg°" plus suffix N, S, E or W F_DM = 'dm' # unsigned format "deg°min′" plus suffix F_DMS = 'dms' # unsigned format "deg°min′sec″" plus suffix F_DEG = _deg_ # unsigned format "[D]DD" plus suffix without symbol F_MIN = 'min' # unsigned format "[D]DDMM" plus suffix without symbols F_SEC = 'sec' # unsigned format "[D]DDMMSS" plus suffix without symbols F__E = _e_ # unsigned format "%E" plus suffix without symbol F__F = _f_ # unsigned format "%F" plus suffix without symbol F__G = _g_ # unsigned format "%G" plus suffix without symbol F_RAD = 'rad' # convert degrees to radians and format unsigned "RR" plus suffix F_D_ = '-d' # signed format "-/deg°" without suffix F_DM_ = '-dm' # signed format "-/deg°min′" without suffix F_DMS_ = '-dms' # signed format "-/deg°min′sec″" without suffix F_DEG_ = '-deg' # signed format "-/[D]DD" without suffix and symbol F_MIN_ = '-min' # signed format "-/[D]DDMM" without suffix and symbols F_SEC_ = '-sec' # signed format "-/[D]DDMMSS" without suffix and symbols F__E_ = '-e' # signed format "-%E" without suffix and symbol F__F_ = '-f' # signed format "-%F" without suffix and symbol F__G_ = '-g' # signed format "-%G" without suffix and symbol F_RAD_ = '-rad' # convert degrees to radians and format as signed "-/RR" without suffix F_D__ = '+d' # signed format "-/+deg°" without suffix F_DM__ = '+dm' # signed format "-/+deg°min′" without suffix F_DMS__ = '+dms' # signed format "-/+deg°min′sec″" without suffix F_DEG__ = '+deg' # signed format "-/+[D]DD" without suffix and symbol F_MIN__ = '+min' # signed format "-/+[D]DDMM" without suffix and symbols F_SEC__ = '+sec' # signed format "-/+[D]DDMMSS" without suffix and symbols F__E__ = '+e' # signed format "-/+%E" without suffix and symbol F__F__ = '+f' # signed format "-/+%F" without suffix and symbol F__G__ = '+g' # signed format "-/+%G" without suffix and symbol F_RAD__ = '+rad' # convert degrees to radians and format signed "-/+RR" without suffix S_DEG = '°' # degrees "°" symbol S_MIN = '′' # minutes "′" symbol S_SEC = '″' # seconds "″" symbol S_RAD = NN # radians symbol "" S_SEP = NN # separator between deg, min and sec "" S_NUL = NN # empty string _F_case = {F_D: F_D, F_DEG: F_D, _degrees_: F_D, F_DM: F_DM, F_MIN: F_DM, 'deg+min': F_DM, F__E: F__E, F__F: F__F, F__G: F__G, F_RAD: F_RAD, _radians_: F_RAD} _F_prec = {F_D: 6, F_DM: 4, F_DMS: 2, # default precs F_DEG: 6, F_MIN: 4, F_SEC: 2, F__E: 8, F__F: 8, F__G: 8, F_RAD: 5} _F_symb = {F_DEG, F_MIN, F_SEC, F__E, F__F, F__G} # set({}) pychok -Tb _S_norm = {'^': S_DEG, '˚': S_DEG, # normalized DMS "'": S_MIN, '’': S_MIN, '′': S_MIN, '"': S_SEC, '″': S_SEC, '”': S_SEC} _S_ALL = (S_DEG, S_MIN, S_SEC) + tuple(_S_norm.keys()) # alternates def _toDMS(deg, form, prec, sep, ddd, suff): # MCCABE 15 by .units.py '''(INTERNAL) Convert degrees to C{str}, with/-out sign and/or suffix. ''' try: deg = float(deg) except (TypeError, ValueError) as x: raise _ValueError(deg=deg, txt=str(x)) form = form.lower() sign = form[:1] if sign in _PLUSMINUS_: form = form[1:] else: sign = S_NUL if prec is None: z = p = _F_prec.get(form, 6) else: z = int(prec) p = abs(z) w = p + (1 if p else 0) d = abs(deg) if form in _F_symb: s_deg = s_min = s_sec = S_NUL # no symbols else: s_deg, s_min, s_sec = S_DEG, S_MIN, S_SEC F = _F_case.get(form, F_DMS) if F is F_DMS: # 'deg+min+sec' d, s = divmod(round(d * _3600_0, p), _3600_0) m, s = divmod(s, _60_0) t = NN(_0wpF(ddd, 0, d), s_deg, sep, _0wpF( 2, 0, m), s_min, sep, _0wpF(w+2, p, s)) s = s_sec elif F is F_DM: # 'deg+min' d, m = divmod(round(d * _60_0, p), _60_0) t = NN(_0wpF(ddd, 0, d), s_deg, sep, _0wpF(w+2, p, m)) s = s_min elif F is F_D: # 'deg' t = _0wpF(ddd+w, p, d) s = s_deg elif F is F_RAD: t = NN(_PERCENTDOTSTAR_, 'F') % (p, radians(d)) s = S_RAD else: # F in (F__E, F__F, F__G) t = NN(_PERCENTDOTSTAR_, F) % (p, d) s = S_NUL if z > 1: t = fstrzs(t, ap1z=F is F__G) if sign: if deg < 0: t = _MINUS_ + t elif deg > 0 and sign == _PLUS_: t = _PLUS_ + t elif suff: # and deg: # zero suffix? s += sep + suff return t + s def bearingDMS(bearing, form=F_D, prec=None, sep=S_SEP): '''Convert bearing to a string. @arg bearing: Bearing from North (compass C{degrees360}). @kwarg form: Optional B{C{bearing}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Optional separator (C{str}). @return: Compass degrees per the specified B{C{form}} (C{str}). @JSname: I{toBrng}. ''' return _toDMS(bearing % _360_0, form, prec, sep, 1, NN) def _clipped_(angle, limit, units): '''(INTERNAL) Helper for C{clipDegrees} and C{clipRadians}. ''' c = min(limit, max(-limit, angle)) if c != angle and _rangerrors: t = _SPACE_(fstr(angle, prec=6, ints=True), 'beyond', copysign0(limit, angle), units) raise RangeError(t, txt=None) return c def clipDegrees(deg, limit): '''Clip a lat- or longitude to the given range. @arg deg: Unclipped lat- or longitude (C{degrees}). @arg limit: Valid B{C{-limit..+limit}} range (C{degrees}). @return: Clipped value (C{degrees}). @raise RangeError: If B{C{abs(deg)}} beyond B{C{limit}} and L{pygeodesy.rangerrors} set to C{True}. ''' return _clipped_(deg, limit, _degrees_) if limit and limit > 0 else deg def clipRadians(rad, limit): '''Clip a lat- or longitude to the given range. @arg rad: Unclipped lat- or longitude (C{radians}). @arg limit: Valid B{C{-limit..+limit}} range (C{radians}). @return: Clipped value (C{radians}). @raise RangeError: If B{C{abs(rad)}} beyond B{C{limit}} and L{pygeodesy.rangerrors} set to C{True}. ''' return _clipped_(rad, limit, _radians_) if limit and limit > 0 else rad def compassDMS(bearing, form=F_D, prec=None, sep=S_SEP): '''Convert bearing to a string suffixed with compass point. @arg bearing: Bearing from North (compass C{degrees360}). @kwarg form: Optional B{C{bearing}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Optional separator (C{str}). @return: Compass degrees and point in the specified form (C{str}). ''' return _toDMS(bearing % _360_0, form, prec, sep, 1, compassPoint(bearing)) def compassPoint(bearing, prec=3): '''Convert bearing to a compass point. @arg bearing: Bearing from North (compass C{degrees360}). @kwarg prec: Optional precision (1 for cardinal or basic winds, 2 for intercardinal or ordinal or principal winds, 3 for secondary-intercardinal or half-winds or 4 for quarter-winds). @return: Compass point (1-, 2-, 3- or 4-letter C{str}). @raise ValueError: Invalid B{C{prec}}. @see: U{Dms.compassPoint <https://GitHub.com/ChrisVeness/geodesy/blob/master/dms.js>} and U{Compass rose<https://WikiPedia.org/wiki/Compass_rose>}. @example: >>> p = compassPoint(24, 1) # 'N' >>> p = compassPoint(24, 2) # 'NE' >>> p = compassPoint(24, 3) # 'NNE' >>> p = compassPoint(24) # 'NNE' >>> p = compassPoint(11, 4) # 'NbE' >>> p = compassPoint(30, 4) # 'NEbN' >>> p = compassPoint(11.249) # 'N' >>> p = compassPoint(11.25) # 'NNE' >>> p = compassPoint(-11.25) # 'N' >>> p = compassPoint(348.749) # 'NNW' ''' try: # m = 2 << prec; x = 32 // m m, x = _MOD_X[prec] except KeyError: raise _ValueError(prec=prec) # not round(), i.e. half-even rounding in Python 3, # but round-away-from-zero as int(b + 0.5) iff b is # non-negative, otherwise int(b + copysign0(_0_5, b)) q = int((bearing % _360_0) * m / _360_0 + _0_5) % m return _WINDS[q * x] _MOD_X = {1: (4, 8), 2: (8, 4), 3: (16, 2), 4: (32, 1)} # [prec] _WINDS = (_N_, 'NbE', 'NNE', 'NEbN', _NE_, 'NEbE', 'ENE', 'EbN', _E_, 'EbS', 'ESE', 'SEbE', _SE_, 'SEbS', 'SSE', 'SbE', _S_, 'SbW', 'SSW', 'SWbS', _SW_, 'SWbW', 'WSW', 'WbS', _W_, 'WbN', 'WNW', 'NWbW', _NW_, 'NWbN', 'NNW', 'NbW') # cardinals def degDMS(deg, prec=6, s_D=S_DEG, s_M=S_MIN, s_S=S_SEC, neg=_MINUS_, pos=NN): '''Convert degrees to a string in degrees, minutes I{or} seconds. @arg deg: Value in degrees (C{scalar}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg s_D: Symbol for degrees (C{str}). @kwarg s_M: Symbol for minutes (C{str}) or C{""}. @kwarg s_S: Symbol for seconds (C{str}) or C{""}. @kwarg neg: Optional sign for negative (C{'-'}). @kwarg pos: Optional sign for positive (C{''}). @return: I{Either} degrees, minutes I{or} seconds (C{str}). ''' try: deg = float(deg) except (TypeError, ValueError) as x: raise _ValueError(deg=deg, txt=str(x)) d, s = abs(deg), s_D if d < 1: if s_M: d *= _60_0 if d < 1 and s_S: d *= _60_0 s = s_S else: s = s_M elif s_S: d *= 3600 s = s_S z = int(prec) t = Fmt.F(d, prec=abs(z)) if z > 1: t = fstrzs(t) n = neg if deg < 0 else pos return NN(n, t, s) def latDMS(deg, form=F_DMS, prec=2, sep=S_SEP): '''Convert latitude to a string, optionally suffixed with N or S. @arg deg: Latitude to be formatted (C{degrees}). @kwarg form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_D_}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_} L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Optional separator (C{str}). @return: Degrees in the specified form (C{str}). @JSname: I{toLat}. ''' return _toDMS(deg, form, prec, sep, 2, _S_ if deg < 0 else _N_) def latlonDMS(lls, form=F_DMS, prec=None, sep=None): '''Convert one or more C{LatLon} instances to strings. @arg lls: Single or a list, sequence, tuple, etc. (C{LatLon}s). @kwarg form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Separator joining B{C{lls}} (C{str} or C{None}). @return: A C{str} or C{tuple} of B{C{sep}} is C{None} or C{NN}. ''' if issequence(lls): t = tuple(ll.toStr(form=form, prec=prec) for ll in lls) if sep: t = sep.join(t) else: t = lls.toStr(form=form, prec=prec) return t def lonDMS(deg, form=F_DMS, prec=2, sep=S_SEP): '''Convert longitude to a string, optionally suffixed with E or W. @arg deg: Longitude to be formatted (C{degrees}). @kwarg form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Optional separator (C{str}). @return: Degrees in the specified form (C{str}). @JSname: I{toLon}. ''' return _toDMS(deg, form, prec, sep, 3, _W_ if deg < 0 else _E_) def normDMS(strDMS, norm=NN): '''Normalize all degree ˚, minute ' and second " symbols in a string to the default symbols %s, %s and %s. @arg strDMS: DMS (C{str}). @kwarg norm: Optional replacement symbol, default symbol otherwise (C{str}). @return: Normalized DMS (C{str}). ''' if norm: for s in _S_ALL: strDMS = strDMS.replace(s, norm) strDMS = strDMS.rstrip(norm) else: for s, S in _S_norm.items(): strDMS = strDMS.replace(s, S) return strDMS def parseDDDMMSS(strDDDMMSS, suffix=_NSEW_, sep=S_SEP, clip=0): '''Parse a lat- or longitude represention form [D]DDMMSS in degrees. @arg strDDDMMSS: Degrees in any of several forms (C{str}) and types (C{float}, C{int}, other). @kwarg suffix: Optional, valid compass points (C{str}, C{tuple}). @kwarg sep: Optional separator between "[D]DD", "MM" and "SS" (%r). @kwarg clip: Optionally, limit value to -clip..+clip (C{degrees}). @return: Degrees (C{float}). @raise ParseError: Invalid B{C{strDDDMMSS}} or B{C{clip}} or the B{C{strDDDMMSS}} form is incompatible with the suffixed or B{C{suffix}} compass point. @raise RangeError: Value of B{C{strDDDMMSS}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @note: Type C{str} values "[D]DD", "[D]DDMM" and "[D]DDMMSS" for B{C{strDDDMMSS}} are parsed properly only if I{either} unsigned and suffixed with a valid, compatible, C{cardinal} L{compassPoint} I{or} if unsigned or signed, unsuffixed and with keyword argument B{C{suffix}} set to B{%r}, B{%r} or a compatible L{compassPoint}. @note: Unlike function L{parseDMS}, type C{float}, C{int} and other non-C{str} B{C{strDDDMMSS}} values are interpreted form [D]DDMMSS. For example, C{int(1230)} is returned as 12.5 I{and not 1230.0} degrees. However, C{int(345)} is considered form "DDD" 345 I{and not "DDMM" 0345}, unless B{C{suffix}} specifies compass point B{%r}. @see: Functions L{parseDMS}, L{parseDMS2} and L{parse3llh}. ''' def _DDDMMSS_(strDDDMMSS, suffix, sep, clip): S = suffix.upper() if isstr(strDDDMMSS): t = strDDDMMSS.strip() if sep: t = t.replace(sep, NN).strip() s = t[:1] # sign or digit P = t[-1:] # compass point, digit or dot t = t.lstrip(_PLUSMINUS_).rstrip(S).strip() f = t.split(_DOT_) d = len(f[0]) f = NN.join(f) if 1 < d < 8 and f.isdigit() and ( (P in S and s.isdigit()) or (P.isdigit() and s in '-0123456789+' # PYCHOK indent and S in ((_NS_, _EW_) + _WINDS))): # check [D]DDMMSS form and compass point X = _EW_ if isodd(d) else _NS_ if not (P in X or (S in X and (P.isdigit() or P == _DOT_))): t = 'DDDMMSS'[0 if isodd(d) else 1:d | 1], X[:1], X[1:] raise ParseError('form %s applies %s-%s' % t) f = 0 # fraction else: # try other forms return _DMS2deg(strDDDMMSS, S, sep, clip) else: # float or int to [D]DDMMSS[.fff] f = float(strDDDMMSS) s = _MINUS_ if f < 0 else NN P = _0_ # anything except _SW_ f, i = modf(abs(f)) t = Fmt.f(i, prec=0) # str(i) == 'i.0' d = len(t) # bump number of digits to match # the given, valid compass point if S in (_NS_ if isodd(d) else _EW_): t = _0_ + t d += 1 # P = S # elif d > 1: # P = (_EW_ if isodd(d) else _NS_)[0] if d < 4: # [D]DD[.ddd] if f: t = float(t) + f t = t, 0, 0 else: f += float(t[d-2:]) if d < 6: # [D]DDMM[.mmm] t = t[:d-2], f, 0 else: # [D]DDMMSS[.sss] t = t[:d-4], t[d-4:d-2], f d = _dms2deg(s, P, *map2(float, t)) return clipDegrees(d, float(clip)) if clip else d return _parseX(_DDDMMSS_, strDDDMMSS, suffix, sep, clip, strDDDMMSS=strDDDMMSS, suffix=suffix) if __debug__: # no __doc__ at -O and -OO parseDDDMMSS.__doc__ %= (S_SEP, _NS_, _EW_, _NS_) def _dms2deg(s, P, deg, min, sec): '''(INTERNAL) Helper for C{parseDDDMMSS} and C{parseDMS}. ''' deg += (min + (sec / _60_0)) / _60_0 if s == _MINUS_ or P in _SW_: deg = neg(deg) return deg def _DMS2deg(strDMS, suffix, sep, clip): '''(INTERNAL) Helper for C{parseDDDMMSS} and C{parseDMS}. ''' try: d = float(strDMS) except (TypeError, ValueError): strDMS = strDMS.strip() t = strDMS.lstrip(_PLUSMINUS_).rstrip(suffix.upper()).strip() if sep: t = t.replace(sep, _SPACE_) for s in _S_ALL: t = t.replace(s, NN) else: for s in _S_ALL: t = t.replace(s, _SPACE_) t = map2(float, t.strip().split()) + (0, 0) d = _dms2deg(strDMS[:1], strDMS[-1:], *t[:3]) return clipDegrees(d, float(clip)) if clip else d def parseDMS(strDMS, suffix=_NSEW_, sep=S_SEP, clip=0): # MCCABE 14 '''Parse a lat- or longitude representation C{"lat, lon"} in C{degrees}. This is very flexible on formats, allowing signed decimal degrees, degrees and minutes or degrees minutes and seconds optionally suffixed by a cardinal compass point. A variety of symbols, separators and suffixes are accepted, for example "3°37′09″W". Minutes and seconds may be omitted. @arg strDMS: Degrees in any of several forms (C{str}) and types (C{float}, C{int}, other). @kwarg suffix: Optional, valid compass points (C{str}, C{tuple}). @kwarg sep: Optional separator between deg°, min′ and sec″ ("''"). @kwarg clip: Optionally, limit value to -clip..+clip (C{degrees}). @return: Degrees (C{float}). @raise ParseError: Invalid B{C{strDMS}} or B{C{clip}}. @raise RangeError: Value of B{C{strDMS}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @note: Inlike function L{parseDDDMMSS}, type C{float}, C{int} and other non-C{str} B{C{strDMS}} values are considered as decimal degrees. For example, C{int(1230)} is returned as 1230.0 I{and not as 12.5} degrees and C{float(345)} as 345.0 I{and not as 3.75} degrees! @see: Functions L{parseDDDMMSS}, L{parseDMS2} and L{parse3llh}. ''' return _parseX(_DMS2deg, strDMS, suffix, sep, clip, strDMS=strDMS, suffix=suffix) def parseDMS2(strLat, strLon, sep=S_SEP, clipLat=90, clipLon=180): '''Parse a lat- and a longitude representions in C{degrees}. @arg strLat: Latitude in any of several forms (C{str} or C{degrees}). @arg strLon: Longitude in any of several forms (C{str} or C{degrees}). @kwarg sep: Optional separator between deg°, min′ and sec″ (''). @kwarg clipLat: Keep latitude in B{C{-clipLat..+clipLat}} range (C{degrees}). @kwarg clipLon: Keep longitude in B{C{-clipLon..+clipLon}} range (C{degrees}). @return: A L{LatLon2Tuple}C{(lat, lon)} in C{degrees}. @raise ParseError: Invalid B{C{strLat}} or B{C{strLon}}. @raise RangeError: Value of B{C{strLat}} or B{C{strLon}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. @note: See the B{Notes} at function L{parseDMS}. @see: Functions L{parseDDDMMSS}, L{parseDMS} and L{parse3llh}. ''' from pygeodesy.namedTuples import LatLon2Tuple # avoid circluar import return LatLon2Tuple(parseDMS(strLat, suffix=_NS_, sep=sep, clip=clipLat), parseDMS(strLon, suffix=_EW_, sep=sep, clip=clipLon)) def parse3llh(strllh, height=0, sep=_COMMA_, clipLat=90, clipLon=180): '''Parse a string C{"lat lon [h]"} representing lat-, longitude in C{degrees} and optional height in C{meter}. The lat- and longitude value must be separated by a separator character. If height is present it must follow, separated by another separator. The lat- and longitude values may be swapped, provided at least one ends with the proper compass point. @arg strllh: Latitude, longitude[, height] (C{str}, ...). @kwarg height: Optional, default height (C{meter}) or C{None}. @kwarg sep: Optional separator (C{str}). @kwarg clipLat: Keep latitude in B{C{-clipLat..+clipLat}} (C{degrees}). @kwarg clipLon: Keep longitude in B{C{-clipLon..+clipLon}} range (C{degrees}). @return: A L{LatLon3Tuple}C{(lat, lon, height)} in C{degrees}, C{degrees} and C{float}. @raise RangeError: Lat- or longitude value of B{C{strllh}} outside valid range and L{pygeodesy.rangerrors} set to C{True}. @raise ValueError: Invalid B{C{strllh}} or B{C{height}}. @note: See the B{Notes} at function L{parseDMS}. @see: Functions L{parseDDDMMSS}, L{parseDMS} and L{parseDMS2}. @example: >>> parse3llh('000°00′05.31″W, 51° 28′ 40.12″ N') (51.4778°N, 000.0015°W, 0) ''' from pygeodesy.namedTuples import LatLon3Tuple # avoid circluar import def _3llh_(strllh, height, sep): ll = strllh.strip().split(sep) if len(ll) > 2: # XXX interpret height unit h = float(ll.pop(2).rstrip(_LETTERS).strip()) else: h = height # None from wgrs.Georef.__new__ if len(ll) != 2: raise ValueError a, b = [_.strip() for _ in ll] # PYCHOK false if a[-1:] in _EW_ or b[-1:] in _NS_: a, b = b, a return LatLon3Tuple(parseDMS(a, suffix=_NS_, clip=clipLat), parseDMS(b, suffix=_EW_, clip=clipLon), h) return _parseX(_3llh_, strllh, height, sep, strllh=strllh) def parseRad(strRad, suffix=_NSEW_, clip=0): '''Parse a string representing angle in C{radians}. @arg strRad: Degrees in any of several forms (C{str} or C{radians}). @kwarg suffix: Optional, valid compass points (C{str}, C{tuple}). @kwarg clip: Optionally, limit value to -clip..+clip (C{radians}). @return: Radians (C{float}). @raise ParseError: Invalid B{C{strRad}} or B{C{clip}}. @raise RangeError: Value of B{C{strRad}} outside the valid range and L{pygeodesy.rangerrors} set to C{True}. ''' def _Rad_(strRad, suffix, clip): try: r = float(strRad) except (TypeError, ValueError): strRad = strRad.strip() r = float(strRad.lstrip(_PLUSMINUS_).rstrip(suffix.upper()).strip()) if strRad[:1] == _MINUS_ or strRad[-1:] in _SW_: r = neg(r) return clipRadians(r, float(clip)) if clip else r return _parseX(_Rad_, strRad, suffix, clip, strRad=strRad, suffix=suffix) def precision(form, prec=None): '''Set the default precison for a given F_ form. @arg form: L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G} or L{F_RAD} (C{str}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @return: Previous precision (C{int}). @raise ValueError: Invalid B{C{form}} or B{C{prec}} or B{C{prec}} outside valid range. ''' try: p = _F_prec[form] except KeyError: raise _ValueError(form=form) if prec is not None: from pygeodesy.units import Precision_ _F_prec[form] = Precision_(prec=prec, low=-9, high=9) return p def toDMS(deg, form=F_DMS, prec=2, sep=S_SEP, ddd=2, neg=_MINUS_, pos=NN): '''Convert I{signed} C{degrees} to string, without suffix. @arg deg: Degrees to be formatted (C{degrees}). @kwarg form: Optional B{C{deg}} format (C{str} or L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F__E}, L{F__F}, L{F__G}, L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__}, L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F__E__}, L{F__F__}, L{F__G__} or L{F_RAD__}). @kwarg prec: Optional number of decimal digits (0..9 or C{None} for default). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}}. @kwarg sep: Optional separator (C{str}). @kwarg ddd: Optional number of digits for deg° (2 or 3). @kwarg neg: Optional sign for negative degrees ('-'). @kwarg pos: Optional sign for positive degrees (''). @return: Degrees in the specified form (C{str}). ''' t = _toDMS(deg, form, prec, sep, ddd, NN) if deg and form[:1] not in _PLUSMINUS_: t = NN((neg if deg < 0 else (pos if deg > 0 else NN)), t) return t # **) MIT License # # Copyright (C) 2016-2021 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.