# Coverage for pygeodesy/wgrs.py : 98%

## 187 statements 183 run 4 missing 7 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 | # -*- coding: utf-8 -*- u'''World Geographic Reference System (WGRS) en-/decoding. Classes L{Georef} and L{WGRSError} and several functions to encode, decode and inspect WGRS references. Transcoded from I{Charles Karney}'s C++ class U{Georef <https://GeographicLib.SourceForge.io/html/classGeographicLib_1_1Georef.html>}, but with modified C{precision} and extended with C{height} and C{radius}. See also U{World Geographic Reference System <https://WikiPedia.org/wiki/World_Geographic_Reference_System>}. ''' # from pygeodesy.basics import isstr # from .named from pygeodesy.dms import parse3llh # parseDMS2 from pygeodesy.errors import _ValueError, _xkwds from pygeodesy.interns import NN, _AtoZnoIO_, _float, _height_, \ _radius_, _SPACE_, _0to9_, _0_5, _0_001, \ _1_0, _2_0, _60_0, _90_EPS_2, _1000_0 from pygeodesy.lazily import _ALL_LAZY, _ALL_OTHER from pygeodesy.named import isstr, nameof, Property_RO from pygeodesy.namedTuples import LatLon2Tuple, LatLonPrec3Tuple # from pygeodesy.props import Property_RO # from .named from pygeodesy.streprs import Fmt, _0wd from pygeodesy.units import Height, Int, Lat, Lon, Precision_, \ Radius, Scalar_, Str, _xStrError from pygeodesy.utily import ft2m, m2ft, m2NM from math import floor __all__ = _ALL_LAZY.wgrs __version__ = '22.04.14' _Base = 10 _BaseLen = 4 _DegChar = _AtoZnoIO_.tillQ _Digits = _0to9_ _Height_ = Height.__name__ _INV_ = 'INV' _LatOrig = -90 _LatTile = _AtoZnoIO_.tillM _LonOrig = -180 _LonTile = _AtoZnoIO_ _M_ = 60000000000 # == 60_000_000_000 == 60 * pow(10, 9) _MaxPrec = 11 _Radius_ = Radius.__name__ _Tile = 15 # tile size in degrees _MaxLen = _BaseLen + 2 * _MaxPrec _MinLen = _BaseLen - 2 _LatOrig_M_ = _LatOrig * _M_ _LonOrig_M_ = _LonOrig * _M_ _float_Tile = _float(_Tile) _LatOrig_Tile = _float(_LatOrig) / _Tile _LonOrig_Tile = _float(_LonOrig) / _Tile def _2divmod3(x, Orig_M_): '''(INTERNAL) Convert B{C{x}} to 3_tuple C{(tile, modulo, fraction)}/ ''' i = int(floor(x * _M_)) i, x = divmod(i - Orig_M_, _M_) xt, xd = divmod(i, _Tile) return xt, xd, x def _2fllh(lat, lon, height=None): '''(INTERNAL) Convert lat, lon, height. ''' # lat, lon = parseDMS2(lat, lon) return (Lat(lat, Error=WGRSError), Lon(lon, Error=WGRSError), height) def _2geostr2(georef): '''(INTERNAL) Check a georef string. ''' try: n, geostr = len(georef), georef.upper() p, o = divmod(n, 2) if o or n < _MinLen or n > _MaxLen \ or geostr[:3] == _INV_ \ or not geostr.isalnum(): raise ValueError return geostr, _2Precision(p - 1) except (AttributeError, TypeError, ValueError) as x: raise WGRSError(Georef.__name__, georef, txt=str(x)) def _2Precision(precision): '''(INTERNAL) Return a L{Precision_} instance. ''' return Precision_(precision, Error=WGRSError, low=0, high=_MaxPrec) class WGRSError(_ValueError): '''World Geographic Reference System (WGRS) encode, decode or other L{Georef} issue. ''' pass class Georef(Str): '''Georef class, a named C{str}. ''' # no str.__init__ in Python 3 def __new__(cls, cll, precision=3, name=NN): '''New L{Georef} from an other L{Georef} instance or georef C{str} or from a C{LatLon} instance or lat-/longitude C{str}. @arg cll: Cell or location (L{Georef} or C{str}, C{LatLon} or C{str}). @kwarg precision: Optional, the desired georef resolution and length (C{int} 0..11), see function L{wgrs.encode} for more details. @kwarg name: Optional name (C{str}). @return: New L{Georef}. @raise RangeError: Invalid B{C{cll}} lat- or longitude. @raise TypeError: Invalid B{C{cll}}. @raise WGRSError: INValid or non-alphanumeric B{C{cll}}. ''' ll = p = None if isinstance(cll, Georef): g, p = _2geostr2(str(cll)) elif isstr(cll): if ',' in cll: lat, lon, h = _2fllh(*parse3llh(cll, height=None)) g = encode(lat, lon, precision=precision, height=h) # PYCHOK false ll = lat, lon # original lat, lon else: g = cll.upper() else: # assume LatLon try: lat, lon, h = _2fllh(cll.lat, cll.lon) except AttributeError: raise _xStrError(Georef, cll=cll) # Error=WGRSError h = getattr(cll, _height_, h) g = encode(lat, lon, precision=precision, height=h) # PYCHOK false ll = lat, lon # original lat, lon self = Str.__new__(cls, g, name=name or nameof(cll)) self._latlon = ll self._precision = p return self @Property_RO def decoded3(self): '''Get this georef's attributes (L{LatLonPrec3Tuple}). ''' lat, lon = self.latlon return LatLonPrec3Tuple(lat, lon, self.precision, name=self.name) @Property_RO def decoded5(self): '''Get this georef's attributes (L{LatLonPrec5Tuple}) with height and radius set to C{None} if missing. ''' return self.decoded3.to5Tuple(self.height, self.radius) @Property_RO def _decoded5(self): '''(INTERNAL) Initial L{LatLonPrec5Tuple}. ''' return decode5(self) @Property_RO def height(self): '''Get this georef's height in C{meter} or C{None} if missing. ''' return self._decoded5.height @Property_RO def latlon(self): '''Get this georef's (center) lat- and longitude (L{LatLon2Tuple}). ''' lat, lon = self._latlon or self._decoded5[:2] return LatLon2Tuple(lat, lon, name=self.name) @Property_RO def latlonheight(self): '''Get this georef's (center) lat-, longitude and height (L{LatLon3Tuple}), with height set to C{0} if missing. ''' return self.latlon.to3Tuple(self.height or 0) @Property_RO def precision(self): '''Get this georef's precision (C{int}). ''' p = self._precision return self._decoded5.precision if p is None else p @Property_RO def radius(self): '''Get this georef's radius in C{meter} or C{None} if missing. ''' return self._decoded5.radius def toLatLon(self, LatLon=None, height=None, **LatLon_kwds): '''Return (the center of) this georef cell as an instance of the supplied C{LatLon} class. @kwarg LatLon: Class to use (C{LatLon}) or C{None}. @kwarg height: Optional height (C{meter}). @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: This georef location (B{C{LatLon}}) or if B{C{LatLon}} is C{None}, a L{LatLon3Tuple}C{(lat, lon, height)}. @raise TypeError: Invalid B{C{LatLon}} or B{C{LatLon_kwds}}. ''' if LatLon is None: r = self.latlonheight if height is None else \ self.latlon.to3Tuple(height) else: h = (self.height or 0) if height is None else height r = LatLon(*self.latlon, height=h, **_xkwds(LatLon_kwds, name=self.name)) return r def decode3(georef, center=True): '''Decode a C{georef} to lat-, longitude and precision. @arg georef: To be decoded (L{Georef} or C{str}). @kwarg center: If C{True} the center, otherwise the south-west, lower-left corner (C{bool}). @return: A L{LatLonPrec3Tuple}C{(lat, lon, precision)}. @raise WGRSError: Invalid B{C{georef}}, INValid, non-alphanumeric or odd length B{C{georef}}. ''' def _digit(ll, g, i, m): d = _Digits.find(g[i]) if d < 0 or d >= m: raise _Error(i) return ll * m + d def _Error(i): return WGRSError(Fmt.SQUARE(georef=i), georef) def _index(chars, g, i): k = chars.find(g[i]) if k < 0: raise _Error(i) return k g, precision = _2geostr2(georef) lon = _index(_LonTile, g, 0) + _LonOrig_Tile lat = _index(_LatTile, g, 1) + _LatOrig_Tile u = _1_0 if precision > 0: lon = lon * _Tile + _index(_DegChar, g, 2) lat = lat * _Tile + _index(_DegChar, g, 3) m, p = 6, precision - 1 for i in range(_BaseLen, _BaseLen + p): lon = _digit(lon, g, i, m) lat = _digit(lat, g, i + p, m) u *= m m = _Base u *= _Tile if center: lon = lon * _2_0 + _1_0 lat = lat * _2_0 + _1_0 u *= _2_0 u = _Tile / u return LatLonPrec3Tuple(Lat(lat * u, Error=WGRSError), Lon(lon * u, Error=WGRSError), precision, name=nameof(georef)) def decode5(georef, center=True): '''Decode a C{georef} to lat-, longitude, precision, height and radius. @arg georef: To be decoded (L{Georef} or C{str}). @kwarg center: If C{True} the center, otherwise the south-west, lower-left corner (C{bool}). @return: A L{LatLonPrec5Tuple}C{(lat, lon, precision, height, radius)} where C{height} and/or C{radius} are C{None} if missing. @raise WGRSError: Invalid B{C{georef}}, INValid, non-alphanumeric or odd length B{C{georef}}. ''' def _h2m(kft, name): return Height(ft2m(kft * _1000_0), name=name, Error=WGRSError) def _r2m(NM, name): return Radius(NM / m2NM(1), name=name, Error=WGRSError) def _split2(g, name, _2m): i = max(g.find(name[0]), g.rfind(name[0])) if i > _BaseLen: return g[:i], _2m(int(g[i+1:]), _SPACE_(georef, name)) else: return g, None g = Str(georef, Error=WGRSError) g, h = _split2(g, _Height_, _h2m) # H is last g, r = _split2(g, _Radius_, _r2m) # R before H return decode3(g, center=center).to5Tuple(h, r) def encode(lat, lon, precision=3, height=None, radius=None): # MCCABE 14 '''Encode a lat-/longitude as a C{georef} of the given precision. @arg lat: Latitude (C{degrees}). @arg lon: Longitude (C{degrees}). @kwarg precision: Optional, the desired C{georef} resolution and length (C{int} 0..11). @kwarg height: Optional, height in C{meter}, see U{Designation of area <https://WikiPedia.org/wiki/World_Geographic_Reference_System>}. @kwarg radius: Optional, radius in C{meter}, see U{Designation of area <https://WikiPedia.org/wiki/World_Geographic_Reference_System>}. @return: The C{georef} (C{str}). @raise RangeError: Invalid B{C{lat}} or B{C{lon}}. @raise WGRSError: Invalid B{C{precision}}, B{C{height}} or B{C{radius}}. @note: The B{C{precision}} value differs from U{Georef<https:// GeographicLib.SourceForge.io/html/classGeographicLib_1_1Georef.html>}. The C{georef} length is M{2 * (precision + 1)} and the C{georef} resolution is I{15°} for B{C{precision}} 0, I{1°} for 1, I{1′} for 2, I{0.1′} for 3, I{0.01′} for 4, ... M{10**(2 - precision)}. ''' def _option(name, m, m2_, K): f = Scalar_(m, name=name, Error=WGRSError) return NN(name[0].upper(), int(m2_(f * K) + _0_5)) p = _2Precision(precision) lat, lon, _ = _2fllh(lat, lon) lat = _90_EPS_2(lat) xt, xd, x = _2divmod3(lon, _LonOrig_M_) yt, yd, y = _2divmod3(lat, _LatOrig_M_) g = _LonTile[xt], _LatTile[yt] if p > 0: g += _DegChar[xd], _DegChar[yd] p -= 1 if p > 0: d = pow(_Base, _MaxPrec - p) x = _0wd(p, x // d) y = _0wd(p, y // d) g += x, y if radius is not None: # R before H g += _option(_radius_, radius, m2NM, _1_0), if height is not None: # H is last g += _option(_height_, height, m2ft, _0_001), return NN.join(g) # XXX Georef(''.join(g)) def precision(res): '''Determine the L{Georef} precision to meet a required (geographic) resolution. @arg res: The required resolution (C{degrees}). @return: The L{Georef} precision (C{int} 0..11). @raise ValueError: Invalid B{C{res}}. @see: Function L{wgrs.encode} for more C{precision} details. ''' r = Scalar_(res=res) for p in range(_MaxPrec): if resolution(p) <= r: return p return _MaxPrec def resolution(prec): '''Determine the (geographic) resolution of a given L{Georef} precision. @arg prec: The given precision (C{int}). @return: The (geographic) resolution (C{degrees}). @raise ValueError: Invalid B{C{prec}}. @see: Function L{wgrs.encode} for more C{precision} details. ''' p = Int(prec=prec, Error=WGRSError) if p > 1: r = _1_0 / (_60_0 * pow(_Base, min(p, _MaxPrec) - 1)) elif p < 1: r = _float_Tile else: r = _1_0 return r __all__ += _ALL_OTHER(decode3, decode5, # functions encode, precision, resolution) # **) MIT License # # Copyright (C) 2016-2022 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.