[frames] | no frames]

[ Module Hierarchy | Class Hierarchy ]

# Class Hierarchy

- object: The most base type
  - exceptions.BaseException: Common base class for all exceptions
    - exceptions.Exception: Common base class for all non-exit exceptions.
      - exceptions.StandardError: Base class for all standard Python exceptions that do not represent interpreter exiting.
        - exceptions.ValueError: Inappropriate argument value (of correct type).
          - pygeodesy.vector3d.CrossError: Error raised for zero or near-zero vectorial cross products, occurring for coincident or colinear points, paths or bearings.
          - pygeodesy.utily.LimitError: Error raised for lat- and/or longitudinal deltas exceeding the limit in functions equirectangular and equirectangular_.
          - pygeodesy.dms.RangeError: Error raised for lat- or longitude values outside the clip, clipLat, clipLon or limit range in function clipDMS, parse3llh, parseDMS or parseDMS2.
          - pygeodesy.utm.UTMError: UTM parse or other error.
          - pygeodesy.ellipsoidalVincenty.VincentyError: Error raised from Vincenty's direct and inverse methods for coincident points or lack of convergence.
  - _abcoll.Container
    - _abcoll.Sequence: All the operations on a read-only sequence.
      - pygeodesy.points._Basequence: (INTERNAL) Base class.
        - pygeodesy.points.LatLon2psxy: Wrapper for `LatLon` points as "on-the-fly" pseudo-xy coordinates.
        - pygeodesy.points._Array2LatLon: Base class for Numpy2LatLon or Tuple2LatLon.
          - pygeodesy.points.Numpy2LatLon: Wrapper for `NumPy` arrays as "on-the-fly" `LatLon` points.
          - pygeodesy.points.Tuple2LatLon: Wrapper for tuple sequences as "on-the-fly" `LatLon` points.
  - pygeodesy.fmath.Fsum: Precision floating point summation similar to standard Python function `math.fsum`.
  - _abcoll.Iterable
    - _abcoll.Sequence: All the operations on a read-only sequence.
      - pygeodesy.points._Basequence: (INTERNAL) Base class.
        - pygeodesy.points.LatLon2psxy: Wrapper for `LatLon` points as "on-the-fly" pseudo-xy coordinates.
        - pygeodesy.points._Array2LatLon: Base class for Numpy2LatLon or Tuple2LatLon.
          - pygeodesy.points.Numpy2LatLon: Wrapper for `NumPy` arrays as "on-the-fly" `LatLon` points.
          - pygeodesy.points.Tuple2LatLon: Wrapper for tuple sequences as "on-the-fly" `LatLon` points.
  - pygeodesy.points.LatLon_: Low-overhead `LatLon` class for Numpy2LatLon or Tuple2LatLon'
  - pygeodesy.bases.Named: (INTERNAL) Base class for object with a name.
    - pygeodesy.bases.Based: (INTERNAL) Base class with name.
      - pygeodesy.bases.LatLonHeightBase: (INTERNAL) Base class for `LatLon` points on spherical or ellipsiodal earth models.
        - pygeodesy.ellipsoidalBase.LatLonEllipsoidalBase: (INTERNAL) Base class for ellipsoidal `LatLon`.
          - pygeodesy.ellipsoidalKarney.LatLon: An ellipsoidal LatLon similar to ellipsoidalVincenty.LatLon but using Charles F. F. Karney's Python GeographicLib to compute the geodesic distance, initial and final bearing (azimuths) between two given points or the destination point given a start point and an initial bearing.
          - pygeodesy.ellipsoidalNvector.LatLon: An n-vector-based ellipsoidal LatLon point.
          - pygeodesy.ellipsoidalVincenty.LatLon: Using the formulae devised by Thaddeus Vincenty (1975) with an ellipsoidal model of the earth to compute the geodesic distance and bearings between two given points or the destination point given an start point and initial bearing.
        - pygeodesy.nvector.LatLonNvectorBase: (INTERNAL) Base class for n-vector-based ellipsoidal and spherical `LatLon` classes.
          - pygeodesy.ellipsoidalNvector.LatLon: An n-vector-based ellipsoidal LatLon point.
          - pygeodesy.sphericalNvector.LatLon: New n-vector based point on spherical earth model.
        - pygeodesy.sphericalBase.LatLonSphericalBase: (INTERNAL) Base class for spherical `LatLon`.
          - pygeodesy.sphericalNvector.LatLon: New n-vector based point on spherical earth model.
          - pygeodesy.sphericalTrigonometry.LatLon: New point on spherical model earth model.
      - pygeodesy.lcc.Lcc: Lambert conformal conic East-/Northing location.
      - pygeodesy.mgrs.Mgrs: Military Grid Reference System (MGRS/NATO) references, with method to convert to UTM coordinates.
      - pygeodesy.osgr.Osgr: Ordinance Survey Grid References (OSGR) coordinate.
      - pygeodesy.utm.Utm: Universal Transverse Mercator (UTM) coordinate.
      - pygeodesy.bases.VectorBased: (INTERNAL) Base class for Vector3d.
        - pygeodesy.vector3d.Vector3d: Generic 3-D vector manipulation.
          - pygeodesy.ellipsoidalBase.CartesianBase: (INTERNAL) Base class for ellipsoidal Cartesian.
            - pygeodesy.ellipsoidalKarney.Cartesian: Extended to convert (geocentric) Cartesian points to Karney-based (ellipsoidal) geodetic LatLon.
            - pygeodesy.ellipsoidalNvector.Cartesian: Extended to convert (geocentric) Cartesian points to (ellipsoidal) Nvector and n-vector-based geodetic LatLon.
            - pygeodesy.ellipsoidalVincenty.Cartesian: Extended to convert (geocentric) Cartesian points to Vincenty-based (ellipsoidal) geodetic LatLon.
          - pygeodesy.nvector.Nvector: Base class for ellipsoidal and spherical Nvector.
            - pygeodesy.ellipsoidalNvector.Nvector: An n-vector is a position representation using a (unit) vector normal to the earth ellipsoid.
            - pygeodesy.sphericalNvector.Nvector: An n-vector is a position representation using a (unit) vector normal to the earth's surface.
      - pygeodesy.webmercator.Wm: Web Mercator (WM) coordinate.
      - pygeodesy.datum._Based: (INTERNAL) Base class.
        - pygeodesy.lcc.Conic: Lambert conformal conic projection (1- or 2-SP).
        - pygeodesy.datum.Datum: Ellipsoid and transform parameters for an earth model.
        - pygeodesy.datum.Ellipsoid: Ellipsoid with semi-major, semi-minor axis, inverse flattening and several other pre-computed, frequently used values.
        - pygeodesy.datum.Transform: Helmert transformation.
    - pygeodesy.geohash.Geohash: Geohash class, sub-class of str.
    - pygeodesy.ellipsoidalNvector.Ned: North-Eeast-Down (NED), also known as Local Tangent Plane (LTP), is a vector in the local coordinate frame of a body.
  - _abcoll.Sized
    - _abcoll.Sequence: All the operations on a read-only sequence.
      - pygeodesy.points._Basequence: (INTERNAL) Base class.
        - pygeodesy.points.LatLon2psxy: Wrapper for `LatLon` points as "on-the-fly" pseudo-xy coordinates.
        - pygeodesy.points._Array2LatLon: Base class for Numpy2LatLon or Tuple2LatLon.
          - pygeodesy.points.Numpy2LatLon: Wrapper for `NumPy` arrays as "on-the-fly" `LatLon` points.
          - pygeodesy.points.Tuple2LatLon: Wrapper for tuple sequences as "on-the-fly" `LatLon` points.
  - pygeodesy.points._Basequence: (INTERNAL) Base class.
    - pygeodesy.points.LatLon2psxy: Wrapper for `LatLon` points as "on-the-fly" pseudo-xy coordinates.
    - pygeodesy.points._Array2LatLon: Base class for Numpy2LatLon or Tuple2LatLon.
      - pygeodesy.points.Numpy2LatLon: Wrapper for `NumPy` arrays as "on-the-fly" `LatLon` points.
      - pygeodesy.points.Tuple2LatLon: Wrapper for tuple sequences as "on-the-fly" `LatLon` points.
  - basestring: Type basestring cannot be instantiated; it is the base for str and unicode.
    - str: str(object='') -> string
      - pygeodesy.geohash.Geohash: Geohash class, sub-class of str.
  - type: type(object) -> the object's type type(name, bases, dict) -> a new type
    - abc.ABCMeta: Metaclass for defining Abstract Base Classes (ABCs).