1

2# -*- coding: utf-8 -*-

3

4 u'''European Petroleum Survey Group (EPSG) en-/decoding.

5

6 Classes L{Epsg} and L{EPSGError} and functions to L{encode} and L{decode2}

7(U{EPSG<https://EPSG.org>}) codes from and to U{UTM

8<https://WikiPedia.org/wiki/Universal_Transverse_Mercator_coordinate_system>} and

9 U{UPS<https://WikiPedia.org/wiki/Universal_polar_stereographic_coordinate_system>}

10 zones.

11

12 A pure Python implementation transcoded from I{Charles Karney}'s C++ class U{UTMUPS

13<https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1UTMUPS.html>},

14 including coverage of UPS as zone C{0}.

15'''

16

17 from pygeodesy.basics import isint, isstr, _xinstanceof

18 from pygeodesy.errors import _ValueError

19 from pygeodesy.interns import NN, _N_, _NS_, _S_, _SPACE_

20 from pygeodesy.lazily import _ALL_DOCS, _ALL_LAZY

21 from pygeodesy.namedTuples import UtmUps2Tuple

22 from pygeodesy.props import Property_RO

23 from pygeodesy.streprs import Fmt

24 from pygeodesy.units import Int

25 from pygeodesy.ups import Ups

26 from pygeodesy.utm import Utm

27 from pygeodesy.utmupsBase import _to3zBhp, _UPS_ZONE, _UTM_ZONE_MIN, \

28 _UTM_ZONE_MAX, _UTMUPS_ZONE_INVALID

29

30__all__ = _ALL_LAZY.epsg

31__version__ = '24.08.05'

32

33# _EPSG_INVALID = _UTMUPS_ZONE_INVALID

34_EPSG_N_01 = 32601 # EPSG code for UTM zone 01 N

35_EPSG_N_60 = 32660 # EPSG code for UTM zone 60 N

36_EPSG_N = 32661 # EPSG code for UPS pole N

37

38_EPSG_S_01 = 32701 # EPSG code for UTM zone 01 S

39_EPSG_S_60 = 32760 # EPSG code for UTM zone 60 S

40_EPSG_S = 32761 # EPSG code for UPS pole S

41

42

43 class Epsg(Int):

44 '''U{EPSG<https://EPSG.org>} class, a named C{int}.

45 '''

46 _band = NN

47 _epsg = None

48 _hemisphere = NN

49 _utmups = None

50 _zone = _UTMUPS_ZONE_INVALID

51

52 def __new__(cls, eisu, **name):

53 '''New L{Epsg} (I{European Petroleum Survey Group}) code from a

54 UTM/USP coordinate or other EPSG code.

55

56 @arg eisu: Other code (L{Epsg}, C{int}, C{str}, L{Utm} or L{Ups}).

57 @kwarg name: Optional C{B{name}=NN} (C{str}).

58

59 @return: New L{Epsg}.

60

61 @raise TypeError: Invalid B{C{eisu}}.

62

63 @raise EPSGError: Invalid B{C{eisu}}.

64 '''

65 if isinstance(eisu, Epsg):

66 self = int.__new__(cls, int(eisu))

67 self._band = eisu.band

68 self._epsg = self # XXX eisu

69 self._hemisphere = eisu.hemisphere

70 self._utmups = eisu.utmups

71 self._zone = eisu.zone

72 if eisu.name:

73 self.name = eisu.name

74

75 elif isint(eisu):

76 self = int.__new__(cls, eisu)

77 self._epsg = eisu

78 self._zone, self._hemisphere = decode2(eisu) # PYCHOK UtmUps2Tuple

79

80 elif isstr(eisu):

81 self = encode(eisu)

82

83 else:

84 u = eisu

85 _xinstanceof(Utm, Ups, eisu=u)

86 self = encode(u.zone, hemipole=u.hemisphere, band=u.band) # PYCHOK **kwds

87 self._utmups = u

88 if u.name:

89 self.name = u.name

90

91 if name:

92 self.rename(name)

93 return self

94

95 def __repr__(self):

96 return Fmt.PAREN(self.named, int.__repr__(self))

97

98 def __str__(self):

99 return int.__str__(self)

100

101 @Property_RO

102 def band(self):

103 '''Get the I{latitudinal} UTM or I{polar} UPS Band

104 (C{'A'|'B'|'C'|'D'|..|'W'|'X'|'Y'|'Z'} or C{""}).

105 '''

106 return self._band

107

108 @Property_RO

109 def hemisphere(self):

110 '''Get the UTM/UPS hemisphere/-pole (C{'N'|'S'}).

111 '''

112 return self._hemisphere

113

114 @Property_RO

115 def utmups(self):

116 '''Get the UTM/UPS original (L{Utm}, L{Ups}).

117 '''

118 return self._utmups

119

120 def utmupsStr(self, B=False):

121 '''Get the UTM/UPS zone, band and hemisphere/-pole (C{str}).

122 '''

123 b = self.band if B else NN

124 h = s = self.hemisphere

125 if h:

126 s = _SPACE_

127 return NN(Fmt.zone(self.zone), b, s, h)

128

129 @Property_RO

130 def zone(self):

131 '''Get the (longitudinal) UTM/UPS zone (C{int}, C{1..60} for UTM, C{0} for UPS).

132 '''

133 return self._zone

134

135

136 class EPSGError(_ValueError):

137 '''EPSG encode, decode or other L{Epsg} issue.

138 '''

139 pass

140

141

142 def decode2(epsg):

143 '''Determine the UTM/USP zone and hemisphere from a given

144 U{EPSG<https://EPSG.org>}.

145

146 @arg epsg: The EPSG (L{Epsg}, C{str} or C{scalar}).

147

148 @return: A L{UtmUps2Tuple}C{(zone, hemipole)}.

149

150 @raise EPSGError: Invalid B{C{epsg}}.

151

152 @note: Coverage of UPS as zone C{0} follows I{Karney}'s function U{UTMUPS::DecodeEPSG

153 <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1UTMUPS.html>}.

154 '''

155 if isinstance(epsg, Epsg):

156 z, h = epsg.zone, epsg.hemisphere

157

158 else:

159 try:

160 e = int(epsg) # int(long) OK

161 if _EPSG_N_01 <= e <= _EPSG_N_60:

162 z, h = int(e - _EPSG_N_01 + _UTM_ZONE_MIN), _N_

163

164 elif _EPSG_S_01 <= e <= _EPSG_S_60:

165 z, h = int(e - _EPSG_S_01 + _UTM_ZONE_MIN), _S_

166

167 elif e == _EPSG_N:

168 z, h = _UPS_ZONE, _N_

169

170 elif e == _EPSG_S:

171 z, h = _UPS_ZONE, _S_

172

173 else:

174 raise ValueError(NN)

175 except (TypeError, ValueError) as x:

176 raise EPSGError(epsg=epsg, cause=x)

177

178 return UtmUps2Tuple(z, h)

179

180

181 def encode(zone, hemipole=NN, band=NN):

182 '''Determine the U{EPSG<https://EPSG.org>} code for

183 a given UTM/UPS zone number, hemisphere/pole and/or Band.

184

185 @arg zone: The (longitudinal) UTM zone (C{int}, 1..60) or UPS

186 zone (C{int}, 0) or UTM zone with/-out I{latitudinal}

187 Band letter (C{str}, '01C'..'60X') or UPS zone

188 with/-out I{polar} Band letter (C{str}, '00A', '00B',

189 '00Y' or '00Z').

190 @kwarg hemipole: UTM/UPS hemisphere or UPS projection top/center

191 pole (C{str}, C{'N[orth]'} or C{'S[outh]'}).

192 @kwarg band: Optional I{latitudinal} UTM or I{polar} UPS Band

193 letter (C{str}).

194

195 @return: C{EPSG} code (L{Epsg}).

196

197 @raise EPSGError: Invalid B{C{zone}}, B{C{hemipole}} or B{C{band}}.

198

199 @note: Coverage of UPS as zone C{0} follows I{Karney}'s function U{UTMUPS::EncodeEPSG

200 <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1UTMUPS.html>}.

201 '''

202 try:

203 z, B, hp = _to3zBhp(zone, band, hemipole=hemipole) # in .utmupsBase

204 if hp not in _NS_:

205 raise ValueError

206 except (TypeError, ValueError) as x:

207 raise EPSGError(zone=zone, hemipole=hemipole, band=band, cause=x)

208

209 if _UTM_ZONE_MIN <= z <= _UTM_ZONE_MAX:

210 e = z - _UTM_ZONE_MIN + (_EPSG_N_01 if hp == _N_ else _EPSG_S_01)

211 elif z == _UPS_ZONE:

212 e = _EPSG_N if hp == _N_ else _EPSG_S

213 else:

214 raise EPSGError(zone=zone)

215

216 e = Epsg(e)

217 e._band = B

218 # e._hemisphere = hp

219 return e

220

221

222__all__ += _ALL_DOCS(decode2, encode)

223

224# **) MIT License

225#

226# Copyright (C) 2016-2024 -- mrJean1 at Gmail -- All Rights Reserved.

227#

228# Permission is hereby granted, free of charge, to any person obtaining a

229# copy of this software and associated documentation files (the "Software"),

230# to deal in the Software without restriction, including without limitation

231# the rights to use, copy, modify, merge, publish, distribute, sublicense,

232# and/or sell copies of the Software, and to permit persons to whom the

233# Software is furnished to do so, subject to the following conditions:

234#

235# The above copyright notice and this permission notice shall be included

236# in all copies or substantial portions of the Software.

237#

238# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

239# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

240# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

241# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

242# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

243# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

244# OTHER DEALINGS IN THE SOFTWARE.