1

2# -*- coding: utf-8 -*-

3

4 u'''Parsers and formatters of angles in degrees, minutes and seconds or radians.

5

6 Functions to parse and format bearing, compass, lat- and longitudes in various forms of

7 degrees, minutes and seconds with or without degrees, minute and second symbols plus a

8 compass point suffix, including parsing of C{decimal} and C{sexagecimal} degrees.

9

10 Set env variable C{PYGEODESY_FMT_FORM} to any C{F_...} form to override default C{F_DMS}

11 formatting of lat- and longitudes or to an empty string to restore the default.

12

13 After I{(C) Chris Veness 2011-2024} published under the same MIT Licence**, see

14 U{Latitude/Longitude<https://www.Movable-Type.co.UK/scripts/latlong.html>} and

15 U{Vector-based geodesy<https://www.Movable-Type.co.UK/scripts/latlong-vectors.html>}.

16

17@var F_D: Format degrees as unsigned "deg°" with symbol, plus compass point suffix C{N, S, E} or C{W} (C{str}).

18@var F_DM: Format degrees as unsigned "deg°min′" with symbols, plus suffix (C{str}).

19@var F_DMS: Format degrees as unsigned "deg°min′sec″" with symbols, plus suffix (C{str}).

20@var F_DEG: Format degrees as unsigned "[D]DD" I{without} symbol, plus suffix (C{str}).

21@var F_MIN: Format degrees as unsigned "[D]DDMM" I{without} symbols, plus suffix (C{str}).

22@var F_SEC: Format degrees as unsigned "[D]DDMMSS" I{without} symbols, plus suffix (C{str}).

23@var F_D60: Format degrees as unsigned "[D]DD.MMSS" C{sexagecimal} I{without} symbols, plus suffix (C{str}).

24@var F__E: Format degrees as unsigned "%E" I{without} symbols, plus suffix (C{str}).

25@var F__F: Format degrees as unsigned "%F" I{without} symbols, plus suffix (C{str}).

26@var F__G: Format degrees as unsigned "%G" I{without} symbols, plus suffix (C{str}).

27@var F_RAD: Convert degrees to radians and format as unsigned "RR" with symbol, plus suffix (C{str}).

28

29@var F_D_: Format degrees as signed "-/deg°" with symbol, I{without} suffix (C{str}).

30@var F_DM_: Format degrees as signed "-/deg°min′" with symbols, I{without} suffix (C{str}).

31@var F_DMS_: Format degrees as signed "-/deg°min′sec″" with symbols, I{without} suffix (C{str}).

32@var F_DEG_: Format degrees as signed "-/[D]DD" I{without} symbol, I{without} suffix (C{str}).

33@var F_MIN_: Format degrees as signed "-/[D]DDMM" I{without} symbols, I{without} suffix (C{str}).

34@var F_SEC_: Format degrees as signed "-/[D]DDMMSS" I{without} symbols, I{without} suffix (C{str}).

35@var F_D60_: Format degrees as signed "-/[D]DD.MMSS" C{sexagecimal} I{without} symbols, I{without} suffix (C{str}).

36@var F__E_: Format degrees as signed "-/%E" I{without} symbols, I{without} suffix (C{str}).

37@var F__F_: Format degrees as signed "-/%F" I{without} symbols, I{without} suffix (C{str}).

38@var F__G_: Format degrees as signed "-/%G" I{without} symbols, I{without} suffix (C{str}).

39@var F_RAD_: Convert degrees to radians and format as signed "-/RR" I{without} symbol, I{without} suffix (C{str}).

40

41@var F_D__: Format degrees as signed "-/+deg°" with symbol, I{without} suffix (C{str}).

42@var F_DM__: Format degrees as signed "-/+deg°min′" with symbols, I{without} suffix (C{str}).

43@var F_DMS__: Format degrees as signed "-/+deg°min′sec″" with symbols, I{without} suffix (C{str}).

44@var F_DEG__: Format degrees as signed "-/+[D]DD" I{without} symbol, I{without} suffix (C{str}).

45@var F_MIN__: Format degrees as signed "-/+[D]DDMM" I{without} symbols, without suffix (C{str}).

46@var F_SEC__: Format degrees as signed "-/+[D]DDMMSS" I{without} symbols, I{without} suffix (C{str}).

47@var F_D60__: Format degrees as signed "-/+[D]DD.MMSS" C{sexagecimal} I{without} symbols, I{without} suffix (C{str}).

48@var F__E__: Format degrees as signed "-/+%E" I{without} symbols, I{without} suffix (C{str}).

49@var F__F__: Format degrees as signed "-/+%F" I{without} symbols, I{without} suffix (C{str}).

50@var F__G__: Format degrees as signed "-/+%G" I{without} symbols, I{without} suffix (C{str}).

51@var F_RAD__: Convert degrees to radians and format as signed "-/+RR" I{without} symbol, I{without} suffix (C{str}).

52

53@var S_DEG: Degrees symbol, default C{"°"}

54@var S_MIN: Minutes symbol, default C{"′"} aka I{PRIME}

55@var S_SEC: Seconds symbol, default C{"″"} aka I{DOUBLE_PRIME}

56@var S_RAD: Radians symbol, default C{""} aka L{pygeodesy.NN}

57@var S_DMS: If C{True} include, otherwise cancel all DMS symbols, default C{True}.

58@var S_SEP: Separator between C{deg°|min′|sec″|suffix}, default C{""} aka L{pygeodesy.NN}

59

60@note: In Python 2-, L{S_DEG}, L{S_MIN}, L{S_SEC}, L{S_RAD} and L{S_SEP} may be multi-byte,

61 non-ascii characters and if so, I{not} C{unicode}.

62'''

63

64 from pygeodesy.basics import copysign0, isLatLon, isodd, issequence, isstr, \

65 neg as _neg # in .ups

66 from pygeodesy.constants import _umod_360, _0_0, _0_5, _60_0, _360_0, _3600_0

67 from pygeodesy.errors import ParseError, RangeError, _TypeError, _ValueError, \

68 _parseX, rangerrors, _xError, _xkwds, _getPYGEODESY

69# from pygeodesy.internals import _getPYGEODESY # from .errors

70 from pygeodesy.interns import NN, _COMMA_, _d_, _DASH_, _deg_, _degrees_, _DOT_, \

71 _0_, _e_, _E_, _EW_, _f_, _F_, _g_, _MINUS_, _N_, \

72 _NE_, _NS_, _NSEW_, _NW_, _PERCENTDOTSTAR_, _PLUS_, \

73 _PLUSMINUS_, _QUOTE1_, _QUOTE2_, _radians_, _S_, \

74 _SE_, _SPACE_, _SW_, _W_

75 from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS

76# from pygeodesy.namedTuples import LatLon2Tuple # _MODS

77# from pygeodesy.props import _throwarning # _MODS

78 from pygeodesy.streprs import Fmt, fstr, fstrzs, _0wpF

79# from pygeodesy.units import Precision_ # _MODS

80# from pygeodesy.utily import _Wrap # _MODS

81

82 from math import fabs, modf, radians

83 try:

84 from string import letters as _LETTERS

85 except ImportError: # Python 3+

86 from string import ascii_letters as _LETTERS

87

88__all__ = _ALL_LAZY.dms

89__version__ = '24.10.18'

90

91_beyond_ = 'beyond'

92_deg_min_ = 'deg+min'

93_sexagecimal_ = 'sexagecimal'

94_SEXAGECIMUL = 1.e4 # sexagecimal C{D.MMSSss} into decimal C{DMMSS.ss}

95

96 F_D, F_DM, F_DMS, F_DEG, F_MIN, F_SEC, F_D60, F__E, F__F, F__G, F_RAD = _F_s = (

97 _d_, 'dm', 'dms', _deg_, 'min', 'sec', 'd60', _e_, _f_, _g_, 'rad')

98 F_D_, F_DM_, F_DMS_, F_DEG_, F_MIN_, F_SEC_, F_D60_, F__E_, F__F_, F__G_, F_RAD_ = (NN(

99 _MINUS_, _) for _ in _F_s)

100 F_D__, F_DM__, F_DMS__, F_DEG__, F_MIN__, F_SEC__, F_D60__, F__E__, F__F__, F__G__, F_RAD__ = (NN(

101 _PLUS_, _) for _ in _F_s)

102 del _F_s

103_F_DMS = _getPYGEODESY('FMT_FORM') or F_DMS

104

105_F_case = {F_D: F_D, F_DEG: F_D, _degrees_: F_D, # unsigned _F_s

106 F_DM: F_DM, F_MIN: F_DM, _deg_min_: F_DM,

107 F_D60: F_D60, F_RAD: F_RAD, _radians_: F_RAD,

108 F__E: F__E, F__F: F__F, F__G: F__G} # default F_DMS

109_F_prec = {F_D: 6, F_DM: 4, F_DMS: 2, # default precs

110 F_DEG: 6, F_MIN: 4, F_SEC: 2, F_D60: 0,

111 F__E: 8, F__F: 8, F__G: 8, F_RAD: 5}

112_F_symb = set((F_D, F_DM, F_DMS, _deg_min_)) # == {} pychok -Tb

113

114 S_DEG = _DEGREES_ = '°' # ord() = 176

115 S_MIN = _MINUTES_ = '′' # PRIME

116 S_SEC = _SECONDS_ = '″' # DOUBLE_PRIME

117 S_RAD = _RADIANS_ = NN # PYCHOK radians symbol ""

118 S_DMS = True # include DMS symbols

119 S_SEP = NN # separator between deg|min|sec|suffix ""

120 S_NUL = NN # empty string, kept INTERNAL

121

122# note: ord(_DEGREES_) == ord('°') == 176, ord('˚') == 730

123_S_norm = {S_DEG: _DEGREES_, '˚': _DEGREES_, '^': _DEGREES_, # _d_: _DEGREES_,

124 S_MIN: _MINUTES_, '’': _MINUTES_, _QUOTE1_: _MINUTES_, # _r_: _RADIANS_

125 S_SEC: _SECONDS_, '”': _SECONDS_, _QUOTE2_: _SECONDS_}

126

127_WINDS = (_N_, 'NbE', 'NNE', 'NEbN', _NE_, 'NEbE', 'ENE', 'EbN',

128 _E_, 'EbS', 'ESE', 'SEbE', _SE_, 'SEbS', 'SSE', 'SbE',

129 _S_, 'SbW', 'SSW', 'SWbS', _SW_, 'SWbW', 'WSW', 'WbS',

130 _W_, 'WbN', 'WNW', 'NWbW', _NW_, 'NWbN', 'NNW', 'NbW')

131

132

133 def _D603(sep, s_D=_DOT_, s_M=None, s_S=S_NUL, s_DMS=S_DMS, **unused):

134 '''(INTERNAL) Get the overridden or default pseudo-C{DMS} symbols.

135 '''

136 if s_DMS:

137 M = sep if s_M is None else s_M

138 return s_D, (M or S_NUL), s_S

139 else: # no overriden symbols

140 return _DOT_, sep, S_NUL

141

142

143 def _DMS3(form, s_D=S_DEG, s_M=S_MIN, s_S=S_SEC, s_DMS=S_DMS, **unused):

144 '''(INTERNAL) Get the overridden or default C{DMS} symbols.

145 '''

146 return (s_D, s_M, s_S) if s_DMS and form in _F_symb else (S_NUL, S_NUL, S_NUL)

147

148

149 def _dms3(d, ddd, p, w):

150 '''(INTERNAL) Format C{d} as (deg, min, sec) C{str}s with leading zeros.

151 '''

152 d = round(d * _3600_0, p)

153 d, s = divmod(d, _3600_0)

154 m, s = divmod(s, _60_0)

155 return (_0wpF(ddd, 0, d),

156 _0wpF( 2, 0, m),

157 _0wpF(w+2, p, s))

158

159

160 def _DR2(s_D=S_NUL, s_R=S_RAD, **unused):

161 '''(INTERNAL) Get the overridden or default C{D} and C{RAD} symbols.

162 '''

163 return s_D, s_R

164

165

166 def _fstrzs(t, **unused):

167 '''(INTERNAL) Pass-thru version of C{.streprs.fstrzs}.

168 '''

169 return t

170

171

172 def _split3(strDMS, suffix=_NSEW_):

173 '''(INTERNAL) Return sign, stripped B{C{strDMS}} and compass point.

174 '''

175 t = strDMS.strip()

176 s = t[:1] # sign or digit

177 P = t[-1:] # compass point or digit or dot

178 t = t.lstrip(_PLUSMINUS_).rstrip(suffix)

179 return s, t.strip(), P

180

181

182 def _toDMS(deg, form, prec, sep, ddd, P, s_D_M_S): # MCCABE 15 in .units

183 '''(INTERNAL) Convert C{deg} to C{str}, with/-out sign, DMS symbols and/or suffix.

184 '''

185 try:

186 F = None

187 deg = float(deg)

188

189 f, s = form, form[:1]

190 if s in _PLUSMINUS_: # signed

191 n = _MINUS_ if deg < 0 else (

192 _PLUS_ if deg > 0 and s == _PLUS_ else NN)

193 P = NN # no suffix

194 f = f.lstrip(_PLUSMINUS_)

195 else: # suffixed

196 n = NN

197 if sep and P: # no sep if no suffix

198 P = NN(sep, P)

199 try:

200 F = _F_case[f] # .strip()

201 except KeyError:

202 f = f.lower() # .strip()

203 F = _F_case.get(f, F_DMS)

204

205 if prec is None:

206 z = p = _F_prec.get(F, 6)

207 else:

208 z = int(prec)

209 p = abs(z)

210 w = p + (1 if p else 0)

211 z = fstrzs if z > 1 else _fstrzs

212 d = fabs(deg)

213

214 if F is F_DMS: # 'deg+min+sec', default

215 D, M, S = _DMS3(f, **s_D_M_S)

216 d, m, s = _dms3(d, ddd, p, w)

217 t = NN(n, d, D, sep,

218 m, M, sep,

219 z(s), S, P)

220

221 elif F is F_DM: # 'deg+min'

222 D, M, _ = _DMS3(f, **s_D_M_S)

223 d, m = divmod(round(d * _60_0, p), _60_0)

224 t = NN(n, _0wpF(ddd, 0, d), D, sep,

225 z(_0wpF(w+2, p, m)), M, P)

226

227 elif F is F_D: # 'deg'

228 D, _, _ = _DMS3(f, **s_D_M_S)

229 t = NN(n, z(_0wpF(w+ddd, p, d)), D, P)

230

231 elif F is F_D60: # 'deg.MM|SSss|'

232 D, M, S = _D603(sep, **s_D_M_S)

233 d, m, s = _dms3(d, ddd, p, w)

234 t = z(s).split(_DOT_) + [S, P]

235 t = NN(n, d, D, m, M, *t)

236

237 elif F is F_RAD:

238 _, R = _DR2(**s_D_M_S)

239 r = NN(_PERCENTDOTSTAR_, _F_) % (p, radians(d))

240 t = NN(n, z(r), R, P)

241

242 else: # F in (F__E, F__F, F__G)

243 D, _ = _DR2(**s_D_M_S)

244 d = NN(_PERCENTDOTSTAR_, F) % (p, d) # XXX f?

245 t = NN(n, z(d, ap1z=F is F__G), D, P)

246

247 except Exception as x:

248 d = {} if F is None else dict(F_=F, P=P)

249 raise _xError(x, deg=deg, form=form, prec=prec, **d)

250

251 return t # NOT unicode in Python 2-

252

253

254 def bearingDMS(bearing, form=F_D, prec=None, sep=S_SEP, **s_D_M_S):

255 '''Convert bearing to a string (without compass point suffix).

256

257 @arg bearing: Bearing from North (compass C{degrees360}).

258 @kwarg form: Format specifier for B{C{deg}} (C{str} or C{F_...}).

259 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

260 @kwarg sep: Separator between degrees, minutes, seconds, suffix (C{str}).

261 @kwarg s_D_M_S: Optional keyword arguments to override any or cancel all

262 DMS symbol suffixes, see function L{pygeodesy.toDMS}.

263

264 @return: Compass degrees per the specified B{C{form}} (C{str}).

265

266 @see: Function L{pygeodesy.toDMS} and its B{Notes} for further details.

267 '''

268 return _toDMS(_umod_360(bearing), form, prec, sep, 1, NN, s_D_M_S)

269

270

271 def _clip(angle, limit, units):

272 '''(INTERNAL) Helper for C{clipDegrees} and C{clipRadians}.

273 '''

274 c = min(limit, max(-limit, angle))

275 if c != angle and rangerrors():

276 t = _SPACE_(fstr(angle, prec=6, ints=True), _beyond_,

277 copysign0(limit, angle), units)

278 raise RangeError(t, txt=None)

279 return c

280

281

282 def clipDegrees(deg, limit):

283 '''Clip a lat- or longitude to the given range.

284

285 @arg deg: Unclipped lat- or longitude (C{scalar degrees}).

286 @arg limit: Valid C{-/+B{limit}} range (C{degrees}).

287

288 @return: Clipped value (C{degrees}).

289

290 @raise RangeError: If B{C{deg}} outside the valid C{-/+B{limit}} range

291 and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

292 '''

293 return _clip(deg, limit, _degrees_) if limit and limit > 0 else deg

294

295

296 def clipRadians(rad, limit):

297 '''Clip a lat- or longitude to the given range.

298

299 @arg rad: Unclipped lat- or longitude (C{radians}).

300 @arg limit: Valid C{-/+B{limit}} range (C{radians}).

301

302 @return: Clipped value (C{radians}).

303

304 @raise RangeError: If B{C{rad}} outside the valid C{-/+B{limit}} range

305 and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

306 '''

307 return _clip(rad, limit, _radians_) if limit and limit > 0 else rad

308

309

310 def compassDMS(bearing, form=F_D, prec=None, sep=S_SEP, **s_D_M_S):

311 '''Convert bearing to a string suffixed with compass point.

312

313 @arg bearing: Bearing from North (compass C{degrees360}).

314 @kwarg form: Format specifier for B{C{deg}} (C{str} or C{F_...}).

315 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

316 @kwarg sep: Separator between degrees, minutes, seconds, suffix (C{str}).

317 @kwarg s_D_M_S: Optional keyword arguments to override any or cancel all

318 DMS symbol suffixes, see function L{pygeodesy.toDMS}.

319

320 @return: Compass degrees and point in the specified form (C{str}).

321

322 @see: Function L{pygeodesy.toDMS} and its B{Notes} for further details.

323 '''

324 b = _umod_360(bearing)

325 return _toDMS(b, form, prec, sep, 1, compassPoint(b), s_D_M_S)

326

327

328 def compassPoint(bearing, prec=3):

329 '''Convert a C{bearing} from North to a compass point.

330

331 @arg bearing: Bearing (compass C{degrees360}).

332 @kwarg prec: Precision, number of compass point characters:

333 1 for cardinal or basic winds,

334 2 for intercardinal or ordinal or principal winds,

335 3 for secondary-intercardinal or half-winds or

336 4 for quarter-winds).

337

338 @return: Compass point (1-, 2-, 3- or 4-letter C{str}).

339

340 @raise ValueError: Invalid B{C{bearing}} or B{C{prec}}.

341

342 @see: U{Dms.compassPoint

343 <https://GitHub.com/ChrisVeness/geodesy/blob/master/dms.js>}

344 and U{Compass rose<https://WikiPedia.org/wiki/Compass_rose>}.

345 '''

346 try: # like .streprs.enstr2

347 b = _umod_360(bearing)

348 p = _MODS.units.Precision_(prec, low=1, high=4) \

349 if prec != 3 else int(prec)

350 m = 2 << p

351 w = 32 // m # if m in (4, 8, 16, 32)

352 # not round(b), half-even rounding in Python 3+, but

353 # round-away-from-zero as int(b + copysign0(_0_5, b))

354 w *= int(b * m / _360_0 + _0_5) % m

355 return _WINDS[w]

356 except Exception as x:

357 raise _xError(x, bearing=bearing, prec=prec)

358

359

360 def degDMS(deg, prec=6, s_D=S_DEG, s_M=S_MIN, s_S=S_SEC, neg=_MINUS_, pos=NN):

361 '''Convert degrees to a string in degrees, minutes I{or} seconds.

362

363 @arg deg: Value in degrees (C{scalar degrees}).

364 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

365 Trailing zero decimals are stripped for C{B{prec}=1}

366 and above, but kept for negative B{C{prec}}.

367 @kwarg s_D: D symbol for degrees (C{str}).

368 @kwarg s_M: M symbol for minutes (C{str}) or C{""} aka L{pygeodesy.NN}.

369 @kwarg s_S: S symbol for seconds (C{str}) or C{""} aka L{pygeodesy.NN}.

370 @kwarg neg: Optional sign for negative (C{'-'}).

371 @kwarg pos: Optional sign for positive (C{""}) aka L{pygeodesy.NN}.

372

373 @return: I{Either} degrees, minutes I{or} seconds (C{str}).

374

375 @see: Function L{pygeodesy.toDMS}.

376 '''

377 try:

378 deg = float(deg)

379 except Exception as x:

380 raise _xError(x, deg=deg, prec=prec)

381

382 d, s = fabs(deg), s_D

383 if d < 1:

384 if s_M:

385 d *= _60_0

386 if d < 1 and s_S:

387 d *= _60_0

388 s = s_S

389 else:

390 s = s_M

391 elif s_S:

392 d *= _3600_0

393 s = s_S

394

395 z = int(prec)

396 t = Fmt.F(d, prec=abs(z))

397 if z > 1:

398 t = fstrzs(t)

399 n = neg if deg < 0 else pos

400 return NN(n, t, s) # NOT unicode in Python 2-

401

402

403 def latDMS(deg, form=_F_DMS, prec=None, sep=S_SEP, **s_D_M_S):

404 '''Convert latitude to a string, optionally suffixed with N or S.

405

406 @arg deg: Latitude to be formatted (C{scalar degrees}).

407 @kwarg form: Format specifier for B{C{deg}} (C{str} or C{F_...}).

408 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

409 @kwarg sep: Separator between degrees, minutes, seconds, suffix (C{str}).

410 @kwarg s_D_M_S: Optional keyword arguments to override any or cancel all

411 DMS symbol suffixes, see function L{pygeodesy.toDMS}.

412

413 @return: Degrees in the specified form (C{str}).

414

415 @see: Function L{pygeodesy.toDMS} and its B{Notes} for further details.

416 '''

417 P = _S_ if deg < 0 else _N_

418 return _toDMS(deg, form, prec, sep, 2, P, s_D_M_S)

419

420

421 def latlonDMS(lls, **m_form_prec_sep_s_D_M_S):

422 '''Convert one or more C{LatLon} instances to strings.

423

424 @arg lls: Single (C{LatLon}) or an iterable (C{LatLon}s).

425 @kwarg m_form_prec_sep_s_D_M_S: Optional keyword arguments C{B{m}eter},

426 C{B{form}at}, C{B{prec}ision}, B{C{s_D}}, B{C{s_M}}, B{C{s_S}},

427 B{C{s_DMS}} and I{DEPRECATED} C{B{sep}=None}, see function

428 L{pygeodesy.toDMS} and method C{LatLon.toStr} for more details.

429

430 @return: A C{tuple} of C{str}s if B{C{lls}} is a list, sequence, tuple, etc.

431 of C{LatLon}s or a single C{str} if B{C{lls}} is a single C{LatLon}.

432

433 @see: Functions L{pygeodesy.latlonDMS_}, L{pygeodesy.latDMS}, L{pygeodesy.lonDMS}

434 and L{pygeodesy.toDMS} and method C{LatLon.toStr}.

435

436 @note: Keyword argument C{B{sep}=None} to join the resturned C{tuple} has

437 been I{DEPRECATED}, use C{B{sep}.join(B{latlonDMS_}(...))} instead.

438 '''

439 sep, kwds = _latlonDMS_sep2(latlonDMS, **m_form_prec_sep_s_D_M_S)

440 if isLatLon(lls):

441 t = lls.toStr(**kwds)

442 elif issequence(lls):

443 t = tuple(ll.toStr(**kwds) for ll in lls)

444 if sep: # XXX DEPRECATED, to be removed

445 t = sep.join(t)

446 else:

447 raise _TypeError(lls=lls, **m_form_prec_sep_s_D_M_S)

448 return t

449

450

451 def latlonDMS_(*lls, **m_form_prec_sep_s_D_M_S):

452 '''Convert one or more C{LatLon} instances to strings.

453

454 @arg lls: The instances (C{LatLon}s), all positional arguments.

455 @kwarg m_form_prec_sep_s_D_M_S: Optional keyword arguments C{B{m}eter},

456 C{B{form}at}, C{B{prec}ision}, B{C{s_D}}, B{C{s_M}}, B{C{s_S}},

457 B{C{s_DMS}} and I{DEPRECATED} C{B{sep}=None}, see function

458 L{pygeodesy.toDMS} and method C{LatLon.toStr} for more details.

459

460 @return: A C{tuple} of C{str}s if 2 or more C{LatLon} instances

461 or a single C{str} if only a single C{LatLon} instance

462 is given in B{C{lls}}.

463

464 @see: Functions L{pygeodesy.latlonDMS}, L{pygeodesy.latDMS} and

465 L{pygeodesy.lonDMS} and L{pygeodesy.toDMS} and method

466 C{LatLon.toStr}.

467

468 @note: Keyword argument C{B{sep}=None} to join the resturned C{tuple} has

469 been I{DEPRECATED}, use C{B{sep}.join(B{latlonDMS_}(...))} instead.

470 '''

471 sep, kwds = _latlonDMS_sep2(latlonDMS, **m_form_prec_sep_s_D_M_S)

472 if not lls:

473 raise _ValueError(lls=lls, **m_form_prec_sep_s_D_M_S)

474 elif len(lls) < 2:

475 lls, sep = lls[0], None

476 t = latlonDMS(lls, **kwds)

477 return sep.join(t) if sep else t

478

479

480 def _latlonDMS_sep2(where, sep=None, **kwds):

481 '''DEPRECATED, use %r.join(%s(...)) instead.'''

482 if sep: # PYCHOK no cover

483 i = _MODS.inters

484 k = Fmt.EQUAL(sep=repr(sep))

485 k = _SPACE_(i._keyword_, i._arg_, k, i._of_)

486 n = where.__name__

487 t = _latlonDMS_sep2.__doc__ % (sep, n)

488 _MODS.props._throwarning(k, n, t)

489 return sep, kwds

490

491

492 def lonDMS(deg, form=_F_DMS, prec=None, sep=S_SEP, **s_D_M_S):

493 '''Convert longitude to a string, optionally suffixed with E or W.

494

495 @arg deg: Longitude to be formatted (C{scalar degrees}).

496 @kwarg form: Format specifier for B{C{deg}} (C{str} or C{F_...}).

497 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

498 @kwarg sep: Separator between degrees, minutes, seconds, suffix (C{str}).

499 @kwarg s_D_M_S: Optional keyword arguments to override any or cancel all

500 DMS symbol suffixes.

501

502 @return: Degrees in the specified form (C{str}).

503

504 @see: Function L{pygeodesy.toDMS} and its B{Notes} for further details.

505 '''

506 P = _W_ if deg < 0 else _E_

507 return _toDMS(deg, form, prec, sep, 3, P, s_D_M_S)

508

509

510 def normDMS(strDMS, norm=None, **s_D_M_S):

511 '''Normalize all degrees, minutes and seconds (DMS) I{symbol} suffixes in

512 a string to the default symbols L{S_DEG}, L{S_MIN}, L{S_SEC}.

513

514 @arg strDMS: Original DMS string (C{str}).

515 @kwarg norm: Optional replacement symbol (C{str}) or C{None} for the default

516 DMS symbol). Use C{B{norm}=""} to remove all DMS symbols.

517 @kwarg s_D_M_S: Optional, alternate DMS symbol suffixes C{B{s_D}=}L{S_DEG},

518 C{B{s_M}=}L{S_MIN}, C{B{s_S}=}L{S_SEC} and C{B{s_R}=}L{S_RAD}

519 for radians, each to be replaced by B{C{norm}}.

520

521 @return: Normalized DMS (C{str}).

522 '''

523 def _s2S2(s_D=S_DEG, s_M=S_MIN, s_S=S_SEC, s_R=S_RAD):

524 d = {s_D: S_DEG, s_M: S_MIN, s_S: S_SEC, s_R: S_RAD}

525 for s, S in _xkwds(d, **_S_norm).items():

526 if s:

527 yield s, S

528

529 # XXX strDMS isn't unicode in Python 2- and looping

530 # thru strDMS will yield each byte, hence the loop

531 # thru _s2S2 and replacing the DMS symbols in strDMS

532

533 if norm is None: # back to default DMS

534 for s, S in _s2S2(**s_D_M_S):

535 if s != S:

536 strDMS = strDMS.replace(s, S)

537

538 else: # replace or remove all DMS

539 n = norm or NN

540 for s, _ in _s2S2(**s_D_M_S):

541 if s != n:

542 strDMS = strDMS.replace(s, n)

543 if n:

544 strDMS = strDMS.rstrip(n) # XXX not .strip?

545

546 return strDMS # NOT unicode in Python 2-

547

548

549 def parseDDDMMSS(strDDDMMSS, suffix=_NSEW_, sep=S_SEP, clip=0, sexagecimal=False):

550 '''Parse a lat- or longitude represention forms as [D]DDMMSS in degrees.

551

552 @arg strDDDMMSS: Degrees in any of several forms (C{str}) and types (C{float},

553 C{int}, other).

554 @kwarg suffix: Optional compass points (C{str}), valid in B{C{strDDDMMSS}}.

555 @kwarg sep: Optional separator between "[D]DD", "MM", "SS", B{C{suffix}}

556 (L{S_SEP}) in B{C{strDDDMMSS}}.

557 @kwarg clip: Optionally, limit value to range C{-/+B{clip}} (C{degrees}).

558 @kwarg sexagecimal: If C{True}, convert C{"D.MMSS"} or C{float(D.MMSS)} to

559 C{base-60} "MM" and "SS" digits. See C{form}s L{F_D60},

560 L{F_D60_} and L{F_D60__}.

561

562 @return: Degrees (C{float}).

563

564 @raise ParseError: Invalid B{C{strDDDMMSS}} or B{C{clip}} or the form of

565 B{C{strDDDMMSS}} is incompatible with or invalid for the

566 given B{C{suffix}} compass point(s).

567

568 @raise RangeError: Value of B{C{strDDDMMSS}} outside the valid C{-/+B{clip}}

569 range and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

570

571 @note: Type C{str} values "[D]DD", "[D]DDMM", "[D]DDMMSS" and "[D]DD.MMSS"

572 for B{C{strDDDMMSS}} are parsed properly only if I{either} unsigned

573 and suffixed with a valid, compatible, C{cardinal} L{compassPoint}

574 I{or} signed I{or} unsigned, unsuffixed and with keyword argument

575 B{C{suffix}="NS"}, B{C{suffix}="EW"} or a compatible L{compassPoint}.

576

577 @note: Unlike function L{parseDMS}, type C{float}, C{int} and other non-C{str}

578 B{C{strDDDMMSS}} values are interpreted as C{form} [D]DDMMSS or

579 [D]DD.MMSS. For example, C{int(1230)} is returned as 12.5 and I{not

580 1230.0} degrees. However, C{int(345)} is considered C{form} "DDD"

581 345 I{and not "DDMM" 0345}, unless B{C{suffix}} specifies the compass

582 point. Also, C{float(15.0523)} is returned as 15.0523 decimal

583 degrees and I{not 15°5′23″ sexagecimal}. To consider the latter, use

584 C{float(15.0523)} or C{"15.0523"} and specify the keyword argument

585 C{B{sexagecimal}=True}.

586

587 @see: Functions L{pygeodesy.parseDMS}, L{pygeodesy.parseDMS2} and

588 L{pygeodesy.parse3llh}.

589 '''

590 def _DDDMMSS(strDDDMMSS, suffix, sep, clip, sexagecimal):

591 S = suffix.upper() or _N_ # bool('' in _NE_) is True

592 if isstr(strDDDMMSS):

593 t = strDDDMMSS.replace(sep, NN) if sep else strDDDMMSS

594 n, s, t, f, P, X = _DDDMMSS6(t, S)

595 if X:

596 pass

597 elif not sexagecimal: # try other forms

598 return _DMS2deg(strDDDMMSS, S, sep, clip, {})

599

600 if sexagecimal: # move decimal dot from ...

601 n += 4 # ... [D]DD.MMSSs to [D]DDMMSS.s

602 if n < 6:

603 t = _SPACE_(_sexagecimal_, 'digits')

604 raise ParseError(t, n)

605 z = n - len(f) # zeros to append

606 t = (f + (_0_ * z)) if z > 0 else _DOT_(f[:n], f[n:])

607 f = _0_0 # fraction

608 else: # float or int to [D]DDMMSS[.fff]

609 f = float(strDDDMMSS)

610 n, s, t, f, P = _DDDMMSS5(f, S, sexagecimal)

611

612 if n < 4: # [D]DD[.ddd]

613 if t:

614 f += float(t)

615 t = f,

616 else:

617 n -= 2

618 f += float(t[n:])

619 if n < 4: # [D]DDMM[.mmm]

620 t = float(t[:n]), f

621 else: # [D]DDMMSS[.sss]

622 d = n - 2

623 t = float(t[:d]), float(t[d:n]), f

624 d = _dms2deg(s, P, *t)

625 return clipDegrees(d, float(clip)) if clip else d

626

627 return _parseX(_DDDMMSS, strDDDMMSS, suffix, sep, clip, sexagecimal,

628 strDDDMMSS=strDDDMMSS, suffix=suffix, sexagecimal=sexagecimal)

629

630

631 def _DDDMMSS5(f, S, sexagecimal):

632 '''(INTERNAL) Partial C{parseDDDMMSS} of C{float}.

633 '''

634 if sexagecimal:

635 f *= _SEXAGECIMUL

636 m = 6

637 else:

638 m = 0

639 s = P = _PLUS_ # anything except NN, _S_, _SW_, _W_

640 if f < 0:

641 f = -f

642 s = _MINUS_

643 f, i = modf(f) # returns ...

644 t = str(int(i)) # ... float(i)

645 n = len(t) # number of digits to ...

646 if n < m: # ... required min or ...

647 t = (_0_ * (m - n)) + t

648 # ... match the given compass point

649 elif S in (_NS_ if isodd(n) else _EW_):

650 t = _0_ + t

651 # P = S

652 # elif n > 1:

653 # P = (_EW_ if isodd(n) else _NS_)[0]

654 return len(t), s, t, f, P # float(f) fraction

655

656

657 def _DDDMMSS6(t, S):

658 '''(INTERNAL) Partial C{parseDDDMMSS} of C{str}.

659 '''

660 s, t, P = _split3(t, S)

661 f = t.split(_DOT_)

662 if len(f) > 2:

663 raise ParseError('dots', len(f) - 1)

664 n = len(f[0])

665 f = NN.join(f)

666 if 1 < n < 8 and f.isdigit() and ( # dddN/S/E/W or ddd or +/-ddd

667 (P in S and s.isdigit()) or

668 (P.isdigit() and S in _WINDS # PYCHOK indent

669 and (s in _PLUSMINUS_ or s.isdigit()))):

670 # check [D]DDMMSS form and compass point

671 X = _EW_ if isodd(n) else _NS_

672 if not (P in X or (S in X and (P.isdigit() or P == _DOT_))):

673 t = parseDDDMMSS.__name__[5 if isodd(n) else 6:]

674 t = _SPACE_('form', t, 'applies', _DASH_.join(X))

675 raise ParseError(t)

676 else:

677 X = NN

678 return n, s, t, f, P, X # str(f) fraction

679

680

681 def _DMS2deg(strDMS, suffix, sep, clip, s_D_M_S):

682 '''(INTERNAL) Helper for C{parseDDDMMSS} and C{parseDMS}.

683 '''

684 try:

685 d = float(strDMS)

686 except (TypeError, ValueError):

687 s, t, P = _split3(strDMS, suffix.upper())

688 if sep: # remove all DMS symbols

689 t = t.replace(sep, _SPACE_)

690 t = normDMS(t, norm=NN, **s_D_M_S)

691 else: # replace all DMS symbols

692 t = normDMS(t, norm=_SPACE_, **s_D_M_S)

693 t = t.strip().split()

694 d = _dms2deg(s, P, *map(float, t))

695 return clipDegrees(d, float(clip)) if clip else d

696

697

698 def _dms2deg(n, P, d, m=_0_0, s=_0_0):

699 '''(INTERNAL) Helper for C{parseDDDMMSS}, C{parseRad} and C{_DMS2deg}.

700 '''

701 m += s / _60_0

702 d += m / _60_0

703 if n == _MINUS_ or (P and P in _SW_):

704 d = _neg(d)

705 return d

706

707

708 def parseDMS(strDMS, suffix=_NSEW_, sep=S_SEP, clip=0, **s_D_M_S): # MCCABE 14

709 '''Parse a lat- or longitude representation in C{degrees}.

710

711 This is very flexible on formats, allowing signed decimal degrees, degrees

712 and minutes or degrees minutes and seconds optionally suffixed by a cardinal

713 compass point.

714

715 A variety of symbols, separators and suffixes are accepted, for example

716 "3°37′09″W". Minutes and seconds may be omitted.

717

718 @arg strDMS: Degrees in any of several forms (C{str}) and types (C{float},

719 C{int}, other).

720 @kwarg suffix: Optional, valid compass points (C{str}, C{tuple}).

721 @kwarg sep: Optional separator between C{deg°}, C{min′}, C{sec″},

722 B{C{suffix}} (C{''}).

723 @kwarg clip: Optionally, limit value to range C{-/+B{clip}} (C{degrees}).

724 @kwarg s_D_M_S: Optional, alternate DMS symbol suffixes for degrees

725 C{B{s_D}=}L{S_DEG}, minutes C{B{s_M}=}L{S_MIN} and

726 seconds C{B{s_S}=}L{S_SEC}, see function L{pygeodesy.toDMS}.

727

728 @return: Degrees (C{float}).

729

730 @raise ParseError: Invalid B{C{strDMS}} or B{C{clip}}.

731

732 @raise RangeError: Value of B{C{strDMS}} outside the valid C{-/+B{clip}} range

733 and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

734

735 @note: Unlike function L{parseDDDMMSS}, type C{float}, C{int} and other non-C{str}

736 B{C{strDMS}} values are considered decimal (and not sexagecimal) degrees.

737 For example, C{int(1230)} is returned as 1230.0 I{and not as 12.5} degrees

738 and C{float(345)} as 345.0 I{and not as 3.75} degrees!

739

740 @see: Functions L{pygeodesy.parseDDDMMSS}, L{pygeodesy.parseDMS2},

741 L{pygeodesy.parse3llh} and L{pygeodesy.toDMS}.

742 '''

743 return _parseX(_DMS2deg, strDMS, suffix, sep, clip, s_D_M_S, strDMS=strDMS, suffix=suffix)

744

745

746 def parseDMS2(strLat, strLon, sep=S_SEP, clipLat=90, clipLon=180, wrap=False, **s_D_M_S):

747 '''Parse a lat- and a longitude representions C{"lat, lon"} in C{degrees}.

748

749 @arg strLat: Latitude in any of several forms (C{str} or C{degrees}).

750 @arg strLon: Longitude in any of several forms (C{str} or C{degrees}).

751 @kwarg sep: Optional separator between deg°, min′, sec″, suffix (C{''}).

752 @kwarg clipLat: Limit latitude to range C{-/+B{clipLat}} (C{degrees}).

753 @kwarg clipLon: Limit longitude to range C{-/+B{clipLon}} (C{degrees}).

754 @kwarg wrap: If C{True}, wrap or I{normalize} the lat- and longitude,

755 overriding B{C{clipLat}} and B{C{clipLon}} (C{bool}).

756 @kwarg s_D_M_S: Optional, alternate DMS symbol suffixes for degrees

757 C{B{s_D}=}L{S_DEG}, minutes C{B{s_M}=}L{S_MIN} and

758 seconds C{B{s_S}=}L{S_SEC}, see function L{pygeodesy.toDMS}.

759

760 @return: A L{LatLon2Tuple}C{(lat, lon)} in C{degrees}.

761

762 @raise ParseError: Invalid B{C{strLat}} or B{C{strLon}}.

763

764 @raise RangeError: Value of B{C{strLat}} or B{C{strLon}} outside the

765 valid C{-/+B{clipLat}} or C{-/+B{clipLon}} range

766 and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

767

768 @note: See the B{Notes} at function L{parseDMS}.

769

770 @see: Functions L{pygeodesy.parseDDDMMSS}, L{pygeodesy.parseDMS},

771 L{pygeodesy.parse3llh} and L{pygeodesy.toDMS}.

772 '''

773 return _2Tuple(strLat, strLon, clipLat, clipLon, wrap, sep=sep, **s_D_M_S)

774

775

776 def _2Tuple(strLat, strLon, clipLat, clipLon, wrap, **kwds):

777 '''(INTERNAL) Helper for C{parseDMS2} and C{parse3llh}.

778 '''

779 if wrap:

780 _W = _MODS.utily._Wrap

781 ll = _W.latlon(parseDMS(strLat, suffix=_NS_, **kwds),

782 parseDMS(strLon, suffix=_EW_, **kwds))

783 else:

784 # if wrap is None:

785 # clipLat = clipLon = 0

786 ll = (parseDMS(strLat, suffix=_NS_, clip=clipLat, **kwds),

787 parseDMS(strLon, suffix=_EW_, clip=clipLon, **kwds))

788 return _MODS.namedTuples.LatLon2Tuple(*ll)

789

790

791 def parse3llh(strllh, height=0, sep=_COMMA_, clipLat=90, clipLon=180, wrap=False, **s_D_M_S):

792 '''Parse a string C{"lat, lon [, h]"} representing lat-, longitude in

793 C{degrees} and optional height in C{meter}.

794

795 The lat- and longitude value must be separated by a separator

796 character. If height is present it must follow, separated by

797 another separator.

798

799 The lat- and longitude values may be swapped, provided at least

800 one ends with the proper compass point.

801

802 @arg strllh: Latitude, longitude[, height] (C{str}, ...).

803 @kwarg height: Optional, default height (C{meter}) or C{None}.

804 @kwarg sep: Optional separator between C{"lat lon [h] suffix"} (C{str}).

805 @kwarg clipLat: Limit latitude to range C{-/+B{clipLat}} (C{degrees}).

806 @kwarg clipLon: Limit longitude to range C{-/+B{clipLon}} (C{degrees}).

807 @kwarg wrap: If C{True}, wrap or I{normalize} the lat- and longitude,

808 overriding B{C{clipLat}} and B{C{clipLon}} (C{bool}).

809 @kwarg s_D_M_S: Optional, alternate DMS symbol suffixes for degrees

810 C{B{s_D}=}L{S_DEG}, minutes C{B{s_M}=}L{S_MIN} and

811 seconds C{B{s_S}=}L{S_SEC}, see function L{pygeodesy.toDMS}.

812

813 @return: A L{LatLon3Tuple}C{(lat, lon, height)} in C{degrees},

814 C{degrees} and C{float}.

815

816 @raise RangeError: Lat- or longitude value of B{C{strllh}} outside the

817 valid C{-/+B{clipLat}} or C{-/+B{clipLon}} range

818 and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

819

820 @raise ValueError: Invalid B{C{strllh}} or B{C{height}}.

821

822 @note: See the B{Notes} at function L{parseDMS}.

823

824 @see: Functions L{pygeodesy.parseDDDMMSS}, L{pygeodesy.parseDMS},

825 L{pygeodesy.parseDMS2} and L{pygeodesy.toDMS}.

826 '''

827 def _3llh(strllh, height, sep, wrap):

828 ll = strllh.strip().split(sep)

829 if len(ll) > 2: # XXX interpret height unit

830 h = float(ll.pop(2).rstrip(_LETTERS + _SPACE_))

831 else:

832 h = height # None from wgrs.Georef.__new__

833 if len(ll) != 2:

834 raise ValueError

835

836 a, b = [_.strip() for _ in ll] # PYCHOK false

837 if a[-1:] in _EW_ or b[-1:] in _NS_:

838 a, b = b, a

839 t = _2Tuple(a, b, clipLat, clipLon, wrap, **s_D_M_S)

840 return t.to3Tuple(h)

841

842 return _parseX(_3llh, strllh, height, sep, wrap, strllh=strllh)

843

844

845 def parseRad(strRad, suffix=_NSEW_, clip=0):

846 '''Parse a string representing angle in C{radians}.

847

848 @arg strRad: Degrees in any of several forms (C{str} or C{radians}).

849 @kwarg suffix: Optional, valid compass points (C{str}, C{tuple}).

850 @kwarg clip: Optionally, limit value to range C{-/+B{clip}} (C{radians}).

851

852 @return: Radians (C{float}).

853

854 @raise ParseError: Invalid B{C{strRad}} or B{C{clip}}.

855

856 @raise RangeError: Value of B{C{strRad}} outside the valid C{-/+B{clip}}

857 range and L{rangerrors<pygeodesy.rangerrors>} is C{True}.

858 '''

859 def _Rad(strRad, suffix, clip):

860 try:

861 r = float(strRad)

862 except (TypeError, ValueError):

863 s, t, P = _split3(strRad, suffix.upper())

864 r = _dms2deg(s, P, float(t))

865 return clipRadians(r, float(clip)) if clip else r

866

867 return _parseX(_Rad, strRad, suffix, clip, strRad=strRad, suffix=suffix)

868

869

870 def precision(form, prec=None):

871 '''Set the default precison for a given F_ form.

872

873 @arg form: L{F_D}, L{F_DM}, L{F_DMS}, L{F_DEG}, L{F_MIN}, L{F_SEC},

874 L{F_D60}, L{F__E}, L{F__F}, L{F__G} or L{F_RAD} (C{str}).

875 @kwarg prec: Number of decimal digits (0..9 or C{None} for default).

876 Trailing zero decimals are stripped for C{B{prec}=1}

877 and above, but kept for negative B{C{prec}}.

878

879 @return: Previous precision for the B{C{form}} (C{int}).

880

881 @raise ValueError: Invalid B{C{form}} or B{C{prec}} or B{C{prec}}

882 outside range C{-9..+9}.

883 '''

884 try:

885 p = _F_prec[form]

886 except KeyError:

887 raise _ValueError(form=form)

888 if prec is not None: # set as default

889 P_ = _MODS.units.Precision_

890 _F_prec[form] = P_(prec, low=-9, high=9)

891 return p

892

893

894 def toDMS(deg, form=_F_DMS, prec=2, sep=S_SEP, ddd=2, neg=_MINUS_, pos=_PLUS_, **s_D_M_S):

895 '''Convert I{signed} C{degrees} to string, without suffix.

896

897 @arg deg: Degrees to be formatted (C{scalar degrees}).

898 @kwarg form: Format specifier for B{C{deg}} (C{str} or L{F_D}, L{F_DM}, L{F_DMS},

899 L{F_DEG}, L{F_MIN}, L{F_SEC}, L{F_D60}, L{F__E}, L{F__F}, L{F__G},

900 L{F_RAD}, L{F_D_}, L{F_DM_}, L{F_DMS_}, L{F_DEG_}, L{F_MIN_}, L{F_SEC_},

901 L{F_D60_}, L{F__E_}, L{F__F_}, L{F__G_}, L{F_RAD_}, L{F_D__}, L{F_DM__},

902 L{F_DMS__}, L{F_DEG__}, L{F_MIN__}, L{F_SEC__}, L{F_D60__}, L{F__E__},

903 L{F__F__}, L{F__G__} or L{F_RAD__}).

904 @kwarg prec: Number of decimal digits (0..9 or C{None} for default). Trailing zero

905 decimals are stripped for C{B{prec}=1} and above, but kept for negative

906 B{C{prec}}.

907 @kwarg sep: Separator between degrees, minutes, seconds, suffix (C{str}).

908 @kwarg ddd: Number of (integer) digits for B{C{deg}°} (2 or 3).

909 @kwarg neg: Prefix for negative B{C{deg}} (C{'-'}).

910 @kwarg pos: Prefix for positive B{C{deg}} and signed B{C{form}} (C{'+'}).

911 @kwarg s_D_M_S: Optional keyword arguments C{B{s_D}=}L{S_DEG}, C{B{s_M}=}L{S_MIN}

912 C{B{s_S}=}L{S_SEC}, C{B{s_R}=}L{S_RAD} and C{B{s_DMS}=True} to

913 override any or cancel all DMS symbol suffixes. See the B{Notes}

914 below.

915

916 @return: Degrees in the specified form (C{str}).

917

918 @note: The degrees, minutes and seconds (DMS) symbol can be overridden in this and

919 other C{*DMS} functions by using optional keyword argments C{B{s_D}="d"},

920 C{B{s_M}="'"} respectively C{B{s_S}='"'}. Using B{C{s_DMS}=None} cancels

921 all C{DMS} symbols to C{""} aka L{pygeodesy.NN}.

922

923 @note: Sexagecimal format B{C{F_D60}} supports overridable pseudo-DMS symbols

924 positioned at C{"[D]DD<B{s_D}>MM<B{s_M}>SS<B{s_S}>"} with defaults

925 C{B{s_D}="."}, C{B{s_M}=B{sep}} and C{B{s_S}=}L{pygeodesy.NN}.

926

927 @note: Formats B{C{F__E}}, B{C{F__F}} and B{C{F__G}} is extended with a C{D}-only

928 symbol suffix if defined with keyword argument C{B{s_D}=}L{pygeodesy.NN}.

929 Likewise for B{C{F_RAD}} forms with keyword argument C{B{s_R}=}L{S_RAD}.

930

931 @see: Function L{pygeodesy.degDMS}

932 '''

933 s = form[:1]

934 f = form[1:] if s in _PLUSMINUS_ else form

935 t = _toDMS(deg, f, prec, sep, ddd, NN, s_D_M_S) # unsigned and -suffixed

936 if deg < 0 and neg:

937 t = neg + t

938 elif deg > 0 and s == _PLUS_ and pos:

939 t = pos + t

940 return t

941

942# **) MIT License

943#

944# Copyright (C) 2016-2024 -- mrJean1 at Gmail -- All Rights Reserved.

945#

946# Permission is hereby granted, free of charge, to any person obtaining a

947# copy of this software and associated documentation files (the "Software"),

948# to deal in the Software without restriction, including without limitation

949# the rights to use, copy, modify, merge, publish, distribute, sublicense,

950# and/or sell copies of the Software, and to permit persons to whom the

951# Software is furnished to do so, subject to the following conditions:

952#

953# The above copyright notice and this permission notice shall be included

954# in all copies or substantial portions of the Software.

955#

956# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

957# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

958# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

959# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

960# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

961# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

962# OTHER DEALINGS IN THE SOFTWARE.