# Coverage for pygeodesy/trf.py : 93%

## 83 statements 77 run 6 missing 16 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 | # -*- coding: utf-8 -*- u'''Terrestrial Reference Frame (TRF) classes L{RefFrame}, registry L{RefFrames} and L{TRFError}. Transcribed from I{Chris Veness'} (C) 2006-2019 JavaScript originals U{latlon-ellipsoidal-referenceframe.js<https://GitHub.com/chrisveness/geodesy/blob/master/ latlon-ellipsoidal-referenceframe.js>} and U{latlon-ellipsoidal-referenceframe-txparams.js <https://GitHub.com/chrisveness/geodesy/blob/master/latlon-ellipsoidal-referenceframe-txparams.js>}. Modern geodetic reference frames: a latitude/longitude point defines a geographic location on, above or below the earth’s surface, measured in degrees from the equator and the U{International Reference Meridian<https://WikiPedia.org/wiki/IERS_Reference_Meridian>} (IRM) and metres above the ellipsoid within a given I{Terrestrial Reference Frame} at a given I{epoch}. This is scratching the surface of complexities involved in high precision geodesy, but may be of interest and/or value to those with less demanding requirements. More information U{here <https://www.Movable-Type.co.UK/scripts/geodesy-library.html>} and U{here <https://www.Movable-Type.co.UK/scripts/geodesy-library.html#latlon-ellipsoidal-referenceframe>}. Note that I{ITRF solutions} do not directly use an ellipsoid, but are specified by Cartesian coordinates. The GRS80 ellipsoid is recommended for transformations to geographical coordinates. Note WGS84(G730/G873/G1150) are coincident with ITRF at 10-centimetre level, see also U{here <ftp://ITRF.ENSG.IGN.FR/pub/itrf/WGS84.TXT>}. WGS84(G1674) and ITRF20014 / ITRF2008 ‘are likely to agree at the centimeter level’, see also U{QPS/QINSy<https://Confluence.QPS.NL/qinsy/ en/how-to-deal-with-etrs89-datum-and-time-dependent-transformation-parameters-45353274.html>}. @var RefFrames.ETRF2000: RefFrame(name='ETRF2000', epoch=2005.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.GDA94: RefFrame(name='GDA94', epoch=1994.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF2000: RefFrame(name='ITRF2000', epoch=1997.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF2005: RefFrame(name='ITRF2005', epoch=2000.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF2008: RefFrame(name='ITRF2008', epoch=2005.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF2014: RefFrame(name='ITRF2014', epoch=2010.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF91: RefFrame(name='ITRF91', epoch=1988.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.ITRF93: RefFrame(name='ITRF93', epoch=1988.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.NAD83: RefFrame(name='NAD83', epoch=1997.0, ellipsoid=Ellipsoid(name='GRS80') @var RefFrames.WGS84g1150: RefFrame(name='WGS84g1150', epoch=2001.0, ellipsoid=Ellipsoid(name='WGS84') @var RefFrames.WGS84g1674: RefFrame(name='WGS84g1674', epoch=2005.0, ellipsoid=Ellipsoid(name='WGS84') @var RefFrames.WGS84g1762: RefFrame(name='WGS84g1762', epoch=2005.0, ellipsoid=Ellipsoid(name='WGS84') ''' from pygeodesy.basics import _isnotError, isscalar, map1, property_RO, \ _TypeError from pygeodesy.datum import Ellipsoid, Ellipsoids, Transform from pygeodesy.lazily import _ALL_LAZY from pygeodesy.named import classname, _NamedDict as _X, \ _NamedEnum, _NamedEnumItem from pygeodesy.streprs import fstrzs __all__ = _ALL_LAZY.trf __version__ = '20.03.23' _mDays = (0, 31, 29, 31, 30, 31, 30, 31, 31, 30, 31, 30, 31) # temporarily hold a single instance for each float value and name _trfFs = {} # trashed below _trfSs = {} # trashed below def _F(f): '''(INTERNAL) Cache a single C{float}. ''' return _trfFs.setdefault(f, f) # PYCHOK undefined by del _trfFs def _S(n): '''(INTERNAL) Cache a single C{str}. ''' return _trfSs.setdefault(n, n) # PYCHOK undefined by del _trfSs def _S2(n1, n2): '''(INTERNAL) Cache two C{str}s. ''' return _S(n1), _S(n2) def _T(*fs): '''(INTERNAL) Cache a tuple of single C{float}s. ''' return map1(_F, *fs) def _2epoch(epoch): # imported by .ellipsoidalBase.py '''(INTERNAL) Validate an C{epoch}. ''' if isscalar(epoch) and epoch > 0: # XXX 1970? return _F(epoch) raise _isnotError('scalar', epoch=epoch) class TRFError(ValueError): '''Terrestrial Reference Frame (TRF) or L{RefFrame} conversion issue. ''' pass class RefFrame(_NamedEnumItem): '''Terrestrial Reference Frame (TRF) parameters. ''' _ellipsoid = None #: Ellipsoid GRS80 or WGS84 (L{Ellipsoid}). _epoch = 0 #: Epoch, calendar year (C{float}). def __init__(self, epoch, ellipsoid, name=''): '''New L{RefFrame}. @arg epoch: Epoch, a fractional calendar year (C{scalar}). @arg ellipsoid: The ellipsoid (L{Ellipsoid}). @kwarg name: Optional, unique name (C{str}). @raise NameError: A L{RefFrame} with that B{C{name}} already exists. @raise TypeError: If B{C{epoch}} is not C{scalar} or B{C{ellipsoid}} is not an L{Ellipsoid}. ''' _TypeError(Ellipsoid, ellipsoid=ellipsoid) self._ellipsoid = ellipsoid self._epoch = _2epoch(epoch) self._register(RefFrames, name) @property_RO def ellipsoid(self): '''Get this reference frame's ellipsoid (L{Ellipsoid}). ''' return self._ellipsoid @property_RO def epoch(self): '''Get this reference frame's epoch (C{float}). ''' return self._epoch def toStr(self): # PYCHOK expected '''Return this reference frame as a text string. @return: This L{RefFrame}'s attributes (C{str}). ''' e = self.ellipsoid t = ('name=%r' % (self.name,), 'epoch=%s' % (fstrzs('%.3F' % (self.epoch,)),), 'ellipsoid=%s(name=%r)' % (classname(e), e.name)) return ', '.join(t) RefFrames = _NamedEnum('RefFrames', RefFrame) #: Registered reference frames. # <https://GitHub.com/chrisveness/geodesy/blob/master/latlon-ellipsoidal-referenceframe.js> RefFrames._assert( # ITRF2014AU = RefFrame(_F(2020.0), Ellipsoids.GRS80, _S('ITRF2014AU')), ITRF2014 = RefFrame(_F(2010.0), Ellipsoids.GRS80, _S('ITRF2014')), ITRF2008 = RefFrame(_F(2005.0), Ellipsoids.GRS80, _S('ITRF2008')), ITRF2005 = RefFrame(_F(2000.0), Ellipsoids.GRS80, _S('ITRF2005')), ITRF2000 = RefFrame(_F(1997.0), Ellipsoids.GRS80, _S('ITRF2000')), ITRF93 = RefFrame(_F(1988.0), Ellipsoids.GRS80, _S('ITRF93')), ITRF91 = RefFrame(_F(1988.0), Ellipsoids.GRS80, _S('ITRF91')), WGS84g1762 = RefFrame(_F(2005.0), Ellipsoids.WGS84, _S('WGS84g1762')), WGS84g1674 = RefFrame(_F(2005.0), Ellipsoids.WGS84, _S('WGS84g1674')), WGS84g1150 = RefFrame(_F(2001.0), Ellipsoids.WGS84, _S('WGS84g1150')), ETRF2000 = RefFrame(_F(2005.0), Ellipsoids.GRS80, _S('ETRF2000')), # ETRF2000(R08) NAD83 = RefFrame(_F(1997.0), Ellipsoids.GRS80, _S('NAD83')), # CORS96 GDA94 = RefFrame(_F(1994.0), Ellipsoids.GRS80, _S('GDA94'))) def date2epoch(year, month, day): '''Return the reference frame C{epoch} for a calendar day. @arg year: Year of the date (C{scalar}). @arg month: Month in the B{C{year}} (C{scalar}, 1..12). @arg day: Day in the B{C{month}} (C{scalar}, 1..31). @return: Epoch, the fractional year (C{float}). @raise TRFError: Invalid B{C{year}}, B{C{month}} or B{C{day}}. @note: Any B{C{year}} is considered a leap year, i.e. having 29 days in February. ''' try: y, m, d = map1(int, year, month, day) if y > 0 and 1 <= m <= 12 and 1 <= d <= _mDays[m]: return y + float(sum(_mDays[:m]) + d) / 366.0 except (ValueError, TypeError): pass raise TRFError('%s invalid: %s-%s-%s' % ('date', year, month, day)) # TRF conversions specified as 7-parameter Helmert transforms and an epoch. Most # from U{Transformation Parameters<http://ITRF.IGN.FR/trans_para.php>}, more at U{QPS # <https://Confluence.QPS.NL/qinsy/files/en/29856813/45482834/2/1453459502000/ITRF_Transformation_Parameters.xlsx>}. _trfNs = ('tx', 'ty', 'tz', 's', 'sx', 'sy', 'sz') _trfXs = { # (from_TRF, to_TRF): mm mm mm ppb mas mas mas # see U{Transformation Parameters ITRF2014<http://ITRF.IGN.FR/doc_ITRF/Transfo-ITRF2014_ITRFs.txt>} _S2('ITRF2014', 'ITRF2008'): _X(epoch=_F(2010.0), # <http://ITRF.ENSG.IGN.FR/ITRF_solutions/2014/tp_14-08.php> xform=_T( 1.6, 1.9, 2.4, -0.02, 0.0, 0.0, 0.0), rates=_T( 0.0, 0.0, -0.1, 0.03, 0.0, 0.0, 0.0)), _S2('ITRF2014', 'ITRF2005'): _X(epoch=_F(2010.0), xform=_T( 2.6, 1.0, -2.3, 0.92, 0.0, 0.0, 0.0), rates=_T( 0.3, 0.0, -0.1, 0.03, 0.0, 0.0, 0.0)), _S2('ITRF2014', 'ITRF2000'): _X(epoch=_F(2010.0), xform=_T( 0.7, 1.2, -26.1, 2.12, 0.0, 0.0, 0.0), rates=_T( 0.1, 0.1, -1.9, 0.11, 0.0, 0.0, 0.0)), _S2('ITRF2014', 'ITRF97'): _X(epoch=_F(2010.0), xform=_T( 7.4, -0.5, -62.8, 3.8, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF96'): _X(epoch=_F(2010.0), xform=_T( 7.4, -0.5, -62.8, 3.8, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF94'): _X(epoch=_F(2010.0), xform=_T( 7.4, -0.5, -62.8, 3.8, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF93'): _X(epoch=_F(2010.0), xform=_T(-50.4, 3.3, -60.2, 4.29, -2.81, -3.38, 0.4), rates=_T( -2.8, -0.1, -2.5, 0.12, -0.11, -0.19, 0.07)), _S2('ITRF2014', 'ITRF92'): _X(epoch=_F(2010.0), xform=_T( 15.4, 1.5, -70.8, 3.09, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF91'): _X(epoch=_F(2010.0), xform=_T( 27.4, 15.5, -76.8, 4.49, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF90'): _X(epoch=_F(2010.0), xform=_T( 25.4, 11.5, -92.8, 4.79, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF89'): _X(epoch=_F(2010.0), xform=_T( 30.4, 35.5, -130.8, 8.19, 0.0, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), _S2('ITRF2014', 'ITRF88'): _X(epoch=_F(2010.0), xform=_T( 25.4, -0.5, -154.8, 11.29, 0.1, 0.0, 0.26), rates=_T( 0.1, -0.5, -3.3, 0.12, 0.0, 0.0, 0.02)), # see U{Transformation Parameters ITRF2008<http://ITRF.IGN.FR/doc_ITRF/Transfo-ITRF2008_ITRFs.txt>} # _S2('ITRF2008', 'ITRF2005'): _X(epoch=_F(2005.0), # <http://ITRF.ENSG.IGN.FR/ITRF_solutions/2008/tp_08-05.php> # xform=_T( -0.5, -0.9, -4.7, 0.94, 0.0, 0.0, 0.0), # rates=_T( 0.3, 0.0, 0.0, 0.0, 0.0, 0.0, 0.0)), _S2('ITRF2008', 'ITRF2005'): _X(epoch=_F(2000.0), xform=_T( -2.0, -0.9, -4.7, 0.94, 0.0, 0.0, 0.0), rates=_T( 0.3, 0.0, 0.0, 0.0, 0.0, 0.0, 0.0)), _S2('ITRF2008', 'ITRF2000'): _X(epoch=_F(2000.0), xform=_T( -1.9, -1.7, -10.5, 1.34, 0.0, 0.0, 0.0), rates=_T( 0.1, 0.1, -1.8, 0.08, 0.0, 0.0, 0.0)), _S2('ITRF2008', 'ITRF97'): _X(epoch=_F(2000.0), xform=_T( 4.8, 2.6, -33.2, 2.92, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF96'): _X(epoch=_F(2000.0), xform=_T( 4.8, 2.6, -33.2, 2.92, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF94'): _X(epoch=_F(2000.0), xform=_T( 4.8, 2.6, -33.2, 2.92, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF93'): _X(epoch=_F(2000.0), xform=_T(-24.0, 2.4, -38.6, 3.41, -1.71, -1.48, -0.3), rates=_T( -2.8, -0.1, -2.4, 0.09, -0.11, -0.19, 0.07)), _S2('ITRF2008', 'ITRF92'): _X(epoch=_F(2000.0), xform=_T( 12.8, 4.6, -41.2, 2.21, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF91'): _X(epoch=_F(2000.0), xform=_T( 24.8, 18.6, -47.2, 3.61, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF90'): _X(epoch=_F(2000.0), xform=_T( 22.8, 14.6, -63.2, 3.91, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF89'): _X(epoch=_F(2000.0), xform=_T( 27.8, 38.6, -101.2, 7.31, 0.0, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2008', 'ITRF88'): _X(epoch=_F(2000.0), xform=_T( 22.8, 2.6, -125.2, 10.41, 0.1, 0.0, 0.06), rates=_T( 0.1, -0.5, -3.2, 0.09, 0.0, 0.0, 0.02)), _S2('ITRF2005', 'ITRF2000'): _X(epoch=_F(2000.0), # <http://ITRF.ENSG.IGN.FR/ITRF_solutions/2005/tp_05-00.php> xform=_T( 0.1, -0.8, -5.8, 0.4, 0.0, 0.0, 0.0), rates=_T( -0.2, 0.1, -1.8, 0.08, 0.0, 0.0, 0.0)), _S2('ITRF2000', 'ITRF97'): _X(epoch=_F(1997.0), xform=_T( 0.67, 0.61, -1.85, 1.55, 0.0, 0.0, 0.0), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF96'): _X(epoch=_F(1997.0), xform=_T( 0.67, 0.61, -1.85, 1.55, 0.0, 0.0, 0.0), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF94'): _X(epoch=_F(1997.0), xform=_T( 0.67, 0.61, -1.85, 1.55, 0.0, 0.0, 0.0), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF93'): _X(epoch=_F(1988.0), xform=_T( 12.7, 6.5, -20.9, 1.95, -0.39, 0.8, -1.14), rates=_T( -2.9, -0.2, -0.6, 0.01, -0.11, -0.19, 0.07)), _S2('ITRF2000', 'ITRF92'): _X(epoch=_F(1988.0), xform=_T( 1.47, 1.35, -1.39, 0.75, 0.0, 0.0, -0.18), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF91'): _X(epoch=_F(1988.0), xform=_T( 26.7, 27.5, -19.9, 2.15, 0.0, 0.0, -0.18), rates=_T( 0.0, -0.6, -1.4, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF90'): _X(epoch=_F(1988.0), xform=_T( 2.47, 2.35, -3.59, 2.45, 0.0, 0.0, -0.18), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF89'): _X(epoch=_F(1988.0), xform=_T( 2.97, 4.75, -7.39, 5.85, 0.0, 0.0, -0.18), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), _S2('ITRF2000', 'ITRF88'): _X(epoch=_F(1988.0), xform=_T( 2.47, 1.15, -9.79, 8.95, 0.1, 0.0, -0.18), rates=_T( 0.0, -0.06, -0.14, 0.01, 0.0, 0.0, 0.02)), # see U{Boucher, C. & Altamimi, Z. "Memo: Specifications for reference frame fixing in the # analysis of a EUREF GPS campaign" (2011) <https://ETRS89.ENSG.IGN.FR/memo-V8.pdf>} and # Altamimi, Z. U{"Key results of ITRF2014 and implication to ETRS89 realization", EUREF2016 # <https://www.EUREF.EU/symposia/2016SanSebastian/01-02-Altamimi.pdf>}. _S2('ITRF2014', 'ETRF2000'): _X(epoch=_F(2000.0), xform=_T( 53.7, 51.2, -55.1, 1.02, 0.891, 5.39, -8.712), rates=_T( 0.1, 0.1, -1.9, 0.11, 0.081, 0.49, -0.792)), _S2('ITRF2008', 'ETRF2000'): _X(epoch=_F(2000.0), xform=_T( 52.1, 49.3, -58.5, 1.34, 0.891, 5.39, -8.712), rates=_T( 0.1, 0.1, -1.8, 0.08, 0.081, 0.49, -0.792)), _S2('ITRF2005', 'ETRF2000'): _X(epoch=_F(2000.0), xform=_T( 54.1, 50.2, -53.8, 0.4, 0.891, 5.39, -8.712), rates=_T( -0.2, 0.1, -1.8, 0.08, 0.081, 0.49, -0.792)), _S2('ITRF2000', 'ETRF2000'): _X(epoch=_F(2000.0), xform=_T( 54.0, 51.0, -48.0, 0.0, 0.891, 5.39, -8.712), rates=_T( 0.0, 0.0, 0.0, 0.0, 0.081, 0.49, -0.792)), # see U{Solar, T. & Snay, R.A. "Transforming Positions and Velocities between the # International Terrestrial Reference Frame of 2000 and North American Datum of 1983" # (2004)<https://www.NGS.NOAA.gov/CORS/Articles/SolerSnayASCE.pdf>} _S2('ITRF2000', 'NAD83'): _X(epoch=_F(1997.0), # note NAD83(CORS96) xform=_T(995.6, -1901.3, -521.5, 0.62, 25.915, 9.426, 11.599), rates=_T( 0.7, -0.7, 0.5, -0.18, 0.067, -0.757, -0.051)), # see Table 2 in U{Dawson, J. & Woods, A. "ITRF to GDA94 coordinate transformations", Journal of # Applied Geodesy 4 (2010), 189-199<https://www.ResearchGate.net/publication/258401581_ITRF_to_GDA94_coordinate_transformations>} # (note, sign of rotations for GDA94 reversed as "Australia assumes rotation to be of coordinate # axes" rather than the more conventional "position around the coordinate axes") _S2('ITRF2008', 'GDA94'): _X(epoch=_F(1994.0), xform=_T(-84.68, -19.42, 32.01, 9.71, -0.4254, 2.2578, 2.4015), rates=_T( 1.42, 1.34, 0.9, 0.109, 1.5461, 1.182, 1.1551)), _S2('ITRF2005', 'GDA94'): _X(epoch=_F(1994.0), xform=_T(-79.73, -6.86, 38.03, 6.636, 0.0351, -2.1211, -2.1411), rates=_T( 2.25, -0.62, -0.56, 0.294, -1.4707, -1.1443, -1.1701)), _S2('ITRF2000', 'GDA94'): _X(epoch=_F(1994.0), xform=_T(-45.91, -29.85, -20.37, 7.07, -1.6705, 0.4594, 1.9356), rates=_T( -4.66, 3.55, 11.24, 0.249, 1.7454, 1.4868, 1.224)), } _Forward = 1.0e-3 # mm2m, ppb2ppM, mas2as _Reverse = -1.0e-3 # same, inverse transforms def _intermediate(n1, n2): '''(INTERNAL) Find a trf* "in between" C{n1} and C{n2}. ''' f1 = set(m for n, m in _trfXs.keys() if n == n1) # from trf1 t2 = set(n for n, m in _trfXs.keys() if m == n2) # to trf2 n = f1.intersection(t2) return n.pop() if n else '' def _reframeTransforms(rf2, rf, epoch): '''(INTERNAL) Get 0, 1 or 2 Helmert C{Transforms} to convert reference frame C{rf} observed at C{epoch} into C{rf2}. ''' n2 = rf2.name # .upper() n1 = rf.name # .upper() if n1 == n2 or (n1.startswith('ITRF') and n2.startswith('WGS84')) \ or (n2.startswith('ITRF') and n1.startswith('WGS84')): return () # PYCHOK returns if (n1, n2) in _trfXs: return (_2Transform((n1, n2), epoch, _Forward),) # PYCHOK returns if (n2, n1) in _trfXs: return (_2Transform((n2, n1), epoch, _Reverse),) # PYCHOK returns n = _intermediate(n1, n2) if n: return (_2Transform((n1, n), epoch, _Forward), # PYCHOK returns _2Transform((n, n2), epoch, _Forward)) n = _intermediate(n2, n1) if n: return (_2Transform((n, n1), epoch, _Reverse), # PYCHOK returns _2Transform((n2, n), epoch, _Reverse)) raise TRFError('no %s % to %s' % ('conversion', n1, n2)) def _2Transform(n1_n2, epoch, _Forward_Reverse): '''(INTERNAL) Combine a 14-element Helmert C{trfX} and C{d_epoch} into a single 7-element C{Transform}. ''' X = _trfXs[n1_n2] e = epoch - X.epoch # fractional delta years d = dict((n, (x + r * e) * _Forward_Reverse) for n, x, r in zip(_trfNs, X.xform, X.rates)) t = Transform(**d) return t if __name__ == '__main__': def _percent(L, cache, number, nl): n = len(cache) m = len(RefFrames) + len(_trfXs) * number t = L, n, m, L, (n * 100.0 / m), nl print('len(_trf%ss) %3d / %3d %ss: %.1F%%%s' % t) _percent('F', _trfFs, 15, '') _percent('S', _trfSs, 2, '\n') for m in range(1, 13): y, d = 2020, _mDays[m] print('date2epoch(%d, %d, %d) %.3F' % (y, m, d, date2epoch(y, m, d))) # __doc__ of this file t = [''] + repr(RefFrames).split('\n') print('\n@var '.join(i.strip(',') for i in t)) _F = float # float back to normal _S = str # str back to normal del _trfFs # trash floats cache del _trfSs # trash strs cache # **) MIT License # # Copyright (C) 2016-2020 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE. # % python -m pygeodesy.trf # len(_trfFs) 216 / len(_trfXs) 627: 34.4% # # date2epoch(2020, 1, 31) 2020.085 # date2epoch(2020, 2, 29) 2020.164 # date2epoch(2020, 3, 31) 2020.249 # date2epoch(2020, 4, 30) 2020.331 # date2epoch(2020, 5, 31) 2020.415 # date2epoch(2020, 6, 30) 2020.497 # date2epoch(2020, 7, 31) 2020.582 # date2epoch(2020, 8, 31) 2020.667 # date2epoch(2020, 9, 30) 2020.749 # date2epoch(2020, 10, 31) 2020.833 # date2epoch(2020, 11, 30) 2020.915 # date2epoch(2020, 12, 31) 2021.000