### Navigation

- index
- modules |
- pywws 14.03.dev1177 documentation »
- Module code »

# Source code for pywws.WeatherStation

    # pywws - Python software for USB Wireless Weather Stations
    # http://github.com/jim-easterbrook/pywws
    # Copyright (C) 2008-13  Jim Easterbrook  jim@jim-easterbrook.me.uk

    # This program is free software; you can redistribute it and/or
    # modify it under the terms of the GNU General Public License
    # as published by the Free Software Foundation; either version 2
    # of the License, or (at your option) any later version.

    # This program is distributed in the hope that it will be useful,
    # but WITHOUT ANY WARRANTY; without even the implied warranty of
    # MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    # GNU General Public License for more details.

    # You should have received a copy of the GNU General Public License
    # along with this program; if not, write to the Free Software
    # Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA  02110-1301, USA.

    """Get data from WH1080/WH3080 compatible weather stations.

    Derived from wwsr.c by Michael Pendec (michael.pendec@gmail.com),
    wwsrdump.c by Svend Skafte (svend@skafte.net), modified by Dave Wells,
    and other sources.

    Introduction
    ------------

    This is the module that actually talks to the weather station base
    unit. I don't have much understanding of USB, so copied a lot from
    Michael Pendec's C program wwsr.

    The weather station memory has two parts: a "fixed block" of 256 bytes
    and a circular buffer of 65280 bytes. As each weather reading takes 16
    bytes the station can store 4080 readings, or 14 days of 5-minute
    interval readings. (The 3080 type stations store 20 bytes per reading,
    so store a maximum of 3264.) As data is read in 32-byte chunks, but
    each weather reading is 16 or 20 bytes, a small cache is used to
    reduce USB traffic. The caching behaviour can be over-ridden with the
    ``unbuffered`` parameter to ``get_data`` and ``get_raw_data``.

    Decoding the data is controlled by the static dictionaries
    ``reading_format``, ``lo_fix_format`` and ``fixed_format``. The keys
    are names of data items and the values can be an ``(offset, type,
    multiplier)`` tuple or another dictionary. So, for example, the
    reading_format dictionary entry ``'rain' : (13, 'us', 0.3)`` means
    that the rain value is an unsigned short (two bytes), 13 bytes from
    the start of the block, and should be multiplied by 0.3 to get a
    useful value.

    The use of nested dictionaries in the ``fixed_format`` dictionary
    allows useful subsets of data to be decoded. For example, to decode
    the entire block ``get_fixed_block`` is called with no parameters::

      ws = WeatherStation.weather_station()
      print ws.get_fixed_block()

    To get the stored minimum external temperature, ``get_fixed_block`` is
    called with a sequence of keys::

      ws = WeatherStation.weather_station()
      print ws.get_fixed_block(['min', 'temp_out', 'val'])

    Often there is no requirement to read and decode the entire fixed
    block, as its first 64 bytes contain the most useful data: the
    interval between stored readings, the buffer address where the current
    reading is stored, and the current date & time. The
    ``get_lo_fix_block`` method provides easy access to these.

    For more examples of using the WeatherStation module, see the
    TestWeatherStation program.

    Detailed API
    ------------

    """

    __docformat__ = "restructuredtext en"

    from datetime import datetime
    import logging
    import sys
    import time

    from pywws import Localisation
    USBDevice = None
    if not USBDevice:
        try:
            from pywws.device_ctypes_hidapi import USBDevice
        except ImportError:
            pass
    if not USBDevice:
        try:
            from pywws.device_cython_hidapi import USBDevice
        except ImportError:
            pass
    if not USBDevice:
        try:
            from pywws.device_pyusb1 import USBDevice
        except ImportError:
            pass
    if not USBDevice:
        from pywws.device_pyusb import USBDevice

    # get meaning for status integer
    rain_overflow   = 0x80
    lost_connection = 0x40
    unknown         = 0x20
    unknown         = 0x10
    unknown         = 0x08
    unknown         = 0x04
    unknown         = 0x02
    unknown         = 0x01

    def decode_status(status):
        result = {}
        for key, mask in (('rain_overflow',   0x80),
                          ('lost_connection', 0x40),
                          ('unknown',         0x3f),
                          ):
            result[key] = status & mask
        return result

    # decode weather station raw data formats
    def _decode(raw, format):
        def _signed_byte(raw, offset):
            res = raw[offset]
            if res == 0xFF:
                return None
            sign = 1
            if res >= 128:
                sign = -1
                res = res - 128
            return sign * res
        def _signed_short(raw, offset):
            lo = raw[offset]
            hi = raw[offset+1]
            if lo == 0xFF and hi == 0xFF:
                return None
            sign = 1
            if hi >= 128:
                sign = -1
                hi = hi - 128
            return sign * ((hi * 256) + lo)
        def _unsigned_short(raw, offset):
            lo = raw[offset]
            hi = raw[offset+1]
            if lo == 0xFF and hi == 0xFF:
                return None
            return (hi * 256) + lo
        def _unsigned_int3(raw, offset):
            lo = raw[offset]
            md = raw[offset+1]
            hi = raw[offset+2]
            if lo == 0xFF and md == 0xFF and hi == 0xFF:
                return None
            return (hi * 256 * 256) + (md * 256) + lo
        def _bcd_decode(byte):
            hi = (byte // 16) & 0x0F
            lo = byte & 0x0F
            return (hi * 10) + lo
        def _date_time(raw, offset):
            year = _bcd_decode(raw[offset])
            month = _bcd_decode(raw[offset+1])
            day = _bcd_decode(raw[offset+2])
            hour = _bcd_decode(raw[offset+3])
            minute = _bcd_decode(raw[offset+4])
            return '%4d-%02d-%02d %02d:%02d' % (year + 2000, month, day, hour, minute)
        def _bit_field(raw, offset):
            mask = 1
            result = []
            for i in range(8):
                result.append(raw[offset] & mask != 0)
                mask = mask << 1
            return result
        if not raw:
            return None
        if isinstance(format, dict):
            result = {}
            for key, value in format.items():
                result[key] = _decode(raw, value)
        else:
            pos, type, scale = format
            if type == 'ub':
                result = raw[pos]
                if result == 0xFF:
                    result = None
            elif type == 'sb':
                result = _signed_byte(raw, pos)
            elif type == 'us':
                result = _unsigned_short(raw, pos)
            elif type == 'u3':
                result = _unsigned_int3(raw, pos)
            elif type == 'ss':
                result = _signed_short(raw, pos)
            elif type == 'dt':
                result = _date_time(raw, pos)
            elif type == 'tt':
                result = '%02d:%02d' % (_bcd_decode(raw[pos]),
                                        _bcd_decode(raw[pos+1]))
            elif type == 'pb':
                result = raw[pos]
            elif type == 'wa':
                # wind average - 12 bits split across a byte and a nibble
                result = raw[pos] + ((raw[pos+2] & 0x0F) << 8)
                if result == 0xFFF:
                    result = None
            elif type == 'wg':
                # wind gust - 12 bits split across a byte and a nibble
                result = raw[pos] + ((raw[pos+1] & 0xF0) << 4)
                if result == 0xFFF:
                    result = None
            elif type == 'bf':
                # bit field - 'scale' is a list of bit names
                result = {}
                for k, v in zip(scale, _bit_field(raw, pos)):
                    result[k] = v
                return result
            else:
                raise IOError('unknown type %s' % type)
            if scale and result:
                result = float(result) * scale
        return result

    class CUSBDrive(object):
        """Low level interface to weather station via USB.

        Loosely modeled on a C++ class obtained from
        http://site.ambientweatherstore.com/easyweather/ws_1080_2080_protocol.zip.
        I don't know the provenance of this, but it looks as if it may
        have come from the manufacturer.

        """
        EndMark          = 0x20
        ReadCommand      = 0xA1
        WriteCommand     = 0xA0
        WriteCommandWord = 0xA2

        def __init__(self):
            self.logger = logging.getLogger('pywws.WeatherStation.CUSBDrive')
            self.logger.info('using %s', USBDevice.__module__)
            self.dev = USBDevice(0x1941, 0x8021)

        def read_block(self, address):
            """Read 32 bytes from the weather station.

            If the read fails for any reason, :obj:`None` is returned.

            :param address: address to read from.

            :type address: int

            :return: the data from the weather station.

            :rtype: list(int)

            """
            buf = [
                self.ReadCommand,
                address // 256,
                address % 256,
                self.EndMark,
                self.ReadCommand,
                address // 256,
                address % 256,
                self.EndMark,
                ]
            if not self.dev.write_data(buf):
                return None
            return self.dev.read_data(32)

        def write_byte(self, address, data):
            """Write a single byte to the weather station.

            :param address: address to write to.

            :type address: int

            :param data: the value to write.

            :type data: int

            :return: success status.

            :rtype: bool

            """
            buf = [
                self.WriteCommandWord,
                address // 256,
                address % 256,
                self.EndMark,
                self.WriteCommandWord,
                data,
                0,
                self.EndMark,
                ]
            if not self.dev.write_data(buf):
                return False
            buf = self.dev.read_data(8)
            if buf is None:
                return False
            for byte in buf:
                if byte != 0xA5:
                    return False
            return True

    class weather_station(object):
        """Class that represents the weather station to user program."""
        # minimum interval between polling for data change
        min_pause = 0.5
        # margin of error for various decisions
        margin = (min_pause * 2.0) - 0.1
        def __init__(self, ws_type='1080', params=None, status=None, avoid=3.0):
            """Connect to weather station and prepare to read data."""
            self.logger = logging.getLogger('pywws.weather_station')
            # create basic IO object
            self.cusb = CUSBDrive()
            # init variables
            self.status = status
            self.avoid = max(avoid, 0.0)
            self._fixed_block = None
            self._data_block = None
            self._data_pos = None
            self._current_ptr = None
            if params:
                params.unset('fixed', 'station clock')
                params.unset('fixed', 'sensor clock')
            if self.status:
                self._station_clock = eval(
                    self.status.get('clock', 'station', 'None'))
                self._sensor_clock = eval(
                    self.status.get('clock', 'sensor', 'None'))
            else:
                self._station_clock = None
                self._sensor_clock = None
            self.ws_type = ws_type

        def live_data(self, logged_only=False):
            # There are two things we want to synchronise to - the data is
            # updated every 48 seconds and the address is incremented
            # every 5 minutes (or 10, 15, ..., 30). Rather than getting
            # data every second or two, we sleep until one of the above is
            # due. (During initialisation we get data every two seconds
            # anyway.)
            read_period = self.get_fixed_block(['read_period'])
            log_interval = float(read_period * 60)
            live_interval = 48.0
            old_ptr = self.current_pos()
            old_data = self.get_data(old_ptr, unbuffered=True)
            now = time.time()
            if self._sensor_clock:
                next_live = now
                next_live -= (next_live - self._sensor_clock) % live_interval
                next_live += live_interval
            else:
                next_live = None
            if self._station_clock and next_live:
                # set next_log
                next_log = next_live - live_interval
                next_log -= (next_log - self._station_clock) % 60
                next_log -= old_data['delay'] * 60
                next_log += log_interval
            else:
                next_log = None
                self._station_clock = None
            ptr_time = 0
            data_time = 0
            last_log = now - (old_data['delay'] * 60)
            last_status = None
            while True:
                now = time.time()
                # wake up just before next reading is due
                advance = now + max(self.avoid, self.min_pause) + self.min_pause
                pause = 600.0
                if next_live:
                    if not logged_only:
                        pause = min(pause, next_live - advance)
                else:
                    pause = self.min_pause
                if next_log:
                    pause = min(pause, next_log - advance)
                elif old_data['delay'] < read_period - 1:
                    pause = min(
                        pause, ((read_period - old_data['delay']) * 60.0) - 110.0)
                else:
                    pause = self.min_pause
                pause = max(pause, self.min_pause)
                self.logger.debug(
                    'delay %s, pause %g', str(old_data['delay']), pause)
                time.sleep(pause)
                # get new data
                last_data_time = data_time
                new_data = self.get_data(old_ptr, unbuffered=True)
                data_time = time.time()
                # log any change of status
                if new_data['status'] != last_status:
                    self.logger.warning(
                        'status %s', str(decode_status(new_data['status'])))
                last_status = new_data['status']
                # 'good' time stamp if we haven't just woken up from long
                # pause and data read wasn't delayed
                valid_time = data_time - last_data_time < self.margin
                # make sure changes because of logging interval aren't
                # mistaken for new live data
                if new_data['delay'] >= read_period:
                    for key in ('delay', 'hum_in', 'temp_in', 'abs_pressure'):
                        old_data[key] = new_data[key]
                # ignore solar data which changes every 60 seconds
                if self.ws_type == '3080':
                    for key in ('illuminance', 'uv'):
                        old_data[key] = new_data[key]
                if new_data != old_data:
                    self.logger.debug('live_data new data')
                    result = dict(new_data)
                    if valid_time:
                        # data has just changed, so definitely at a 48s update time
                        if self._sensor_clock:
                            diff = (data_time - self._sensor_clock) % live_interval
                            if diff > 2.0 and diff < (live_interval - 2.0):
                                self.logger.error('unexpected sensor clock change')
                                self._sensor_clock = None
                        if not self._sensor_clock:
                            self._sensor_clock = data_time
                            self.logger.warning(
                                'setting sensor clock %g', data_time % live_interval)
                            if self.status:
                                self.status.set(
                                    'clock', 'sensor', str(self._sensor_clock))
                        if not next_live:
                            self.logger.warning('live_data live synchronised')
                        next_live = data_time
                    elif next_live and data_time < next_live - self.margin:
                        self.logger.warning(
                            'live_data lost sync %g', data_time - next_live)
                        next_live = None
                        self._sensor_clock = None
                    if next_live and not logged_only:
                        while data_time > next_live + live_interval:
                            self.logger.info('live_data missed')
                            next_live += live_interval
                        result['idx'] = datetime.utcfromtimestamp(int(next_live))
                        next_live += live_interval
                        yield result, old_ptr, False
                    old_data = new_data
                # get new pointer
                if old_data['delay'] < read_period - 1:
                    continue
                last_ptr_time = ptr_time
                new_ptr = self.current_pos()
                ptr_time = time.time()
                valid_time = ptr_time - last_ptr_time < self.margin
                if new_ptr != old_ptr:
                    self.logger.debug('live_data new ptr: %06x', new_ptr)
                    last_log = ptr_time
                    # re-read data, to be absolutely sure it's the last
                    # logged data before the pointer was updated
                    new_data = self.get_data(old_ptr, unbuffered=True)
                    result = dict(new_data)
                    if valid_time:
                        # pointer has just changed, so definitely at a logging time
                        if self._station_clock:
                            diff = (ptr_time - self._station_clock) % 60
                            if diff > 2 and diff < 58:
                                self.logger.error('unexpected station clock change')
                                self._station_clock = None
                        if not self._station_clock:
                            self._station_clock = ptr_time
                            self.logger.warning(
                                'setting station clock %g', ptr_time % 60.0)
                            if self.status:
                                self.status.set(
                                    'clock', 'station', str(self._station_clock))
                        if not next_log:
                            self.logger.warning('live_data log synchronised')
                        next_log = ptr_time
                    elif next_log and ptr_time < next_log - self.margin:
                        self.logger.warning(
                            'live_data lost log sync %g', ptr_time - next_log)
                        next_log = None
                        self._station_clock = None
                    if next_log:
                        result['idx'] = datetime.utcfromtimestamp(int(next_log))
                        next_log += log_interval
                        yield result, old_ptr, True
                    old_ptr = new_ptr
                    old_data['delay'] = 0
                    data_time = 0
                elif ptr_time > last_log + ((new_data['delay'] + 2) * 60):
                    # if station stops logging data, don't keep reading
                    # USB until it locks up
                    raise IOError('station is not logging data')
                elif valid_time and next_log and ptr_time > next_log + 6.0:
                    self.logger.warning('live_data log extended')
                    next_log += 60.0

        def inc_ptr(self, ptr):
            """Get next circular buffer data pointer."""
            result = ptr + self.reading_len[self.ws_type]
            if result >= 0x10000:
                result = self.data_start
            return result

        def dec_ptr(self, ptr):
            """Get previous circular buffer data pointer."""
            result = ptr - self.reading_len[self.ws_type]
            if result < self.data_start:
                result = 0x10000 - self.reading_len[self.ws_type]
            return result

        def get_raw_data(self, ptr, unbuffered=False):
            """Get raw data from circular buffer.

            If unbuffered is false then a cached value that was obtained
            earlier may be returned."""
            if unbuffered:
                self._data_pos = None
            # round down ptr to a 'block boundary'
            idx = ptr - (ptr % 0x20)
            ptr -= idx
            count = self.reading_len[self.ws_type]
            if self._data_pos == idx:
                # cache contains useful data
                result = self._data_block[ptr:ptr + count]
                if len(result) >= count:
                    return result
            else:
                result = list()
            if ptr + count > 0x20:
                # need part of next block, which may be in cache
                if self._data_pos != idx + 0x20:
                    self._data_pos = idx + 0x20
                    self._data_block = self._read_block(self._data_pos)
                result += self._data_block[0:ptr + count - 0x20]
                if len(result) >= count:
                    return result
            # read current block
            self._data_pos = idx
            self._data_block = self._read_block(self._data_pos)
            result = self._data_block[ptr:ptr + count] + result
            return result

        def get_data(self, ptr, unbuffered=False):
            """Get decoded data from circular buffer.

            If unbuffered is false then a cached value that was obtained
            earlier may be returned."""
            return _decode(self.get_raw_data(ptr, unbuffered),
                           self.reading_format[self.ws_type])

        def current_pos(self):
            """Get circular buffer location where current data is being written."""
            new_ptr = _decode(
                self._read_fixed_block(0x0020), self.lo_fix_format['current_pos'])
            if new_ptr == self._current_ptr:
                return self._current_ptr
            if self._current_ptr and new_ptr != self.inc_ptr(self._current_ptr):
                self.logger.error(
                    'unexpected ptr change %06x -> %06x', self._current_ptr, new_ptr)
                for k in self.reading_len:
                    if (new_ptr - self._current_ptr) == self.reading_len[k]:
                        self.logger.warning('type change %s -> %s', self.ws_type, k)
                        self.ws_type = k
                        break
            self._current_ptr = new_ptr
            return self._current_ptr

        def get_raw_fixed_block(self, unbuffered=False):
            """Get the raw "fixed block" of settings and min/max data."""
            if unbuffered or not self._fixed_block:
                self._fixed_block = self._read_fixed_block()
            return self._fixed_block

        def get_fixed_block(self, keys=[], unbuffered=False):
            """Get the decoded "fixed block" of settings and min/max data.

            A subset of the entire block can be selected by keys."""
            if unbuffered or not self._fixed_block:
                self._fixed_block = self._read_fixed_block()
            format = self.fixed_format
            # navigate down list of keys to get to wanted data
            for key in keys:
                format = format[key]
            return _decode(self._fixed_block, format)

        def _wait_for_station(self):
            # avoid times when station is writing to memory
            while True:
                pause = 60.0
                if self._station_clock:
                    phase = time.time() - self._station_clock
                    if phase > 24 * 3600:
                        # station clock was last measured a day ago, so reset it
                        self._station_clock = None
                    else:
                        pause = min(pause, (self.avoid - phase) % 60)
                if self._sensor_clock:
                    phase = time.time() - self._sensor_clock
                    if phase > 24 * 3600:
                        # sensor clock was last measured a day ago, so reset it
                        self._sensor_clock = None
                    else:
                        pause = min(pause, (self.avoid - phase) % 48)
                if pause >= self.avoid * 2.0:
                    return
                self.logger.debug('avoid %s', str(pause))
                time.sleep(pause)

        def _read_block(self, ptr, retry=True):
            # Read block repeatedly until it's stable. This avoids getting corrupt
            # data when the block is read as the station is updating it.
            old_block = None
            while True:
                self._wait_for_station()
                new_block = self.cusb.read_block(ptr)
                if new_block:
                    if (new_block == old_block) or not retry:
                        break
                    if old_block:
                        self.logger.debug('_read_block changing %06x', ptr)
                    old_block = new_block
            return new_block

        def _read_fixed_block(self, hi=0x0100):
            result = []
            for mempos in range(0x0000, hi, 0x0020):
                result += self._read_block(mempos)
            # check 'magic number'
            if result[:2] not in ([0x55, 0xAA], [0xFF, 0xFF],
                                  [0x55, 0x55], [0xC4, 0x00]):
                self.logger.critical(
                    "Unrecognised 'magic number' %02x %02x", result[0], result[1])
            return result

        def _write_byte(self, ptr, value):
            self._wait_for_station()
            if not self.cusb.write_byte(ptr, value):
                raise IOError('_write_byte failed')

        def write_data(self, data):
            """Write a set of single bytes to the weather station. Data must be an
            array of (ptr, value) pairs."""
            # send data
            for ptr, value in data:
                self._write_byte(ptr, value)
            # set 'data changed'
            self._write_byte(self.fixed_format['data_changed'][0], 0xAA)
            # wait for station to clear 'data changed'
            while True:
                ack = _decode(
                    self._read_fixed_block(0x0020), self.fixed_format['data_changed'])
                if ack == 0:
                    break
                self.logger.debug('write_data waiting for ack')
                time.sleep(6)

        # Tables of "meanings" for raw weather station data. Each key
        # specifies an (offset, type, multiplier) tuple that is understood
        # by _decode.
        # depends on weather station type
        reading_format = {}
        reading_format['1080'] = {
            'delay'        : (0, 'ub', None),
            'hum_in'       : (1, 'ub', None),
            'temp_in'      : (2, 'ss', 0.1),
            'hum_out'      : (4, 'ub', None),
            'temp_out'     : (5, 'ss', 0.1),
            'abs_pressure' : (7, 'us', 0.1),
            'wind_ave'     : (9, 'wa', 0.1),
            'wind_gust'    : (10, 'wg', 0.1),
            'wind_dir'     : (12, 'ub', None),
            'rain'         : (13, 'us', 0.3),
            'status'       : (15, 'pb', None),
            }
        reading_format['3080'] = {
            'illuminance' : (16, 'u3', 0.1),
            'uv'          : (19, 'ub', None),
            }
        reading_format['3080'].update(reading_format['1080'])
        lo_fix_format = {
            'read_period'   : (16, 'ub', None),
            'settings_1'    : (17, 'bf', ('temp_in_F', 'temp_out_F', 'rain_in',
                                          'bit3', 'bit4', 'pressure_hPa',
                                          'pressure_inHg', 'pressure_mmHg')),
            'settings_2'    : (18, 'bf', ('wind_mps', 'wind_kmph', 'wind_knot',
                                          'wind_mph', 'wind_bft', 'bit5',
                                          'bit6', 'bit7')),
            'display_1'     : (19, 'bf', ('pressure_rel', 'wind_gust', 'clock_12hr',
                                          'date_mdy', 'time_scale_24', 'show_year',
                                          'show_day_name', 'alarm_time')),
            'display_2'     : (20, 'bf', ('temp_out_temp', 'temp_out_chill',
                                          'temp_out_dew', 'rain_hour', 'rain_day',
                                          'rain_week', 'rain_month', 'rain_total')),
            'alarm_1'       : (21, 'bf', ('bit0', 'time', 'wind_dir', 'bit3',
                                          'hum_in_lo', 'hum_in_hi',
                                          'hum_out_lo', 'hum_out_hi')),
            'alarm_2'       : (22, 'bf', ('wind_ave', 'wind_gust',
                                          'rain_hour', 'rain_day',
                                          'pressure_abs_lo', 'pressure_abs_hi',
                                          'pressure_rel_lo', 'pressure_rel_hi')),
            'alarm_3'       : (23, 'bf', ('temp_in_lo', 'temp_in_hi',
                                          'temp_out_lo', 'temp_out_hi',
                                          'wind_chill_lo', 'wind_chill_hi',
                                          'dew_point_lo', 'dew_point_hi')),
            'timezone'      : (24, 'sb', None),
            'unknown_01'    : (25, 'pb', None),
            'data_changed'  : (26, 'ub', None),
            'data_count'    : (27, 'us', None),
            'display_3'     : (29, 'bf', ('illuminance_fc', 'bit1', 'bit2', 'bit3',
                                          'bit4', 'bit5', 'bit6', 'bit7')),
            'current_pos'   : (30, 'us', None),
            }
        fixed_format = {
            'rel_pressure'  : (32, 'us', 0.1),
            'abs_pressure'  : (34, 'us', 0.1),
            'lux_wm2_coeff' : (36, 'us', 0.1),
            'date_time'     : (43, 'dt', None),
            'unknown_18'    : (97, 'pb', None),
            'alarm'         : {
                'hum_in'        : {'hi' : (48, 'ub', None), 'lo'  : (49, 'ub', None)},
                'temp_in'       : {'hi' : (50, 'ss', 0.1), 'lo'  : (52, 'ss', 0.1)},
                'hum_out'       : {'hi' : (54, 'ub', None), 'lo'  : (55, 'ub', None)},
                'temp_out'      : {'hi' : (56, 'ss', 0.1), 'lo'  : (58, 'ss', 0.1)},
                'windchill'     : {'hi' : (60, 'ss', 0.1), 'lo'  : (62, 'ss', 0.1)},
                'dewpoint'      : {'hi' : (64, 'ss', 0.1), 'lo'  : (66, 'ss', 0.1)},
                'abs_pressure'  : {'hi' : (68, 'us', 0.1), 'lo'  : (70, 'us', 0.1)},
                'rel_pressure'  : {'hi' : (72, 'us', 0.1), 'lo'  : (74, 'us', 0.1)},
                'wind_ave'      : {'bft' : (76, 'ub', None), 'ms' : (77, 'ub', 0.1)},
                'wind_gust'     : {'bft' : (79, 'ub', None), 'ms' : (80, 'ub', 0.1)},
                'wind_dir'      : (82, 'ub', None),
                'rain'          : {'hour' : (83, 'us', 0.3), 'day'   : (85, 'us', 0.3)},
                'time'          : (87, 'tt', None),
                'illuminance'   : (89, 'u3', 0.1),
                'uv'            : (92, 'ub', None),
                },
            'max'           : {
                'uv'            : {'val' : (93, 'ub', None)},
                'illuminance'   : {'val' : (94, 'u3', 0.1)},
                'hum_in'        : {'val' : (98, 'ub', None), 'date'   : (141, 'dt', None)},
                'hum_out'       : {'val' : (100, 'ub', None), 'date'  : (151, 'dt', None)},
                'temp_in'       : {'val' : (102, 'ss', 0.1), 'date'  : (161, 'dt', None)},
                'temp_out'      : {'val' : (106, 'ss', 0.1), 'date'  : (171, 'dt', None)},
                'windchill'     : {'val' : (110, 'ss', 0.1), 'date'  : (181, 'dt', None)},
                'dewpoint'      : {'val' : (114, 'ss', 0.1), 'date'  : (191, 'dt', None)},
                'abs_pressure'  : {'val' : (118, 'us', 0.1), 'date'  : (201, 'dt', None)},
                'rel_pressure'  : {'val' : (122, 'us', 0.1), 'date'  : (211, 'dt', None)},
                'wind_ave'      : {'val' : (126, 'us', 0.1), 'date'  : (221, 'dt', None)},
                'wind_gust'     : {'val' : (128, 'us', 0.1), 'date'  : (226, 'dt', None)},
                'rain'          : {
                    'hour'          : {'val' : (130, 'us', 0.3), 'date'  : (231, 'dt', None)},
                    'day'           : {'val' : (132, 'us', 0.3), 'date'  : (236, 'dt', None)},
                    'week'          : {'val' : (134, 'us', 0.3), 'date'  : (241, 'dt', None)},
                    'month'         : {'val' : (136, 'us', 0.3), 'date'  : (246, 'dt', None)},
                    'total'         : {'val' : (138, 'us', 0.3), 'date'  : (251, 'dt', None)},
                    },
                },
            'min'           : {
                'hum_in'        : {'val' : (99, 'ub', None), 'date'   : (146, 'dt', None)},
                'hum_out'       : {'val' : (101, 'ub', None), 'date'  : (156, 'dt', None)},
                'temp_in'       : {'val' : (104, 'ss', 0.1), 'date'  : (166, 'dt', None)},
                'temp_out'      : {'val' : (108, 'ss', 0.1), 'date'  : (176, 'dt', None)},
                'windchill'     : {'val' : (112, 'ss', 0.1), 'date'  : (186, 'dt', None)},
                'dewpoint'      : {'val' : (116, 'ss', 0.1), 'date'  : (196, 'dt', None)},
                'abs_pressure'  : {'val' : (120, 'us', 0.1), 'date'  : (206, 'dt', None)},
                'rel_pressure'  : {'val' : (124, 'us', 0.1), 'date'  : (216, 'dt', None)},
                },
            }
        fixed_format.update(lo_fix_format)
        # start of readings / end of fixed block
        data_start = 0x0100     # 256
        # bytes per reading, depends on weather station type
        reading_len = {
            '1080'  : 16,
            '3080'  : 20,
            }

### Navigation

- index
- modules |
- pywws 14.03.dev1177 documentation »
- Module code »