### Navigation

- index
- modules |
- pywws 13.09_r1069 documentation »
- Code du module »

# Code source de pywws.TestWeatherStation

    #!/usr/bin/env python

    # pywws - Python software for USB Wireless Weather Stations
    # http://github.com/jim-easterbrook/pywws
    # Copyright (C) 2008-13  Jim Easterbrook  jim@jim-easterbrook.me.uk

    # This program is free software; you can redistribute it and/or
    # modify it under the terms of the GNU General Public License
    # as published by the Free Software Foundation; either version 2
    # of the License, or (at your option) any later version.

    # This program is distributed in the hope that it will be useful,
    # but WITHOUT ANY WARRANTY; without even the implied warranty of
    # MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    # GNU General Public License for more details.

    # You should have received a copy of the GNU General Public License
    # along with this program; if not, write to the Free Software
    # Foundation, Inc., 51 Franklin Street, Fifth Floor, Boston, MA  02110-1301, USA.

    """Test connection to weather station.

    This is a simple utility to test communication with the weather
    station. If this doesn't work, then there's a problem that needs to be
    sorted out before trying any of the other programs. Likely problems
    include not properly installing the USB libraries, or a permissions
    problem. The most unlikely problem is that you forgot to connect the
    weather station to your computer! ::

    %s
    """

    __usage__ = """
     usage: python -m pywws.TestWeatherStation [options]
     options are:
           --help           display this help
      -c | --change         display any changes in "fixed block" data
      -d | --decode         display meaningful values instead of raw data
      -h | --history count  display the last "count" readings
      -l | --live           display 'live' data
      -m | --logged         display 'logged' data
      -u | --unknown        display unknown fixed block values
      -v | --verbose        increase amount of reassuring messages
                            (repeat for even more messages e.g. -vvv)
    """

    __doc__ %= __usage__

    __usage__ = __doc__.split('\n')[0] + __usage__

    import datetime
    import getopt
    import sys
    import time

    from pywws.Logger import ApplicationLogger
    from pywws import WeatherStation

    def raw_dump(pos, data):
        print "%04x" % pos,
        for item in data:
            print "%02x" % item,
        print
    def main(argv=None):
        if argv is None:
            argv = sys.argv
        try:
            opts, args = getopt.getopt(
                argv[1:], "cdh:lmuv",
                ('help', 'change', 'decode', 'history=', 'live', 'logged',
                 'unknown', 'verbose'))
        except getopt.error, msg:
            print >>sys.stderr, 'Error: %s\n' % msg
            print >>sys.stderr, __usage__.strip()
            return 1
        # check arguments
        if len(args) != 0:
            print >>sys.stderr, 'Error: no arguments allowed\n'
            print >>sys.stderr, __usage__.strip()
            return 2
        # process options
        change = False
        history_count = 0
        decode = False
        live = False
        logged = False
        unknown = False
        verbose = 0
        for o, a in opts:
            if o == '--help':
                print __usage__.strip()
                return 0
            elif o in ('-c', '--change'):
                change = True
            elif o in ('-d', '--decode'):
                decode = True
            elif o in ('-h', '--history'):
                history_count = int(a)
            elif o in ('-l', '--live'):
                live = True
                logged = False
            elif o in ('-m', '--logged'):
                live = False
                logged = True
            elif o in ('-u', '--unknown'):
                unknown = True
            elif o in ('-v', '--verbose'):
                verbose += 1
        # do it!
        logger = ApplicationLogger(verbose)
        ws = WeatherStation.weather_station()
        raw_fixed = ws.get_raw_fixed_block()
        if not raw_fixed:
            print "No valid data block found"
            return 3
        if decode:
            # dump entire fixed block
            print ws.get_fixed_block()
            # dump a few selected items
            print "min -> temp_out ->", ws.get_fixed_block(['min', 'temp_out'])
            print "alarm -> hum_out ->", ws.get_fixed_block(['alarm', 'hum_out'])
            print "rel_pressure ->", ws.get_fixed_block(['rel_pressure'])
            print "abs_pressure ->", ws.get_fixed_block(['abs_pressure'])
        else:
            for ptr in range(0x0000, 0x0100, 0x20):
                raw_dump(ptr, raw_fixed[ptr:ptr+0x20])
        if unknown:
            for k in sorted(ws.fixed_format):
                if 'unk' in k:
                    print k, ws.get_fixed_block([k])
            for k in sorted(ws.fixed_format):
                if 'settings' in k or 'display' in k or 'alarm' in k:
                    bits = ws.get_fixed_block([k])
                    for b in sorted(bits):
                        if 'bit' in b:
                            print k, b, bits[b]
        if history_count > 0:
            fixed_block = ws.get_fixed_block()
            print "Recent history"
            ptr = fixed_block['current_pos']
            date = datetime.datetime.now().replace(second=0, microsecond=0)
            for i in range(history_count):
                if decode:
                    data = ws.get_data(ptr)
                    print date, data
                    date = date - datetime.timedelta(minutes=data['delay'])
                else:
                    raw_dump(ptr, ws.get_raw_data(ptr))
                ptr = ws.dec_ptr(ptr)
        if change:
            while True:
                new_fixed = ws.get_raw_fixed_block(unbuffered=True)
                for ptr in range(len(new_fixed)):
                    if new_fixed[ptr] != raw_fixed[ptr]:
                        print datetime.datetime.now().strftime('%H:%M:%S'),
                        print ' %04x (%d)  %02x -> %02x' % (
                            ptr, ptr, raw_fixed[ptr], new_fixed[ptr])
                raw_fixed = new_fixed
                time.sleep(0.5)
        if live:
            for data, ptr, logged in ws.live_data():
                print "%04x" % ptr,
                print data['idx'].strftime('%H:%M:%S'),
                del data['idx']
                print data
        if logged:
            for data, ptr, logged in ws.live_data(logged_only=True):
                print "%04x" % ptr,
                print data['idx'].strftime('%H:%M:%S'),
                del data['idx']
                print data
        del ws
        return 0
    if __name__ == "__main__":
        try:
            sys.exit(main())
        except KeyboardInterrupt:
            pass

### Navigation

- index
- modules |
- pywws 13.09_r1069 documentation »
- Code du module »