### Navigation

- index
- modules |
- next |
- previous |
- pywws 14.03.dev1177 documentation »
- Python programs and modules »

# pywws.Tasks

Routines to perform common tasks such as plotting gaphs or uploading files.

Classes

`Calib`(params, stored_data) | Calibration class that implements default or user calibration.
`RegularTasks`(params, status, raw_data, ...) |
`ToService`(params, status, calib_data, ...) | Upload weather data to weather services such as Weather
`datetime` | datetime(year, month, day[, hour[, minute[, second[, microsecond[,tzinfo]]]]])
`deque` | deque([iterable[, maxlen]]) –> deque object
`timedelta` | Difference between two datetime values.

class `pywws.Tasks.``RegularTasks`(params, status, raw_data, calib_data, hourly_data, daily_data, monthly_data, asynch=False)
  `stop_thread`()
  `has_live_tasks`()
  `do_live`(data)
  `do_tasks`()
  `do_twitter`(template, data=None)
  `do_plot`(template)
  `do_template`(template, data=None)

### Navigation

- index
- modules |
- next |
- previous |
- pywws 14.03.dev1177 documentation »
- Python programs and modules »