1

2# -*- coding: utf-8 -*-

3

4 u'''Military Grid Reference System (MGRS/NATO) references.

5

6 Classes L{Mgrs}, L{Mgrs4Tuple} and L{Mgrs6Tuple} and functions L{parseMGRS}

7 and L{toMgrs}.

8

9 Pure Python implementation of MGRS, UTM and UPS conversions covering the entire

10 I{ellipsoidal} earth, transcoded from I{Chris Veness}' JavaScript originals U{MGRS

11<https://www.Movable-Type.co.UK/scripts/latlong-utm-mgrs.html>} and U{Module mgrs

12<https://www.Movable-Type.co.UK/scripts/geodesy/docs/module-mgrs.html>} and from

13 I{Charles Karney}'s C++ class U{MGRS<https://GeographicLib.SourceForge.io/C++/doc/

14 classGeographicLib_1_1MGRS.html>}.

15

16 MGRS references comprise a grid zone designation (GZD), a 100 km grid (square)

17 tile identification and an easting and northing (in C{meter}). The GZD consists

18 of a longitudinal zone (or column) I{number} and latitudinal band (row) I{letter}

19 in the UTM region between 80°S and 84°N. Each zone (column) is 6° wide and each

20 band (row) is 8° high, except top band 'X' is 12° tall. In UPS polar regions

21 below 80°S and above 84°N the GZD contains only a single I{letter}, C{'A'} or

22 C{'B'} near the south and C{'Y'} or C{'Z'} around the north pole (for west

23 respectively east longitudes).

24

25 See also the U{United States National Grid<https://www.FGDC.gov/standards/projects/

26 FGDC-standards-projects/usng/fgdc_std_011_2001_usng.pdf>} and U{Military Grid

27 Reference System<https://WikiPedia.org/wiki/Military_grid_reference_system>}.

28

29 See module L{pygeodesy.ups} for env variable C{PYGEODESY_UPS_POLES} determining

30 the UPS encoding I{at} the south and north pole.

31

32 Set env variable C{PYGEODESY_GEOCONVERT} to the (fully qualified) path of the

33 C{GeoConvert} executable to run this module as I{python[3] -m pygeodesy.mgrs}

34 and compare the MGRS results with those from I{Karney}'s utility U{GeoConvert

35<https://GeographicLib.sourceforge.io/C++/doc/GeoConvert.1.html>}.

36'''

37

38 from pygeodesy.basics import halfs2, _xinstanceof

39# from pygeodesy.constants import _0_5 # from .units

40 from pygeodesy.datums import _ellipsoidal_datum, _WGS84

41 from pygeodesy.errors import _AssertionError, MGRSError, _parseX, \

42 _ValueError, _xkwds, _ALL_LAZY, _MODS

43 from pygeodesy.interns import NN, _0_, _A_, _AtoZnoIO_, _band_, _B_, \

44 _COMMASPACE_, _datum_, _easting_, _invalid_, \

45 _northing_, _not_, _SPACE_, _splituple, _W_, \

46 _Y_, _Z_, _zone_

47# from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS # from .errors

48 from pygeodesy.named import _NamedBase, _NamedTuple, _Pass, _xnamed

49 from pygeodesy.namedTuples import EasNor2Tuple, UtmUps5Tuple

50 from pygeodesy.props import deprecated_property_RO, property_RO, Property_RO

51 from pygeodesy.streprs import enstr2, _enstr2m3, Fmt, _resolution10, _xzipairs

52 from pygeodesy.units import Easting, Northing, Str, _100km, _0_5

53 from pygeodesy.units import _1um, _2000km # PYCHOK used!

54 from pygeodesy.ups import _hemi, toUps8, Ups, _UPS_ZONE

55 from pygeodesy.utm import toUtm8, _to3zBlat, Utm, _UTM_ZONE_MAX, _UTM_ZONE_MIN

56# from pygeodesy.utmupsBase import _UTM_ZONE_MAX, _UTM_ZONE_MIN # from .utm

57

58__all__ = _ALL_LAZY.mgrs

59__version__ = '23.03.19'

60

61_AN_ = 'AN' # default south pole grid tile and band B

62_AtoPx_ = _AtoZnoIO_.tillP

63# <https://GitHub.com/hrbrmstr/mgrs/blob/master/src/mgrs.c>

64_FeUPS = {_A_: 8, _B_: 20, _Y_: 8, _Z_: 20} # falsed offsets (C{_100kms})

65_FnUPS = {_A_: 8, _B_: 8, _Y_: 13, _Z_: 13} # falsed offsets (C{_100kms})

66_JtoZx_ = 'JKLPQRSTUXYZZ' # _AtoZnoDEIMNOVW.fromJ, duplicate Z

67# 100 km grid tile UTM column (E) letters, repeating every third zone

68_LeUTM = _AtoZnoIO_.tillH, _AtoZnoIO_.fromJ.tillR, _AtoZnoIO_.fromS # grid E colums

69# 100 km grid tile UPS column (E) letters for each polar zone

70_LeUPS = {_A_: _JtoZx_, _B_: 'ABCFGHJKLPQR', _Y_: _JtoZx_, _Z_: 'ABCFGHJ'}

71# 100 km grid tile UTM and UPS row (N) letters, repeating every other zone

72_LnUTM = _AtoZnoIO_.tillV, _AtoZnoIO_.fromF.tillV + _AtoZnoIO_.tillE # grid N rows

73_LnUPS = {_A_: _AtoZnoIO_, _B_: _AtoZnoIO_, _Y_: _AtoPx_, _Z_: _AtoPx_}

74_polar_ = _SPACE_('polar', _zone_)

75

76

77 class Mgrs(_NamedBase):

78 '''Military Grid Reference System (MGRS/NATO) references,

79 with method to convert to UTM coordinates.

80 '''

81 _band = NN # latitudinal (C..X) or polar (ABYZ) band

82 _bandLat = None # band latitude (C{degrees90} or C{None})

83 _datum = _WGS84 # Datum (L{Datum})

84 _easting = 0 # Easting (C{meter}), within 100 km grid tile

85 _EN = NN # EN digraph (C{str}), 100 km grid tile

86 _northing = 0 # Northing (C{meter}), within 100 km grid tile

87 _resolution = 0 # from L{parseMGRS}, centering (C{meter})

88 _zone = 0 # longitudinal or polar zone (C{int}), 0..60

89

90 def __init__(self, zone=0, EN=NN, easting=0, northing=0, band=NN,

91 datum=_WGS84, resolution=0, name=NN):

92 '''New L{Mgrs} Military grid reference.

93

94 @arg zone: The 6° I{longitudinal} zone (C{int}), 1..60 covering

95 180°W..180°E or C{0} for I{polar} regions or (C{str})

96 with the zone number and I{latitudinal} band letter.

97 @arg EN: Two-letter EN digraph (C{str}), grid tile I{using only}

98 the I{AA} aka I{MGRS-New} (row) U{lettering scheme

99 <http://Wikipedia.org/wiki/Military_Grid_Reference_System>}.

100 @kwarg easting: Easting (C{meter}), within 100 km grid tile.

101 @kwarg northing: Northing (C{meter}), within 100 km grid tile.

102 @kwarg band: Optional, I{latitudinal} band or I{polar} region letter

103 (C{str}), 'C'|..|'X' covering 80°S..84°N (no 'I'|'O'),

104 'A'|'B' at the south or 'Y'|'Z' at the north pole.

105 @kwarg datum: This reference's datum (L{Datum}, L{Ellipsoid},

106 L{Ellipsoid2} or L{a_f2Tuple}).

107 @kwarg resolution: Optional resolution (C{meter}), C{0} for default.

108 @kwarg name: Optional name (C{str}).

109

110 @raise MGRSError: Invalid B{C{zone}}, B{C{EN}}, B{C{easting}},

111 B{C{northing}}, B{C{band}} or B{C{resolution}}.

112

113 @raise TypeError: Invalid B{C{datum}}.

114

115 @example:

116

117 >>> from pygeodesy import Mgrs

118 >>> m = Mgrs('31U', 'DQ', 48251, 11932) # 31U DQ 48251 11932

119 >>> m = Mgrs() # defaults to south pole

120 >>> m.toLatLon() # ... lat=-90.0, lon=0.0, datum=...

121 '''

122 if name:

123 self.name = name

124

125 if not (zone or EN or band):

126 EN, band = _AN_, _B_ # default, south pole

127 try:

128 self._zone, self._band, self._bandLat = _to3zBlat(zone, band, Error=MGRSError)

129 en = str(EN)

130 if len(en) != 2 or not en.isalpha():

131 raise ValueError # caught below

132 self._EN = en.upper()

133 _ = self._EN2m # check E and N

134 except (IndexError, KeyError, TypeError, ValueError):

135 raise MGRSError(band=band, EN=EN, zone=zone)

136

137 self._easting = Easting(easting, Error=MGRSError)

138 self._northing = Northing(northing, Error=MGRSError)

139 if datum not in (None, Mgrs._datum):

140 self._datum = _ellipsoidal_datum(datum, name=name) # XXX raiser=_datum_

141

142 if resolution:

143 self.resolution = resolution

144

145 def __str__(self):

146 return self.toStr(sep=_SPACE_) # for backward compatibility

147

148 @property_RO

149 def band(self):

150 '''Get the I{latitudinal} band C{'C'|..|'X'} (no C{'I'|'O'})

151 or I{polar} region C{'A'|'B'|'Y'|'Z'}) letter (C{str}).

152 '''

153 return self._band

154

155 @Property_RO

156 def bandLatitude(self):

157 '''Get the band latitude (C{degrees90}).

158 '''

159 return self._bandLat

160

161 @Property_RO

162 def datum(self):

163 '''Get the datum (L{Datum}).

164 '''

165 return self._datum

166

167 @deprecated_property_RO

168 def digraph(self):

169 '''DEPRECATED, use property C{EN}.'''

170 return self.EN

171

172 @property_RO

173 def EN(self):

174 '''Get the 2-letter grid tile (C{str}).

175 '''

176 return self._EN

177

178 @deprecated_property_RO

179 def en100k(self):

180 '''DEPRECATED, use property C{EN}.'''

181 return self.EN

182

183 @Property_RO

184 def _EN2m(self):

185 '''(INTERNAL) Get the grid 2-tuple (easting, northing) in C{meter}.

186

187 @note: Raises AssertionError, IndexError or KeyError: Invalid

188 C{zone} number, C{EN} letter or I{polar} region letter.

189 '''

190 EN = self.EN

191 if self.isUTM:

192 i = self.zone - 1

193 # get easting from the E column (note, +1 because

194 # easting starts at 166e3 due to 500 km falsing)

195 e = _LeUTM[i % 3].index(EN[0]) + 1

196 # similarly, get northing from the N row

197 n = _LnUTM[i % 2].index(EN[1])

198 elif self.isUPS:

199 B = self.band

200 e = _LeUPS[B].index(EN[0]) + _FeUPS[B]

201 n = _LnUPS[B].index(EN[1]) + _FnUPS[B]

202 else:

203 raise _AssertionError(zone=self.zone)

204 return float(e * _100km), float(n * _100km) # meter

205

206 @property_RO

207 def easting(self):

208 '''Get the easting (C{meter} within grid tile).

209 '''

210 return self._easting

211

212 @Property_RO

213 def eastingnorthing(self):

214 '''Get easting and northing (L{EasNor2Tuple}C{(easting, northing)})

215 I{within} the MGRS grid tile, both in C{meter}.

216 '''

217 return EasNor2Tuple(self.easting, self.northing)

218

219 @Property_RO

220 def isUPS(self):

221 '''Is this MGRS in a (polar) UPS zone (C{bool}).

222 '''

223 return self._zone == _UPS_ZONE

224

225 @Property_RO

226 def isUTM(self):

227 '''Is this MGRS in a (non-polar) UTM zone (C{bool}).

228 '''

229 return _UTM_ZONE_MIN <= self._zone <= _UTM_ZONE_MAX

230

231 @property_RO

232 def northing(self):

233 '''Get the northing (C{meter} within grid tile).

234 '''

235 return self._northing

236

237 @Property_RO

238 def northingBottom(self):

239 '''Get the northing of the band bottom (C{meter}).

240 '''

241 a = self.bandLatitude

242 u = toUtm8(a, 0, datum=self.datum, Utm=None) if self.isUTM else \

243 toUps8(a, 0, datum=self.datum, Ups=None)

244 return int(u.northing / _100km) * _100km

245

246 def parse(self, strMGRS, name=NN):

247 '''Parse a string to a similar L{Mgrs} instance.

248

249 @arg strMGRS: The MGRS reference (C{str}),

250 see function L{parseMGRS}.

251 @kwarg name: Optional instance name (C{str}),

252 overriding this name.

253

254 @return: The similar instance (L{Mgrs}).

255

256 @raise MGRSError: Invalid B{C{strMGRS}}.

257 '''

258 return parseMGRS(strMGRS, datum=self.datum, Mgrs=self.classof,

259 name=name or self.name)

260

261 @property

262 def resolution(self):

263 '''Get the MGRS resolution (C{meter}, power of 10)

264 or C{0} if undefined.

265 '''

266 return self._resolution

267

268 @resolution.setter # PYCHOK setter!

269 def resolution(self, resolution):

270 '''Set the MGRS resolution (C{meter}, power of 10)

271 or C{0} to undefine and disable UPS/UTM centering.

272

273 @raise MGRSError: Invalid B{C{resolution}}, over

274 C{1.e+5} or under C{1.e-6}.

275 '''

276 if resolution: # and resolution > 0

277 r = _resolution10(resolution, Error=MGRSError)

278 else:

279 r = 0

280 if self._resolution != r:

281 self._resolution = r

282

283 @Property_RO

284 def tilesize(self):

285 '''Get the MGRS grid tile size (C{meter}).

286 '''

287 assert _MODS.utmups._MGRS_TILE is _100km

288 return _100km

289

290 def toLatLon(self, LatLon=None, center=True, **toLatLon_kwds):

291 '''Convert this MGRS grid reference to a UTM coordinate.

292

293 @kwarg LatLon: Optional, ellipsoidal class to return the

294 geodetic point (C{LatLon}) or C{None}.

295 @kwarg center: Optionally, return the grid's center or

296 lower left corner (C{bool}).

297 @kwarg toLatLon_kwds: Optional, additional L{Utm.toLatLon}

298 and B{C{LatLon}} keyword arguments.

299

300 @return: A B{C{LatLon}} instance or if C{B{LatLon} is None}

301 a L{LatLonDatum5Tuple}C{(lat, lon, datum, gamma,

302 scale)}.

303

304 @raise TypeError: If B{C{LatLon}} is not ellipsoidal.

305

306 @raise UTMError: Invalid meridional radius or H-value.

307

308 @see: Methods L{Mgrs.toUtm} and L{Utm.toLatLon}.

309 '''

310 u = self.toUtmUps(center=center)

311 return u.toLatLon(LatLon=LatLon, **toLatLon_kwds)

312

313 def toRepr(self, fmt=Fmt.SQUARE, sep=_COMMASPACE_, **prec): # PYCHOK expected

314 '''Return a string representation of this MGRS grid reference.

315

316 @kwarg fmt: Enclosing backets format (C{str}).

317 @kwarg sep: Separator between name:values (C{str}).

318 @kwarg prec: Precision (C{int}), see method L{Mgrs.toStr}.

319

320 @return: This Mgrs as "[Z:[dd]B, G:EN, E:easting, N:northing]"

321 (C{str}), with C{B{sep} ", "}.

322

323 @note: MGRS grid references are truncated, not rounded (unlike

324 UTM/UPS coordinates).

325

326 @raise ValueError: Invalid B{C{prec}}.

327 '''

328 t = self.toStr(sep=None, **prec)

329 return _xzipairs('ZGEN', t, sep=sep, fmt=fmt)

330

331 def toStr(self, prec=0, sep=NN): # PYCHOK expected

332 '''Return this MGRS grid reference as a string.

333

334 @kwarg prec: Precision, the number of I{decimal} digits (C{int}) or if

335 negative, the number of I{units to drop}, like MGRS U{PRECISION

336 <https://GeographicLib.SourceForge.io/C++/doc/GeoConvert.1.html#PRECISION>}.

337 @kwarg sep: Optional separator to join (C{str}) or C{None} to return an unjoined

338 3-C{tuple} of C{str}s.

339

340 @return: This Mgrs as 4-tuple C{("dd]B", "EN", "easting", "northing")} if C{B{sep}=NN}

341 or "[dd]B EN easting northing" (C{str}) with C{B{sep} " "}.

342

343 @note: Both C{easting} and C{northing} strings are C{NN} or missing if C{B{prec} <= -5}.

344

345 @note: MGRS grid references are truncated, not rounded (unlike UTM/UPS).

346

347 @raise ValueError: Invalid B{C{prec}}.

348

349 @example:

350

351 >>> from pygeodesy import Mgrs, NN, parseMGRS

352 >>> m = Mgrs(31, 'DQ', 48251, 11932, band='U')

353 >>> m.toStr() # '31U DQ 48251 11932'

354 >>> m = parseMGRS('BAN1234567890')

355 >>> str(m) # 'B AN 12345 67890'

356 >>> m.toStr() # 'BAN1234567890'

357 >>> m.toStr(prec=-2) # 'BAN123678'

358 '''

359 zB = self.zoneB

360 t = enstr2(self._easting, self._northing, prec, zB, self.EN)

361 return t if sep is None else sep.join(t).rstrip()

362

363 def toUps(self, Ups=Ups, center=False):

364 '''Convert this MGRS grid reference to a UPS coordinate.

365

366 @kwarg Ups: Optional class to return the UPS coordinate

367 (L{Ups}) or C{None}.

368 @kwarg center: Optionally, center easting and northing

369 by the resolution (C{bool}).

370

371 @return: A B{C{Ups}} instance or if C{B{Ups} is None}

372 a L{UtmUps5Tuple}C{(zone, hemipole, easting,

373 northing, band)}.

374

375 @raise MGRSError: This MGRS is a I{non-polar} UTM reference.

376 '''

377 if self.isUTM:

378 raise MGRSError(zoneB=self.zoneB, txt=_not_(_polar_))

379 return self._toUtmUps(Ups, center)

380

381 def toUtm(self, Utm=Utm, center=False):

382 '''Convert this MGRS grid reference to a UTM coordinate.

383

384 @kwarg Utm: Optional class to return the UTM coordinate

385 (L{Utm}) or C{None}.

386 @kwarg center: Optionally, center easting and northing

387 by the resolution (C{bool}).

388

389 @return: A B{C{Utm}} instance or if C{B{Utm} is None}

390 a L{UtmUps5Tuple}C{(zone, hemipole, easting,

391 northing, band)}.

392

393 @raise MGRSError: This MGRS is a I{polar} UPS reference.

394 '''

395 if self.isUPS:

396 raise MGRSError(zoneB=self.zoneB, txt=_polar_)

397 return self._toUtmUps(Utm, center)

398

399 def toUtmUps(self, Utm=Utm, Ups=Ups, center=False):

400 '''Convert this MGRS grid reference to a UTM or UPS coordinate.

401

402 @kwarg Utm: Optional class to return the UTM coordinate

403 (L{Utm}) or C{None}.

404 @kwarg Ups: Optional class to return the UPS coordinate

405 (L{Utm}) or C{None}.

406 @kwarg center: Optionally, center easting and northing

407 by the resolution (C{bool}).

408

409 @return: A B{C{Utm}} or B{C{Ups}} instance or if C{B{Utm}

410 or B{Ups} is None} a L{UtmUps5Tuple}C{(zone,

411 hemipole, easting, northing, band)}.

412 '''

413 return self._toUtmUps((Utm if self.isUTM else

414 (Ups if self.isUPS else None)), center)

415

416 def _toUtmUps(self, U, center):

417 '''(INTERNAL) Helper for C{.toUps} and C{.toUtm}.

418 '''

419 e, n = self._EN2m

420 e += self.easting

421 n += self.northing

422 if self.isUTM:

423 # 100 km row letters repeat every 2,000 km north;

424 # add 2,000 km blocks to get into required band

425 b = (self.northingBottom - n) / _2000km

426 if b > 0:

427 b = int(b) + 1

428 b = min(b, (3 if self.band == _W_ else 4))

429 n += b * _2000km

430 if center:

431 c = self.resolution

432 if c:

433 c *= _0_5

434 e += c

435 n += c

436 z = self.zone

437 h = _hemi(self.bandLatitude) # _S_ if self.band < _N_ else _N_

438 B = self.band

439 m = self.name

440 return UtmUps5Tuple(z, h, e, n, B, name=m, Error=MGRSError) if U is None \

441 else U(z, h, e, n, B, name=m, datum=self.datum)

442

443 @property_RO

444 def zone(self):

445 '''Get the I{longitudinal} zone (C{int}), 1..60 or 0 for I{polar}.

446 '''

447 return self._zone

448

449 @Property_RO

450 def zoneB(self):

451 '''Get the I{polar} region letter or the I{longitudinal} zone digits

452 plus I{latitudinal} band letter (C{str}).

453 '''

454 return self.band if self.isUPS else NN(Fmt.zone(self.zone), self.band)

455

456

457 class Mgrs4Tuple(_NamedTuple):

458 '''4-Tuple C{(zone, EN, easting, northing)}, C{zone} and grid

459 tile C{EN} as C{str}, C{easting} and C{northing} in C{meter}.

460

461 @note: The C{zone} consists of either the I{longitudinal} zone

462 number plus the I{latitudinal} band letter or only the

463 I{polar} region letter.

464 '''

465 _Names_ = (_zone_, 'EN', _easting_, _northing_)

466 _Units_ = ( Str, Str, Easting, Northing)

467

468 @deprecated_property_RO

469 def digraph(self):

470 '''DEPRECATED, use attribute C{EN}.'''

471 return self.EN # PYCHOK or [1]

472

473 def toMgrs(self, **Mgrs_and_kwds):

474 '''Return this L{Mgrs4Tuple} as an L{Mgrs} instance.

475 '''

476 return self.to6Tuple(NN, _WGS84).toMgrs(**Mgrs_and_kwds)

477

478 def to6Tuple(self, band=NN, datum=_WGS84):

479 '''Extend this L{Mgrs4Tuple} to a L{Mgrs6Tuple}.

480

481 @kwarg band: The band (C{str}).

482 @kwarg datum: The datum (L{Datum}).

483

484 @return: An L{Mgrs6Tuple}C{(zone, EN, easting,

485 northing, band, datum)}.

486 '''

487 z = self.zone # PYCHOK or [0]

488 B = z[-1:]

489 if B.isalpha():

490 z = z[:-1] or Fmt.zone(0)

491 t = Mgrs6Tuple(z, self.EN, self.easting, self.northing, # PYCHOK attrs

492 band or B, datum, name=self.name)

493 else:

494 t = self._xtend(Mgrs6Tuple, band, datum)

495 return t

496

497

498 class Mgrs6Tuple(_NamedTuple): # XXX only used above

499 '''6-Tuple C{(zone, EN, easting, northing, band, datum)}, with

500 C{zone}, grid tile C{EN} and C{band} as C{str}, C{easting}

501 and C{northing} in C{meter} and C{datum} a L{Datum}.

502

503 @note: The C{zone} is the I{longitudinal} zone C{"01".."60"}

504 or C{"00"} for I{polar} regions and C{band} is the

505 I{latitudinal} band or I{polar} region letter.

506 '''

507 _Names_ = Mgrs4Tuple._Names_ + (_band_, _datum_)

508 _Units_ = Mgrs4Tuple._Units_ + ( Str, _Pass)

509

510 @deprecated_property_RO

511 def digraph(self):

512 '''DEPRECATED, use attribute C{EN}.'''

513 return self.EN # PYCHOK or [1]

514

515 def toMgrs(self, Mgrs=Mgrs, **Mgrs_kwds):

516 '''Return this L{Mgrs6Tuple} as an L{Mgrs} instance.

517 '''

518 kwds = dict(self.items())

519 if self.name:

520 kwds.update(name=self.name)

521 if Mgrs_kwds:

522 kwds.update(Mgrs_kwds)

523 return Mgrs(**kwds)

524

525

526 class _RE(object):

527 '''(INTERNAL) Lazily compiled C{re}gex-es to parse MGRS strings.

528 '''

529 _EN = '([A-Z]{2})' # 2-letter grid tile designation

530 _en = '([0-9]+)' # easting_northing digits, 2-10+

531 _pB = '([ABYZ]{1})' # polar region letter, pseudo-zone 0

532 _zB = '([0-9]{1,2}[C-X]{1})' # zone number and band letter, no I|O

533

534 @Property_RO

535 def pB_EN(self): # split polar "BEN" into 2 parts

536 import re # PYCHOK warning locale.Error

537 return re.compile(_RE._pB + _RE._EN, re.IGNORECASE)

538

539 @Property_RO

540 def pB_EN_en(self): # split polar "BEN1235..." into 3 parts

541 import re # PYCHOK warning locale.Error

542 return re.compile(_RE._pB + _RE._EN + _RE._en, re.IGNORECASE)

543

544 @Property_RO

545 def zB_EN(self): # split "1[2]BEN" into 2 parts

546 import re # PYCHOK warning locale.Error

547 return re.compile(_RE._zB + _RE._EN, re.IGNORECASE)

548

549 @Property_RO

550 def zB_EN_en(self): # split "1[2]BEN1235..." into 3 parts

551 import re # PYCHOK warning locale.Error

552 return re.compile(_RE._zB + _RE._EN + _RE._en, re.IGNORECASE)

553

554_RE = _RE() # PYCHOK singleton

555

556

557 def parseMGRS(strMGRS, datum=_WGS84, Mgrs=Mgrs, name=NN):

558 '''Parse a string representing a MGRS grid reference,

559 consisting of C{"[zone]Band, EN, easting, northing"}.

560

561 @arg strMGRS: MGRS grid reference (C{str}).

562 @kwarg datum: Optional datum to use (L{Datum}).

563 @kwarg Mgrs: Optional class to return the MGRS grid

564 reference (L{Mgrs}) or C{None}.

565 @kwarg name: Optional B{C{Mgrs}} name (C{str}).

566

567 @return: The MGRS grid reference as B{C{Mgrs}} or if

568 C{B{Mgrs} is None} as an L{Mgrs4Tuple}C{(zone,

569 EN, easting, northing)}.

570

571 @raise MGRSError: Invalid B{C{strMGRS}}.

572

573 @example:

574

575 >>> m = parseMGRS('31U DQ 48251 11932')

576 >>> str(m) # '31U DQ 48251 11932'

577 >>> m = parseMGRS('31UDQ4825111932')

578 >>> repr(m) # [Z:31U, G:DQ, E:48251, N:11932]

579 >>> m = parseMGRS('42SXD0970538646')

580 >>> str(m) # '42S XD 09705 38646'

581 >>> m = parseMGRS('42SXD9738') # Km

582 >>> str(m) # '42S XD 97000 38000'

583 >>> m = parseMGRS('YUB17770380') # polar

584 >>> str(m) # 'Y UB 17770 03800'

585 '''

586 def _mg(s, re_UTM, re_UPS): # return re.match groups

587 m = re_UTM.match(s)

588 if m:

589 return m.groups()

590 m = re_UPS.match(s.lstrip(_0_))

591 if m:

592 return m.groups()

593# m = m.groups()

594# t = '00' + m[0]

595# return (t,) + m[1:]

596 raise ValueError(_SPACE_(repr(s), _invalid_))

597

598 def _MGRS(strMGRS, datum, Mgrs, name):

599 m = _splituple(strMGRS.strip())

600 if len(m) == 1: # [01]BEN1234512345'

601 m = _mg(m[0], _RE.zB_EN_en, _RE.pB_EN_en)

602 m = m[:2] + halfs2(m[2])

603 elif len(m) == 2: # [01]BEN 1234512345'

604 m = _mg(m[0], _RE.zB_EN, _RE.pB_EN) + halfs2(m[1])

605 elif len(m) == 3: # [01]BEN 12345 12345'

606 m = _mg(m[0], _RE.zB_EN, _RE.pB_EN) + m[1:]

607 if len(m) != 4: # [01]B EN 12345 12345

608 raise ValueError

609

610 zB, EN = m[0].upper(), m[1].upper()

611 if zB[-1:] in 'IO':

612 raise ValueError(_SPACE_(repr(m[0]), _invalid_))

613 e, n, m = _enstr2m3(*m[2:])

614

615 if Mgrs is None:

616 r = Mgrs4Tuple(zB, EN, e, n, name=name)

617 _ = r.toMgrs(resolution=m) # validate

618 else:

619 r = Mgrs(zB, EN, e, n, datum=datum, resolution=m, name=name)

620 return r

621

622 return _parseX(_MGRS, strMGRS, datum, Mgrs, name,

623 strMGRS=strMGRS, Error=MGRSError)

624

625

626 def toMgrs(utmups, Mgrs=Mgrs, name=NN, **Mgrs_kwds):

627 '''Convert a UTM or UPS coordinate to an MGRS grid reference.

628

629 @arg utmups: A UTM or UPS coordinate (L{Utm}, L{Etm} or L{Ups}).

630 @kwarg Mgrs: Optional class to return the MGRS grid reference

631 (L{Mgrs}) or C{None}.

632 @kwarg name: Optional B{C{Mgrs}} name (C{str}).

633 @kwarg Mgrs_kwds: Optional, additional B{C{Mgrs}} keyword

634 arguments, ignored if C{B{Mgrs} is None}.

635

636 @return: The MGRS grid reference as B{C{Mgrs}} or if

637 C{B{Mgrs} is None} as an L{Mgrs6Tuple}C{(zone,

638 EN, easting, northing, band, datum)}.

639

640 @raise MGRSError: Invalid B{C{utmups}}.

641

642 @raise TypeError: If B{C{utmups}} is not L{Utm} nor L{Etm}

643 nor L{Ups}.

644

645 @example:

646

647 >>> u = Utm(31, 'N', 448251, 5411932)

648 >>> m = u.toMgrs() # 31U DQ 48251 11932

649 '''

650# _MODS.utmups.utmupsValidate(utmups, MGRS=True, Error-MGRSError)

651 _xinstanceof(Utm, Ups, utmups=utmups) # Utm, Etm, Ups

652 try:

653 e, n = utmups.eastingnorthing2(falsed=True)

654 E, e = _um100km2(e)

655 N, n = _um100km2(n)

656 B, z = utmups.band, utmups.zone

657 if _UTM_ZONE_MIN <= z <= _UTM_ZONE_MAX:

658 i = z - 1

659 # columns in zone 1 are A-H, zone 2 J-R, zone 3 S-Z,

660 # then repeating every 3rd zone (note E-1 because

661 # eastings start at 166e3 due to 500km false origin)

662 EN = _LeUTM[i % 3][E - 1]

663 # rows in even zones are A-V, in odd zones are F-E

664 EN += _LnUTM[i % 2][N % len(_LnUTM[0])]

665 elif z == _UPS_ZONE:

666 EN = _LeUPS[B][E - _FeUPS[B]]

667 EN += _LnUPS[B][N - _FnUPS[B]]

668 else:

669 raise _ValueError(zone=z)

670 except (IndexError, TypeError, ValueError) as x:

671 raise MGRSError(B=B, E=E, N=N, utmups=utmups, cause=x)

672

673 if Mgrs is None:

674 r = Mgrs4Tuple(Fmt.zone(z), EN, e, n).to6Tuple(B, utmups.datum)

675 else:

676 kwds = _xkwds(Mgrs_kwds, band=B, datum=utmups.datum)

677 r = Mgrs(z, EN, e, n, **kwds)

678 return _xnamed(r, name or utmups.name)

679

680

681 def _um100km2(m):

682 '''(INTERNAL) An MGRS east-/northing truncated to micrometer (um)

683 precision and to grid tile C{M} and C{m}eter within the tile.

684 '''

685 m = int(m / _1um) * _1um # micrometer

686 M, m = divmod(m, _100km)

687 return int(M), m

688

689

690 if __name__ == '__main__':

691

692 from pygeodesy.ellipsoidalVincenty import fabs, LatLon

693 from pygeodesy.lazily import _getenv, printf

694

695# from math import fabs # from .ellipsoidalVincenty

696 from os import access as _access, linesep as _NL, X_OK as _X_OK

697

698 # <https://GeographicLib.sourceforge.io/C++/doc/GeoConvert.1.html>

699 _GeoConvert = _getenv('PYGEODESY_GEOCONVERT', '/opt/local/bin/GeoConvert')

700 if _access(_GeoConvert, _X_OK):

701 GC_m = _GeoConvert, '-m' # -m converts latlon to MGRS

702 printf(' using: %s ...', _SPACE_.join(GC_m))

703 from pygeodesy.solveBase import _popen2

704 else:

705 GC_m = _popen2 = None

706

707 e = n = 0

708 try:

709 for lat in range(-90, 91, 1):

710 printf('%6s: lat %s ...', n, lat, end=NN, flush=True)

711 nl = _NL

712 for lon in range(-180, 181, 1):

713 m = LatLon(lat, lon).toMgrs()

714 if _popen2:

715 t = '%s %s' % (lat, lon)

716 g = _popen2(GC_m, stdin=t)[1]

717 t = m.toStr() # sep=NN

718 if t != g:

719 e += 1

720 printf('%s%6s: %s: %r vs %r (lon %s)', nl, -e, m, t, g, lon)

721 nl = NN

722 t = m.toLatLon(LatLon=LatLon)

723 d = max(fabs(t.lat - lat), fabs(t.lon - lon))

724 if d > 1e-9 and -90 < lat < 90 and -180 < lon < 180:

725 e += 1

726 printf('%s%6s: %s: %s vs %s %.6e', nl, -e, m, t.latlon, (float(lat), float(lon)), d)

727 nl = NN

728 n += 1

729 if nl:

730 print(' OK')

731 except KeyboardInterrupt:

732 printf(nl)

733

734 p = e * 100.0 / n

735 printf('%6s: %s errors (%.2f%%)', n, (e if e else 'no'), p)

736

737# **) MIT License

738#

739# Copyright (C) 2016-2023 -- mrJean1 at Gmail -- All Rights Reserved.

740#

741# Permission is hereby granted, free of charge, to any person obtaining a

742# copy of this software and associated documentation files (the "Software"),

743# to deal in the Software without restriction, including without limitation

744# the rights to use, copy, modify, merge, publish, distribute, sublicense,

745# and/or sell copies of the Software, and to permit persons to whom the

746# Software is furnished to do so, subject to the following conditions:

747#

748# The above copyright notice and this permission notice shall be included

749# in all copies or substantial portions of the Software.

750#

751# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

752# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

753# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

754# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

755# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

756# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

757# OTHER DEALINGS IN THE SOFTWARE.