Package pygeodesy :: Module etm :: Class Etm |
[frames] | no frames]

# Class Etm

       object --+
                |
     named._Named --+
                    |
     named._NamedBase --+
                        |
    utmupsBase.UtmUpsBase --+
                            |
                      utm.Utm --+
                                |
                               Etm

Exact Transverse Mercator (ETM) coordinate, a sub-class of Utm, a Universal Transverse Mercator (UTM) coordinate using the ExactTransverseMercator projection for highest accuracy.

Note: Conversion of Etm coordinates to and from (geodetic) lat- and longitude is 3-4 times slower than Utm.

See Also: Karney's Detailed Description.

Instance Methods
__init__(self, zone, hemisphere, easting, northing, band=`'````'`, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Tran`...`, falsed=True, convergence=None, scale=None, name=`'````'`) New Etm coordinate. |
parseETM(self, strETM) Parse a string to a ETM coordinate. |
toLatLon(self, LatLon=None, unfalse=True, **unused) Convert this ETM coordinate to an (ellipsoidal) geodetic point. |
toUtm(self) Coopy this ETM to a UTM coordinate. |
Inherited from `utm.Utm`: `__eq__`, `__repr__`, `__str__`, `parseUTM`, `toEtm`, `toMgrs`, `toStr`, `toStr2`, `toUps` Inherited from `utmupsBase.UtmUpsBase`: `eastingnorthing2`, `to2en`, `toEpsg` Inherited from `named._NamedBase`: `others` Inherited from `named._Named`: `_dot_`, `attrs`, `classof`, `copy` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
| exactTM Property to get and set the ETM projection (ExactTransverseMercator).
Inherited from `utm.Utm`: `band`, `falsed2`, `pole`, `zone` Inherited from `utmupsBase.UtmUpsBase`: `convergence`, `datum`, `easting`, `eastingnorthing`, `falsed`, `hemisphere`, `northing`, `scale`, `scale0` Inherited from `named._Named`: `classname`, `classnaming`, `name`, `named`, `named2` Inherited from `object`: `__class__`

Method Details

### __init__ (self, zone, hemisphere, easting, northing, band=`'````'`, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Tran`...`, falsed=True, convergence=None, scale=None, name=`'````'`) (Constructor) |
New Etm coordinate. Arguments: `zone` - Longitudinal UTM zone (`int`, 1..60) or zone with/-out (latitudinal) Band letter (`str`, '01C'..'60X'). `hemisphere` - Northern or southern hemisphere (`str`, `'N[orth]'` or `'S[outh]'`). `easting` - Easting, see `falsed` (`meter`). `northing` - Northing, see `falsed` (`meter`). `band` - Optional, (latitudinal) band (`str`, 'C'..'X'). `datum` - Optional, this coordinate's datum (Datum). `falsed` - Both `easting` and `northing` are falsed (`bool`). `convergence` - Optional meridian convergence, bearing off grid North, clockwise from true North (`degrees`) or `None`. `scale` - Optional grid scale factor (`scalar`) or `None`. `name` - Optional name (`str`). Raises: `ETMError` - Invalid `zone`, `hemishere` or `band`. Overrides: object.__init__ Example:
    >>> import pygeodesy
    >>> u = pygeodesy.Etm(31, 'N', 448251, 5411932)

### parseETM (self, strETM) |
Parse a string to a ETM coordinate. Returns: The coordinate (Etm). See Also: Function parseETM5 in this module etm.

### toLatLon (self, LatLon=None, unfalse=True, **unused) |
Convert this ETM coordinate to an (ellipsoidal) geodetic point. Arguments: `LatLon` - Optional, ellipsoidal class to return the geodetic point (`LatLon`) or `None`. `unfalse` - Unfalse `easting` and `northing` if falsed (`bool`). Returns: This ETM coordinate as (`LatLon`) or a LatLonDatum5Tuple`(lat, lon, datum, convergence, scale)` if `LatLon` is `None`. Raises: `EllipticError` - No convergence. `TypeError` - If `LatLon` is not ellipsoidal. Overrides: utm.Utm.toLatLon Example:
    >>> from pygeodesy import ellipsoidalVincenty as eV, Etm
    >>> u = Etm(31, 'N', 448251.795, 5411932.678)
    >>> ll = u.toLatLon(eV.LatLon)  # 48°51′29.52″N, 002°17′40.20″E

### toUtm (self) |
Coopy this ETM to a UTM coordinate. Arguments: `zone` - New UTM zone (`int`). `eps` - Optional convergence limit, EPS or above (`float`), see method Utm.toLatLon. `falsed` - False both easting and northing (`bool`). Returns: The UTM coordinate (Utm). Overrides: utm.Utm.toUtm

Property Details

### exactTM Property to get and set the ETM projection (ExactTransverseMercator). Get method: exactTM(self) - Get the ETM projection (ExactTransverseMercator). Set method: exactTM(self, exactTM) - Set the ETM projection (ExactTransverseMercator).