# Source code for tecplot.data.query

    from builtins import str

    from collections import namedtuple
    from ctypes import byref, c_double, c_int32, c_int64

    from ..tecutil import _tecutil
    from ..constant import *
    from ..exception import *
    from .. import layout
    from ..tecutil import Index, IndexSet, lock

    @lock()
    def probe_at_position(x, y, z=None, nearest=False, starting_cell=None,
                          starting_zone=None, zones=None, dataset=None, frame=None):
        """Returns field values at a point in space.

        .. note::

            The position is taken according to the axis assignments of the `Frame`
            which may be any of the associated variables in the `Dataset` and not
            necessarily ``(X, Y, Z)``. See: `Cartesian3DFieldAxis.variable`.

        Parameters:
            x,y,z (`float`, *z* is optional): position to probe for field values.
            nearest (`bool`): Returns the values at the nearest node to the given
                position. Probe position must be inside the volume of the data
                being queried, otherwise this will return `None`.
            starting_cell (3-`tuple` of `integers <int>`, optional):
                The ``(i,j,k)``-index of the cell to start looking for the given
                position. This must be used with ``starting_zone``.
            starting_zone (`Zone <data_access>`, optional): The first zone to start
                searching. This is required only when ``starting_cell`` is
                specified.
            zones (`list` of `Zones <data_access>`, optional): Limits the search to
                the given zones. `None` implies searching all zones. (default:
                `None`)
            dataset (`Dataset`, optional): The `Dataset` to probe. (defaults to
                the active `Dataset`.)
            frame (`Frame`, optional): The `Frame` which determines the spatial
                variable assignment ``(X,Y,Z)``. (defaults to the active `Frame`.)

        Returns:
            `namedtuple <collections.namedtuple>`: ``(data, cell, zone)``:

                ``data`` (`list` of `floats <float>`)
                    The values of each variable in the dataset at the given
                    position.
                ``cell`` (3-`tuple` of `integers <int>`)
                    ``(i,j,k)`` of the cell containing the given position.
                ``zone`` (`Zone <data_access>`)
                    Zone containing the given position

        .. note:: Returns `None` if the position can't be probed.

            This method will return `None` if the position is outside the volume
            of the data being queried. This means one should capture the results
            in a single variable and test it against `None` before proceeding::

                result = tp.data.query.probe_at_position(1.0, 2.0, 3.0)
                if result is None:
                    print('probe failed.')
                else:
                    data, cell, zone = result

            Additionally, with Tecplot 360 versions 2018 R1 and later, this
            function will raise an exception if Tecplot 360 was interrupted via the
            GUI during the probe operation.
        """
        if __debug__:
            if frame and dataset and frame.dataset != dataset:
                msg = ('Dataset must be attached to the input Frame: {} != {}'.
                       format(repr(frame.dataset), repr(dataset)))
                raise TecplotValueError(msg)
            if (starting_cell is None) ^ (starting_zone is None):
                msg = 'starting_cell option requires an associated starting_zone'
                raise TecplotLogicError(msg)

        if dataset is None:
            if frame is None:
                frame = layout.active_frame()
            dataset = frame.dataset
        elif frame is None:
            frame = dataset.frame

        with frame.activated():
            if starting_cell is None:
                start_with_local_cell = False
                i, j, k = 0, 0, 0
                starting_zone_index = 0
            else:
                start_with_local_cell = True
                i, j, k = (x+1 for x in starting_cell)
                starting_zone_index = starting_zone.index

            allocd = []
            if zones is not None:
                zones = IndexSet(*zones)
                allocd.append(zones)

            data = (max(3, dataset.num_variables)*c_double)()

            try:
                result = _tecutil.ProbeAtPosition(
                    x, y, z or 0,
                    i, j, k,
                    IJKPlanes.Volume.value,
                    starting_zone_index+1,
                    start_with_local_cell,
                    data,
                    zones,
                    z is not None,
                    False,
                    nearest)
                success, i, j, k, plane, zone_index = result
            except TecplotSystemError as e:
                if 'Assertion' in str(e):
                    raise
                success = False

            if not success:
                try:
                    if _tecutil.InterruptCheck():
                        raise TecplotInterruptError()
                except AttributeError:
                    pass  # InterruptCheck added to TecUtilChecked in SDK 2018.1
                return None

            cell = (Index(i-1), Index(j-1), Index(k-1))
            zone_index = Index(zone_index-1)

            for a in allocd:
                a.dealloc()

            ProbeResult = namedtuple('ProbeResult', ['data', 'cell', 'zone'])
            return ProbeResult(data[:], cell, dataset.zone(zone_index))

    @lock()
    def probe_on_surface(positions=((0,),(0,),(0,)), zones=None, variables=None,
                         probe_nearest=ProbeNearest.Position, obey_blanking=True,
                         num_nearest_nodes=20, tolerance=1e-5, dataset=None,
                         frame=None):
        """Returns field values at points on a surface closest the points given.

        .. note::

            The positions are processed according to the axis assignments of the
            `Frame` which may be any of the associated variables in the `Dataset`
            and not necessarily (but usually) ``(X, Y, Z)``. See:
            `Cartesian3DFieldAxis.variable`.

        Parameters:
            positions (2D `float` array): Array of points to probe dimensioned by
                ``(3, N)`` where the first dimension corresponds to ``(x, y, z)``.
                A 1D `float` array is accepted for single point probes, however
                this should be avoided when probing several positions as the
                internal algorithm is optimized for probing many positions at once.
            zones (`list` of `Zones <data_access>`, optional): Limits the search to
                the given zones. `None` implies searching all active relevant
                surface zones including surfaces of ordered volume zones. To search
                FE or polygonal volume boundaries, include the volume zones in this
                list. (default: `None`)
            variables (`list` of `Variables <Variable>`, optional): The variables
                within the dataset to probe. `None` implies all variables.
                (default: `None`)
            probe_nearest (`ProbeNearest`, optional): Probe at the nodal location
                (`ProbeNearest.Node`) or interpolate to nearest location on the
                surface (`ProbeNearest.Position`, default). The return parameter
                **cells_or_nodes** will be cells if set to `ProbeNearest.Position`
                (default), or nodes if set to `ProbeNearest.Node`.
            obey_blanking (`bool`, optional): Do not search blanked cells according
                the frame's style settings. (default: `True`)
            num_nearest_nodes (`int`, optional): Only consider surface
                cells that contain one of the closest ``N`` nodes to the probed
                position. For highly varying surfaces, the nearest cell may or may
                not contain the nearest nodes to the probe position and so this
                value should be increased accordingly, however doing so increases
                the search-space linearly. (default: 20)
            tolerance (`float`, optional): The percentage of the longest cartesian
                ``(x, y, z)`` dimension subtended by the polygons of the surface.
                This is used in several parts of the algorithm to find the nearest
                position on the surface zones and should be increased when probing
                imprecise nodal position data. (default: 1e-5)
            dataset (`Dataset`, optional): The `Dataset` to probe. (defaults to
                the active `Dataset`.)
            frame (`Frame`, optional): The `Frame` which determines the spatial
                variable assignment ``(X,Y,Z)``. (defaults to the active `Frame`.)

        Returns:
            `namedtuple <collections.namedtuple>`: ``(data, cells_or_nodes, planes,
            zone)``:

                ``data`` (`list` of `floats <float>`)
                    Flattened `float` array which can be reshaped to ``(V, N)``
                    where ``V`` is the number of variables returned (either the
                    number of variables in the dataset or the length of
                    **variables** input parameter) and ``N`` is the number of
                    points probed.
                ``cells_or_nodes`` (`list` of `integers <int>`)
                    The index to the cells (or nodes if `ProbeNearest.Node` was
                    passed in to **probe_nearest**) containing the returned
                    positions.
                ``planes`` (`list` of `IJKPlanes`)
                    For ordered zones, these are the plane-orientations of the
                    cells for each probed position.
                ``zones`` (`list` of `Zones <data_access>`)
                    Zones containing the given positions.

        .. versionadded:: 2018.1
            Probe on surface requires Tecplot 360 2018 R1 or later.

        .. note:: The frame's plot type must be set to `PlotType.Cartesian3D`

            Probe on surface requires the spatial variables to be set according to
            the frame's style. This can be done by setting the plot type to
            `PlotType.Cartesian3D`. Example::

                tp.active_frame().plot_type = tp.constant.PlotType.Cartesian3D

            For probing on 2D data, use `probe_at_position()`.

        .. note:: Linear zones will always return nearest nodal values.

            If linear zones, which are ignored by default, are included in the
            **zones** parameter, the resulting values on that zone will always be
            nodal and no interpolation on the position will be done.

        .. note:: Irregular or jaggged surfaces may behave poorly.

            For performance reasons, this algorithm has the potential to miss the
            closest position on highly varying surfaces. This can be addressed by
            first increasing **num_nearest_nodes** to search more of the zones and
            then by increasing the **tolerance** to allow for imprecise position
            data.

        Example usage:

        .. code-block:: python
            :emphasize-lines: 14,28

            from os import path
            import numpy as np

            import tecplot as tp
            from tecplot.constant import PlotType

            examples = tp.session.tecplot_examples_directory()
            datafile = path.join(examples, 'SimpleData', 'F18.plt')
            ds = tp.data.load_tecplot(datafile)
            fr = tp.active_frame()
            fr.plot_type = PlotType.Cartesian3D

            # probe a single point
            res = tp.data.query.probe_on_surface((13.5, 4.0, 0.6 ))

            '''
            The following line will print:
                (13.499723788684996, 3.9922783797612795, 0.49241572276992346,
                0.0018958827755862578, 0.07313805429221854, 0.997276718375976,
                0.06335166319722907)
            '''
            print(res.data)

            # probe multiple points
            points = np.array([[13.5,  4.0, 0.6],  # just above starboard wing
                               [13.5, -4.0, 0.6]]) # just above port wing

            res = tp.data.query.probe_on_surface(points.transpose())
            values = np.array(res.data).reshape((-1, len(points))).transpose()

            '''
            The following will print the probed position and the result of the probe
                [ 13.5   4.    0.6] [  1.34997238e+01   3.99227838e+00   4.92415723e-01
                   1.89588278e-03   7.31380543e-02   9.97276718e-01   6.33516632e-02]
                [ 13.5  -4.    0.6] [  1.34997238e+01  -3.99227838e+00   4.92415723e-01
                   1.89588278e-03   7.31380543e-02   9.97276718e-01   6.33516632e-02]
            '''
            for pt, v in zip(points, values):
                print(pt, v)
        """
        if __debug__:
            if frame and dataset and frame.dataset != dataset:
                msg = ('Dataset must be attached to the input Frame: {} != {}'.
                       format(repr(frame.dataset), repr(dataset)))
                raise TecplotValueError(msg)

        if dataset is None:
            if frame is None:
                frame = layout.active_frame()
            dataset = frame.dataset
        elif frame is None:
            frame = dataset.frame

        if not hasattr(positions[0], '__iter__'):
            positions = tuple(tuple([p]) for p in positions)

        nvariables = dataset.num_variables if variables is None else len(variables)

        with frame.activated():
            n = max(len(p) for p in positions)
            m = n * nvariables
            x = (c_double * n)(*[float(p) for p in positions[0]])
            y = (c_double * n)(*[float(p) for p in positions[1]])
            z = (c_double * n)(*[float(p) for p in positions[2]])
            v = (c_double * m)()
            cells_or_nodes = (c_int64 * n)()
            planes = (c_int32 * n)()
            zone_indices = (c_int32 * n)()

            zone_set = None if zones is None else IndexSet(zones)
            var_set = None if variables is None else IndexSet(variables)
            try:
                if not _tecutil.ProbeOnSurface(n, x, y, z, zone_set, var_set,
                                               ProbeNearest(probe_nearest).value,
                                               obey_blanking, num_nearest_nodes,
                                               tolerance, v, cells_or_nodes,
                                               planes, zone_indices):
                    raise TecplotSystemError()
            finally:
                if zone_set is not None:
                    zone_set.dealloc()
                if var_set is not None:
                    var_set.dealloc()

            cells_or_nodes = tuple(cells_or_nodes)
            planes = tuple(IJKPlanes(i) for i in planes)
            zones = tuple(dataset.zone(i) for i in zone_indices)

            SurfaceProbeResult = namedtuple('SurfaceProbeResult',
                ['data', 'cells_or_nodes', 'planes', 'zones'])
            return SurfaceProbeResult(tuple(v), cells_or_nodes, planes, zones)