# Source code for sensors.polulu

    '''
    Import data saved with polulu-sensors
    https://www.pololu.com/product/2738
    These are low-cost IMUS (<20 US$), where acceleration/gyroscope data are not
    sampled at the same time as the magnetic field data (just over 100 Hz).
    As a result, the interpolated sampling rate has to be set by hand.
    '''

    '''
    Author: Thomas Haslwanter
    Version: 0.2
    Date: May-2016
    '''

    import numpy as np
    import pandas as pd

    class FileNotFoundError(OSError):
        pass

    def get_data(inFile, rate=125):
        '''Get the sampling rate, as well as the recorded data.

        Parameters
        ----------
        in_file : string
                Filename of the data-file

        Returns
        -------
        out_list: list
                Contains the following parameters:

                - rate
                - acceleration
                - angular_velocity
                - mag_field_direction
        '''

        # Get the sampling rate from the second line in the file
        try:
            # Get the data, and label them
            data = pd.read_csv(inFile, header=None, sep='[ ]*')
            data.columns = ['acc_x', 'acc_y', 'acc_z', 'gyr_x', 'gyr_y', 'gyr_z', 'mag_x', 'mag_y', 'mag_z', 'taccgyr', 'tmag']

            # interpolate with a manually set rate
            dt = 1/np.float(rate)
            t_lin = np.arange(0, 25, dt)

            data_interp = pd.DataFrame()
            for ii in range(6):
                data_interp[data.keys()[ii]] = np.interp(t_lin*1000, data['taccgyr'], data.ix[:,ii])
            for ii in range(6,9):
                data_interp[data.keys()[ii]] = np.interp(t_lin*1000, data['tmag'], data.ix[:,ii])
            data_interp['time'] = t_lin

            # Set the conversion factors by hand, and apply them
            conversions = {}
            conversions['mag'] = 1/6842
            conversions['acc'] = 0.061/1000
            conversions['gyr'] = 4.375/1000 * np.pi/180

            data_interp.ix[:,:3] *= conversions['acc']
            data_interp.ix[:,3:6] *= conversions['gyr']
            data_interp.ix[:,6:9] *= conversions['mag']

        except FileNotFoundError:
            print('{0} does not exist!'.format(in_file))
            return -1

        returnValues = [rate]

        # Extract the columns that you want, by name
        paramList=['acc', 'gyr', 'mag']
        for param in paramList:
            Expression = param + '*'
            returnValues.append(data_interp.filter(regex=Expression).values)

        return returnValues

    if __name__ == '__main__':
        inFile = r'..\tests\data\data_barnobi.txt'
        data = get_data(inFile)
        print(data[0])
        print(data[1])
        input('Done')