### Navigation

- index
- modules |
- FabIO v0.1.4 documentation »
- Module code »

# Source code for fabio.GEimage

    #
    # Reads the header from a GE a-Si Angio Detector
    # Using version 8001 of the header from file:
    #     c:\adept\core\DefaultImageInfoConfig.csv
    #
    #  Antonino Miceli
    #  Thu Jan  4 13:46:31 CST 2007
    #

    # modifications by Jon Wright for style, pychecker and fabio
    #

    import numpy
    import struct, logging
    logger = logging.getLogger("GEimage")
    from fabioimage import fabioimage
    from fabioutils import next_filename, previous_filename

    GE_HEADER_INFO = [
        # Name, length in bytes, format for struct (None means string)
        ('ImageFormat', 10, None),
        ('VersionOfStandardHeader', 2, '=H'),
        ('StandardHeaderSizeInBytes', 4, '=L'),
        ('VersionOfUserHeader', 2, '=H'),
        ('UserHeaderSizeInBytes', 4, '=L'),
        ('NumberOfFrames', 2, '=H'),
        ('NumberOfRowsInFrame', 2, '=H'),
        ('NumberOfColsInFrame', 2, '=H'),
        ('ImageDepthInBits', 2, '=H'),
        ('AcquisitionDate', 20, None),
        ('AcquisitionTime', 20, None),
        ('DUTID', 20, None),
        ('Operator', 50, None),
        ('DetectorSignature', 20, None),
        ('TestSystemName', 20, None),
        ('TestStationRevision', 20, None),
        ('CoreBundleRevision', 20, None),
        ('AcquisitionName', 40, None),
        ('AcquisitionParameterRevision', 20, None),
        ('OriginalNumberOfRows', 2, '=H'),
        ('OriginalNumberOfColumns', 2, '=H'),
        ('RowNumberUpperLeftPointArchiveROI', 2, '=H'),
        ('ColNumberUpperLeftPointArchiveROI', 2, '=H'),
        ('Swapped', 2, '=H'),
        ('Reordered', 2, '=H'),
        ('HorizontalFlipped', 2, '=H'),
        ('VerticalFlipped', 2, '=H'),
        ('WindowValueDesired', 2, '=H'),
        ('LevelValueDesired', 2, '=H'),
        ('AcquisitionMode', 2, '=H'),
        ('AcquisitionType', 2, '=H'),
        ('UserAcquisitionCoffFileName1', 100, None),
        ('UserAcquisitionCoffFileName2', 100, None),
        ('FramesBeforeExpose', 2, '=H'),
        ('FramesDuringExpose', 2, '=H'),
        ('FramesAfterExpose', 2, '=H'),
        ('IntervalBetweenFrames', 2, '=H'),
        ('ExposeTimeDelayInMicrosecs', 8, '=d'),
        ('TimeBetweenFramesInMicrosecs', 8, '=d'),
        ('FramesToSkipExpose', 2, '=H'),
        ('ExposureMode', 2, '=H'),
        ('PrepPresetTimeInMicrosecs', 8, '=d'),
        ('ExposePresetTimeInMicrosecs', 8, '=d'),
        ('AcquisitionFrameRateInFps', 4, '=f'),
        ('FOVSelect', 2, '=H'),
        ('ExpertMode', 2, '=H'),
        ('SetVCommon1', 8, '=d'),
        ('SetVCommon2', 8, '=d'),
        ('SetAREF', 8, '=d'),
        ('SetAREFTrim', 4, '=L'),
        ('SetSpareVoltageSource', 8, '=d'),
        ('SetCompensationVoltageSource', 8, '=d'),
        ('SetRowOffVoltage', 8, '=d'),
        ('SetRowOnVoltage', 8, '=d'),
        ('StoreCompensationVoltage', 4, '=L'),
        ('RampSelection', 2, '=H'),
        ('TimingMode', 2, '=H'),
        ('Bandwidth', 2, '=H'),
        ('ARCIntegrator', 2, '=H'),
        ('ARCPostIntegrator', 2, '=H'),
        ('NumberOfRows', 4, '=L'),
        ('RowEnable', 2, '=H'),
        ('EnableStretch', 2, '=H'),
        ('CompEnable', 2, '=H'),
        ('CompStretch', 2, '=H'),
        ('LeftEvenTristate', 2, '=H'),
        ('RightOddTristate', 2, '=H'),
        ('TestModeSelect', 4, '=L'),
        ('AnalogTestSource', 4, '=L'),
        ('VCommonSelect', 4, '=L'),
        ('DRCColumnSum', 4, '=L'),
        ('TestPatternFrameDelta', 4, '=L'),
        ('TestPatternRowDelta', 4, '=L'),
        ('TestPatternColumnDelta', 4, '=L'),
        ('DetectorHorizontalFlip', 2, '=H'),
        ('DetectorVerticalFlip', 2, '=H'),
        ('DFNAutoScrubOnOff', 2, '=H'),
        ('FiberChannelTimeOutInMicrosecs', 4, '=L'),
        ('DFNAutoScrubDelayInMicrosecs', 4, '=L'),
        ('StoreAECROI', 2, '=H'),
        ('TestPatternSaturationValue', 2, '=H'),
        ('TestPatternSeed', 4, '=L'),
        ('ExposureTimeInMillisecs', 4, '=f'),
        ('FrameRateInFps', 4, '=f'),
        ('kVp', 4, '=f'),
        ('mA', 4, '=f'),
        ('mAs', 4, '=f'),
        ('FocalSpotInMM', 4, '=f'),
        ('GeneratorType', 20, None),
        ('StrobeIntensityInFtL', 4, '=f'),
        ('NDFilterSelection', 2, '=H'),
        ('RefRegTemp1', 8, '=d'),
        ('RefRegTemp2', 8, '=d'),
        ('RefRegTemp3', 8, '=d'),
        ('Humidity1', 4, '=f'),
        ('Humidity2', 4, '=f'),
        ('DetectorControlTemp', 8, '=d'),
        ('DoseValueInmR', 8, '=d'),
        ('TargetLevelROIRow0', 2, '=H'),
        ('TargetLevelROICol0', 2, '=H'),
        ('TargetLevelROIRow1', 2, '=H'),
        ('TargetLevelROICol1', 2, '=H'),
        ('FrameNumberForTargetLevelROI', 2, '=H'),
        ('PercentRangeForTargetLevel', 2, '=H'),
        ('TargetValue', 2, '=H'),
        ('ComputedMedianValue', 2, '=H'),
        ('LoadZero', 2, '=H'),
        ('MaxLUTOut', 2, '=H'),
        ('MinLUTOut', 2, '=H'),
        ('MaxLinear', 2, '=H'),
        ('Reserved', 2, '=H'),
        ('ElectronsPerCount', 2, '=H'),
        ('ModeGain', 2, '=H'),
        ('TemperatureInDegC', 8, '=d'),
        ('LineRepaired', 2, '=H'),
        ('LineRepairFileName', 100, None),
        ('CurrentLongitudinalInMM', 4, '=f'),
        ('CurrentTransverseInMM', 4, '=f'),
        ('CurrentCircularInMM', 4, '=f'),
        ('CurrentFilterSelection', 4, '=L'),
        ('DisableScrubAck', 2, '=H'),
        ('ScanModeSelect', 2, '=H'),
        ('DetectorAppSwVersion', 20, None),
        ('DetectorNIOSVersion', 20, None),
        ('DetectorPeripheralSetVersion', 20, None),
        ('DetectorPhysicalAddress', 20, None),
        ('PowerDown', 2, '=H'),
        ('InitialVoltageLevel_VCOMMON', 8, '=d'),
        ('FinalVoltageLevel_VCOMMON', 8, '=d'),
        ('DmrCollimatorSpotSize', 10, None),
        ('DmrTrack', 5, None),
        ('DmrFilter', 5, None),
        ('FilterCarousel', 2, '=H'),
        ('Phantom', 20, None),
        ('SetEnableHighTime', 2, '=H'),
        ('SetEnableLowTime', 2, '=H'),
        ('SetCompHighTime', 2, '=H'),
        ('SetCompLowTime', 2, '=H'),
        ('SetSyncLowTime', 2, '=H'),
        ('SetConvertLowTime', 2, '=H'),
        ('SetSyncHighTime', 2, '=H'),
        ('SetEOLTime', 2, '=H'),
        ('SetRampOffsetTime', 2, '=H'),
        ('FOVStartingValue', 2, '=H'),
        ('ColumnBinning', 2, '=H'),
        ('RowBinning', 2, '=H'),
        ('BorderColumns64', 2, '=H'),
        ('BorderRows64', 2, '=H'),
        ('FETOffRows64', 2, '=H'),
        ('FOVStartColumn128', 2, '=H'),
        ('FOVStartRow128', 2, '=H'),
        ('NumberOfColumns128', 2, '=H'),
        ('NumberOfRows128', 2, '=H'),
        ('VFPAquisition', 2000, None),
        ('Comment', 200, None)
        ]

    class GEimage(fabioimage):

        _need_a_seek_to_read = True

        def _readheader(self, infile):
            """ Read a GE image header """

            infile.seek(0)

            self.header = {}
            for name, nbytes, format in GE_HEADER_INFO:
                if format is None:
                    self.header[ name ] = infile.read(nbytes)
                else:
                    self.header[ name ] = struct.unpack(format,
                                                         infile.read(nbytes))[0]

        def read(self, fname, frame=None):
            """
            Read in header into self.header and
            the data   into self.data
            """
            if frame is None:
                frame = 0
            self.header = {}
            self.resetvals()
            infile = self._open(fname, "rb")
            self.sequencefilename = fname
            self._readheader(infile)
            self.nframes = self.header['NumberOfFrames']
            self._readframe(infile, frame)
            infile.close()
            return self

        def _makeframename(self):
            """ The thing to be printed for the user to represent a frame inside
            a file """
            self.filename = "%s$%04d" % (self.sequencefilename,
                                       self.currentframe)

        def _readframe(self, filepointer, img_num):
            """
            # Load only one image from the sequence
            #    Note: the first image in the sequence 0
            # raises an exception if you give an invalid image
            # otherwise fills in self.data
            """
            if(img_num > self.nframes or img_num < 0):
                raise Exception("Bad image number")
            imgstart = self.header['StandardHeaderSizeInBytes'] + \
                       self.header['UserHeaderSizeInBytes'] + \
                       img_num * self.header['NumberOfRowsInFrame'] * \
                       self.header['NumberOfColsInFrame'] * \
                       self.header['ImageDepthInBits'] / 8
            # whence = 0 means seek from start of file
            filepointer.seek(imgstart, 0)

            self.bpp = self.header['ImageDepthInBits'] / 8 # hopefully 2
            imglength = self.header['NumberOfRowsInFrame'] * \
                        self.header['NumberOfColsInFrame'] * self.bpp
            if self.bpp != 2:
                logging.warning("Using uint16 for GE but seems to be wrong")

            # Guessing it is always unsigned int?
            self.data = numpy.fromstring(filepointer.read(imglength), numpy.uint16)
            self.data.shape = (self.header['NumberOfRowsInFrame'],
                                self.header['NumberOfColsInFrame'])
            self.dim2 , self.dim1 = self.data.shape
            self.currentframe = int(img_num)
            self._makeframename()

        def write(self, fname, force_type=numpy.uint16):
            """ Not yet implemented"""
            raise Exception("Write is not implemented")

        def getframe(self, num):
            """
            Returns a frame as a new fabioimage object
            """
            if num < 0 or num > self.nframes:
                raise Exception("Requested frame number is out of range")
            # Do a deep copy of the header to make a new one
            newheader = {}
            for k in self.header.keys():
                newheader[k] = self.header[k]
            frame = GEimage(header=newheader)
            frame.nframes = self.nframes
            frame.sequencefilename = self.sequencefilename
            infile = frame._open(self.sequencefilename, "rb")
            frame._readframe(infile, num)
            infile.close()
            return frame

        def next(self):
            """
            Get the next image in a series as a fabio image
            """
            if self.currentframe < (self.nframes - 1) and self.nframes > 1:
                return self.getframe(self.currentframe + 1)
            else:
                newobj = GEimage()
                newobj.read(next_filename(
                    self.sequencefilename))
                return newobj

        def previous(self):
            """
            Get the previous image in a series as a fabio image
            """
            if self.currentframe > 0:
                return self.getframe(self.currentframe - 1)
            else:
                newobj = GEimage()
                newobj.read(previous_filename(
                    self.sequencefilename))
                return newobj

    def demo():
        import sys, time

        if len(sys.argv) < 2:
            print "USAGE: GE_script.py <GEaSi_raw_image_file>"
            sys.exit()

        image_file = sys.argv[1]

        print "init read_GEaSi_data class and load header.."
        sequence1 = GEimage()
        sequence1.read(image_file)

        print "TimeBetweenFramesInMicrosecs = ",
        print sequence1.header['TimeBetweenFramesInMicrosecs']
        print "AcquisitionTime = ",
        print sequence1.header['AcquisitionTime']

        print "Mean = ", sequence1.data.ravel().mean()

        while 1:
            start = time.time()
            try:
                sequence1 = sequence1.next()
                print sequence1.currentframe, sequence1.data.ravel().mean(), \
                      time.time() - start
            except Exception, ex:
                raise ex

    if __name__ == '__main__':
        demo()

### Navigation

- index
- modules |
- FabIO v0.1.4 documentation »
- Module code »