# Coverage for pygeodesy/lcc.py : 96%

## 281 statements 270 run 11 missing 13 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 616 617 618 619 620 621 622 623 624 625 626 627 628 629 630 631 632 633 634 635 636 637 638 639 640 641 642 643 644 645 646 647 648 649 650 651 652 653 654 655 656 657 658 659 660 661 662 663 664 665 666 667 668 669 670 671 672 673 674 675 676 677 678 679 680 681 682 683 684 685 686 687 688 689 690 691 692 693 694 | # -*- coding: utf-8 -*- u'''Lambert Conformal Conic (LCC) projection. Lambert conformal conic projection for 1- or 2-Standard Parallels classes L{Conic}, L{Conics} registry, L{LCCError} and position class L{Lcc}. See U{LCC<https://WikiPedia.org/wiki/Lambert_conformal_conic_projection>}, U{Lambert Conformal Conic to Geographic Transformation Formulae <https://www.Linz.govt.NZ/data/geodetic-system/coordinate-conversion/projection-conversions/lambert-conformal-conic-geographic>}, U{Lambert Conformal Conic Projection<https://MathWorld.Wolfram.com/LambertConformalConicProjection.html>} and John P. Snyder U{'Map Projections - A Working Manual'<https://Pubs.USGS.gov/pp/1395/report.pdf>}, 1987, pp 107-109. @var Conics.Be08Lb: Conic(name='Be08Lb', lat0=50.797815, lon0=4.35921583, par1=49.8333339, par2=51.1666672, E0=649328, N0=665262, k0=1, SP=2, datum=Datum(name='GRS80', ellipsoid=Ellipsoids.GRS80, transform=Transforms.WGS84), @var Conics.Be72Lb: Conic(name='Be72Lb', lat0=90, lon0=4.3674867, par1=49.8333339, par2=51.1666672, E0=150000.013, N0=5400088.438, k0=1, SP=2, datum=Datum(name='NAD83', ellipsoid=Ellipsoids.GRS80, transform=Transforms.NAD83), @var Conics.Fr93Lb: Conic(name='Fr93Lb', lat0=46.5, lon0=3, par1=49, par2=44, E0=700000, N0=6600000, k0=1, SP=2, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), @var Conics.MaNLb: Conic(name='MaNLb', lat0=33.3, lon0=-5.4, par1=31.73, par2=34.87, E0=500000, N0=300000, k0=1, SP=2, datum=Datum(name='NTF', ellipsoid=Ellipsoids.Clarke1880IGN, transform=Transforms.NTF), @var Conics.MxLb: Conic(name='MxLb', lat0=12, lon0=-102, par1=17.5, par2=29.5, E0=2500000, N0=0, k0=1, SP=2, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), @var Conics.PyT_Lb: Conic(name='PyT_Lb', lat0=46.8, lon0=2.33722917, par1=45.8989389, par2=47.6960144, E0=600000, N0=200000, k0=1, SP=2, datum=Datum(name='NTF', ellipsoid=Ellipsoids.Clarke1880IGN, transform=Transforms.NTF), @var Conics.USA_Lb: Conic(name='USA_Lb', lat0=23, lon0=-96, par1=33, par2=45, E0=0, N0=0, k0=1, SP=2, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), @var Conics.WRF_Lb: Conic(name='WRF_Lb', lat0=40, lon0=-97, par1=33, par2=45, E0=0, N0=0, k0=1, SP=2, datum=Datum(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84) ''' # make sure int/int division yields float quotient, see .basics from __future__ import division as _; del _ # PYCHOK semicolon from pygeodesy.basics import copysign0, _xinstanceof, _xsubclassof from pygeodesy.ellipsoidalBase import LatLonEllipsoidalBase as _LLEB from pygeodesy.datums import Datums, _ellipsoidal_datum from pygeodesy.errors import _IsnotError, _ValueError from pygeodesy.fmath import hypot from pygeodesy.interns import EPS, EPS02, NN, PI_2, _COMMASPACE_, _ellipsoidal_, \ _float as _F, _GRS80_, _k0_, _lat0_, _lon0_, _m_, \ _NAD83_, _NTF_, _SPACE_, _WGS84_, _0_0, _0_5, \ _1_0, _2_0, _90_0 from pygeodesy.interns import _C_ # PYCHOK used! from pygeodesy.lazily import _ALL_LAZY from pygeodesy.named import _lazyNamedEnumItem as _lazy, _NamedBase, \ _NamedEnum, _NamedEnumItem, nameof, _xnamed from pygeodesy.namedTuples import EasNor3Tuple, LatLonDatum3Tuple, \ LatLon2Tuple, _LL4Tuple, PhiLam2Tuple from pygeodesy.props import deprecated_method, Property, Property_RO, \ _update_all from pygeodesy.streprs import Fmt, _fstrENH2, _xzipairs from pygeodesy.units import Easting, Height, Lam_, Northing, Phi_, Scalar_ from pygeodesy.utily import degrees90, degrees180, sincos2, tanPI_2_2 from math import atan, log, radians, sin, sqrt __all__ = _ALL_LAZY.lcc __version__ = '22.05.04' _E0_ = 'E0' _N0_ = 'N0' _par1_ = 'par1' _par2_ = 'par2' _SP_ = 'SP' class Conic(_NamedEnumItem): '''Lambert conformal conic projection (1- or 2-SP). ''' _auth = NN # authorization (C{str}) _datum = None # datum (L{Datum}) _name = NN # Conic.__name__, set below _e = _0_0 # ellipsoid excentricity (C{float}) _E0 = _0_0 # false easting (C{float}) _k0 = _1_0 # scale factor (C{float}) _N0 = _0_0 # false northing (C{float}) _SP = 0 # 1- or 2-SP (C{int}) _opt3 = _0_0 # optional, longitude (C{radians}) _par1 = _0_0 # 1st std parallel (C{radians}) _par2 = _0_0 # 2nd std parallel (C{radians}) _phi0 = _0_0 # origin lat (C{radians}) _lam0 = _0_0 # origin lon (C{radians}) _aF = _0_0 # precomputed F (C{float}) _n = _0_0 # precomputed n (C{float}) _1_n = _0_0 # precomputed 1 / n (C{float}) _r0 = _0_0 # precomputed rho0 (C{float}) def __init__(self, latlon0, par1, par2=None, E0=0, N0=0, k0=1, opt3=0, name=NN, auth=NN): '''New Lambert conformal conic projection. @arg latlon0: Origin with (ellipsoidal) datum (C{LatLon}). @arg par1: First standard parallel (C{degrees90}). @kwarg par2: Optional, second standard parallel (C{degrees90}). @kwarg E0: Optional, false easting (C{meter}). @kwarg N0: Optional, false northing (C{meter}). @kwarg k0: Optional scale factor (C{scalar}). @kwarg opt3: Optional meridian (C{degrees180}). @kwarg name: Optional name of the conic (C{str}). @kwarg auth: Optional authentication authority (C{str}). @return: A Lambert projection (L{Conic}). @raise TypeError: Non-ellipsoidal B{C{latlon0}}. @raise ValueError: Invalid B{C{par1}}, B{C{par2}}, B{C{E0}}, B{C{N0}}, B{C{k0}} or B{C{opt3}}. @example: >>> from pygeodesy import Conic, Datums, ellipsoidalNvector >>> ll0 = ellipsoidalNvector.LatLon(23, -96, datum=Datums.NAD27) >>> Snyder = Conic(ll0, 33, 45, E0=0, N0=0, name='Snyder') ''' if latlon0 is not None: _xinstanceof(_LLEB, latlon0=latlon0) self._phi0, self._lam0 = latlon0.philam self._par1 = Phi_(par1=par1) self._par2 = self._par1 if par2 is None else Phi_(par2=par2) if k0 != 1: self._k0 = Scalar_(k0=k0) if E0: self._E0 = Northing(E0=E0, falsed=True) if N0: self._N0 = Easting(N0=N0, falsed=True) if opt3: self._opt3 = Lam_(opt3=opt3) self.toDatum(latlon0.datum)._dup2(self) self._register(Conics, name) elif name: self.name = name if auth: self._auth = str(auth) @Property_RO def auth(self): '''Get the authentication authority (C{str}). ''' return self._auth @deprecated_method def convertDatum(self, datum): '''DEPRECATED, use method L{Conic.toDatum}.''' return self.toDatum(datum) @Property_RO def datum(self): '''Get the datum (L{Datum}). ''' return self._datum @Property_RO def E0(self): '''Get the false easting (C{meter}). ''' return self._E0 @Property_RO def k0(self): '''Get scale factor (C{float}). ''' return self._k0 @Property_RO def lat0(self): '''Get the origin latitude (C{degrees90}). ''' return degrees90(self._phi0) @Property_RO def latlon0(self): '''Get the central origin (L{LatLon2Tuple}C{(lat, lon)}). ''' return LatLon2Tuple(self.lat0, self.lon0, name=self.name) @Property_RO def lam0(self): '''Get the central meridian (C{radians}). ''' return self._lam0 @Property_RO def lon0(self): '''Get the central meridian (C{degrees180}). ''' return degrees180(self._lam0) @Property_RO def N0(self): '''Get the false northing (C{meter}). ''' return self._N0 @Property_RO def name2(self): '''Get the conic and datum names as "conic.datum" (C{str}). ''' return self._DOT_(self.datum.name) @Property_RO def opt3(self): '''Get the optional meridian (C{degrees180}). ''' return degrees180(self._opt3) @Property_RO def par1(self): '''Get the 1st standard parallel (C{degrees90}). ''' return degrees90(self._par1) @Property_RO def par2(self): '''Get the 2nd standard parallel (C{degrees90}). ''' return degrees90(self._par2) @Property_RO def phi0(self): '''Get the origin latitude (C{radians}). ''' return self._phi0 @Property_RO def philam0(self): '''Get the central origin (L{PhiLam2Tuple}C{(phi, lam)}). ''' return PhiLam2Tuple(self.phi0, self.lam0, name=self.name) @Property_RO def SP(self): '''Get the number of standard parallels (C{int}). ''' return self._SP def toDatum(self, datum): '''Convert this conic to the given datum. @arg datum: Ellipsoidal datum to use (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @return: Converted conic, unregistered (L{Conic}). @raise TypeError: Non-ellipsoidal B{C{datum}}. ''' d = _ellipsoidal_datum(datum, name=self.name) E = d.ellipsoid if not E.isEllipsoidal: raise _IsnotError(_ellipsoidal_, datum=datum) c = self if c._e != E.e or c._datum != d: c = Conic(None, 0, name=self._name) self._dup2(c) c._datum = d c._e = E.e if abs(c._par1 - c._par2) < EPS: m1 = c._mdef(c._phi0) t1 = c._tdef(c._phi0) t0 = t1 k = 1 # _1_0 n = sin(c._phi0) sp = 1 else: m1 = c._mdef(c._par1) m2 = c._mdef(c._par2) t1 = c._tdef(c._par1) t2 = c._tdef(c._par2) t0 = c._tdef(c._phi0) k = c._k0 n = (log(m1) - log(m2)) \ / (log(t1) - log(t2)) sp = 2 F = m1 / (n * pow(t1, n)) c._aF = k * E.a * F c._n = n c._1_n = _1_0 / n c._r0 = c._rdef(t0) c._SP = sp return c def toStr(self, prec=8, name=NN, **unused): # PYCHOK expected '''Return this conic as a string. @kwarg prec: Number of (decimal) digits, unstripped (C{int}). @kwarg name: Override name (C{str}) or C{None} to exclude this conic's name. @return: Conic attributes (C{str}). ''' a = [name, prec, _lat0_, _lon0_, _par1_, _par2_, _E0_, _N0_, _k0_, _SP_] if self._SP == 1: _ = a.pop(a.index(_par2_)) return self._instr(datum=self.datum, *a) def _dup2(self, c): '''(INTERNAL) Copy this conic to C{c}. @arg c: Duplicate (L{Conic}). ''' _update_all(c) c._auth = self._auth c._datum = self._datum c._e = self._e c._E0 = self._E0 c._k0 = self._k0 c._N0 = self._N0 c._SP = self._SP c._par1 = self._par1 c._par2 = self._par2 c._phi0 = self._phi0 c._lam0 = self._lam0 c._opt3 = self._opt3 c._aF = self._aF c._n = self._n c._1_n = self._1_n c._r0 = self._r0 def _mdef(self, a): '''(INTERNAL) Compute m(a). ''' s, c = sincos2(a) s = _1_0 - (s * self._e)**2 return (c / sqrt(s)) if s > EPS02 else _0_0 def _pdef(self, a): '''(INTERNAL) Compute p(a). ''' s = self._e * sin(a) return pow((_1_0 - s) / (_1_0 + s), self._e * _0_5) def _rdef(self, t): '''(INTERNAL) Compute r(t). ''' return self._aF * pow(t, self._n) def _tdef(self, a): '''(INTERNAL) Compute t(lat). ''' return max(_0_0, tanPI_2_2(-a) / self._pdef(a)) def _xdef(self, t_x): '''(INTERNAL) Compute x(t_x). ''' return PI_2 - _2_0 * atan(t_x) # XXX + self._phi0 Conic._name = Conic.__name__ class Conics(_NamedEnum): '''(INTERNAL) L{Conic} registry, I{must} be a sub-class to accommodate the L{_LazyNamedEnumItem} properties. ''' def _Lazy(self, lat, lon, datum_name, *args, **kwds): '''(INTERNAL) Instantiate the L{Conic}. ''' return Conic(_LLEB(lat, lon, datum=Datums.get(datum_name)), *args, **kwds) Conics = Conics(Conic) # PYCHOK singleton '''Some pre-defined L{Conic}s, all I{lazily} instantiated.''' Conics._assert( # <https://SpatialReference.org/ref/sr-org/...> # AsLb = _lazy('AsLb', _F(-14.2666667), _F(170), _NAD27_, _0_0, _0_0, # E0=_F(500000), N0=_0_0, auth='EPSG:2155'), # American Samoa ... SP=1 ! Be08Lb = _lazy('Be08Lb', _F(50.7978150), _F(4.359215833), _GRS80_, _F(49.8333339), _F(51.1666672), E0=_F(649328.0), N0=_F(665262.0), auth='EPSG:9802'), # Belgium Be72Lb = _lazy('Be72Lb', _90_0, _F(4.3674867), _NAD83_, _F(49.8333339), _F(51.1666672), E0=_F(150000.013), N0=_F(5400088.438), auth='EPSG:31370'), # Belgium Fr93Lb = _lazy('Fr93Lb', _F(46.5), _F(3), _WGS84_, _F(49), _F(44), E0=_F(700000), N0=_F(6600000), auth='EPSG:2154'), # RFG93, France MaNLb = _lazy('MaNLb', _F(33.3), _F(-5.4), _NTF_, _F(31.73), _F(34.87), E0=_F(500000), N0=_F(300000)), # Marocco MxLb = _lazy('MxLb', _F(12), _F(-102), _WGS84_, _F(17.5), _F(29.5), E0=_F(2500000), N0=_0_0, auth='EPSG:2155'), # Mexico PyT_Lb = _lazy('PyT_Lb', _F(46.8), _F(2.33722917), _NTF_, _F(45.89893890000052), _F(47.69601440000037), E0=_F(600000), N0=_F(200000), auth='Test'), # France? USA_Lb = _lazy('USA_Lb', _F(23), _F(-96), _WGS84_, _F(33), _F(45), E0=_0_0, N0=_0_0), # Conterminous, contiguous USA? WRF_Lb = _lazy('WRF_Lb', _F(40), _F(-97), _WGS84_, _F(33), _F(45), E0=_0_0, N0=_0_0, auth='EPSG:4326') # World ) class LCCError(_ValueError): '''Lambert Conformal Conic C{LCC} or other L{Lcc} issue. ''' pass class Lcc(_NamedBase): '''Lambert conformal conic East-/Northing location. ''' _conic = Conics.WRF_Lb # Lambert projection (L{Conic}) _easting = _0_0 # Easting (C{float}) _height = 0 # height (C{meter}) _northing = _0_0 # Northing (C{float}) def __init__(self, e, n, h=0, conic=Conics.WRF_Lb, name=NN): '''New L{Lcc} Lamber conformal conic position. @arg e: Easting (C{meter}). @arg n: Northing (C{meter}). @kwarg h: Optional height (C{meter}). @kwarg conic: Optional, the conic projection (L{Conic}). @kwarg name: Optional name (C{str}). @return: The Lambert location (L{Lcc}). @raise LCCError: Invalid B{C{h}} or invalid or negative B{C{e}} or B{C{n}}. @raise TypeError: If B{C{conic}} is not L{Conic}. @example: >>> lb = Lcc(448251, 5411932.0001) ''' if conic not in (None, Lcc._conic): self.conic = conic self._easting = Easting(e, falsed=conic.E0 > 0, Error=LCCError) self._northing = Northing(n, falsed=conic.N0 > 0, Error=LCCError) if h: self._height = Height(h=h, Error=LCCError) if name: self.name = name @Property def conic(self): '''Get the conic projection (L{Conic}). ''' return self._conic @conic.setter # PYCHOK setter! def conic(self, conic): '''Set the conic projection. @arg conic: The projection (L{Conic}). @raise TypeError: Invalid B{C{conic}}. ''' _xinstanceof(Conic, conic=conic) if conic != self._conic: _update_all(self) self._conic = conic # def dup(self, name=NN, **e_n_h_conic): # PYCHOK signature # '''Duplicate this location with some attributes modified. # # @kwarg e_n_h_conic: Use keyword argument C{B{e}=...}, C{B{n}=...}, # C{B{h}=...} and/or C{B{conic}=...} to override # the current C{easting}, C{northing} C{height} # or C{conic} projection, respectively. # ''' # def _args_kwds(e=None, n=None, **kwds): # return (e, n), kwds # # kwds = _xkwds(e_n_h_conic, e=self.easting, n=self.northing, # h=self.height, conic=self.conic, # name=name or self.name) # args, kwds = _args_kwds(**kwds) # return self.__class__(*args, **kwds) # .classof @Property_RO def easting(self): '''Get the easting (C{meter}). ''' return self._easting @Property_RO def height(self): '''Get the height (C{meter}). ''' return self._height @Property_RO def latlon(self): '''Get the lat- and longitude in C{degrees} (L{LatLon2Tuple}). ''' ll = self.toLatLon(LatLon=None, datum=None) return LatLon2Tuple(ll.lat, ll.lon, name=self.name) @Property_RO def latlonheight(self): '''Get the lat-, longitude and height (L{LatLon3Tuple}C{(lat, lon, height)}). ''' return self.latlon.to3Tuple(self.height) @Property_RO def latlonheightdatum(self): '''Get the lat-, longitude in C{degrees} with height and datum (L{LatLon4Tuple}C{(lat, lon, height, datum)}). ''' return self.latlonheight.to4Tuple(self.conic.datum) @Property_RO def northing(self): '''Get the northing (C{meter}). ''' return self._northing @Property_RO def philam(self): '''Get the lat- and longitude in C{radians} (L{PhiLam2Tuple}). ''' return PhiLam2Tuple(radians(self.latlon.lat), radians(self.latlon.lon), name=self.name) @Property_RO def philamheight(self): '''Get the lat-, longitude in C{radians} and height (L{PhiLam3Tuple}C{(phi, lam, height)}). ''' return self.philam.to3Tuple(self.height) @Property_RO def philamheightdatum(self): '''Get the lat-, longitude in C{radians} with height and datum (L{PhiLam4Tuple}C{(phi, lam, height, datum)}). ''' return self.philamheight.to4Tuple(self.datum) @deprecated_method def to3lld(self, datum=None): # PYCHOK no cover '''DEPRECATED, use method C{toLatLon}. @kwarg datum: Optional datum to use, otherwise use this B{C{Lcc}}'s conic.datum (C{Datum}). @return: A L{LatLonDatum3Tuple}C{(lat, lon, datum)}. @raise TypeError: If B{C{datum}} is not ellipsoidal. ''' if datum in (None, self.conic.datum): r = LatLonDatum3Tuple(self.latlon.lat, self.latlon.lon, self.conic.datum, name=self.name) else: r = self.toLatLon(LatLon=None, datum=datum) r = LatLonDatum3Tuple(r.lat, r.lon, r.datum, name=r.name) return r def toLatLon(self, LatLon=None, datum=None, height=None, **LatLon_kwds): '''Convert this L{Lcc} to an (ellipsoidal) geodetic point. @kwarg LatLon: Optional, ellipsoidal class to return the geodetic point (C{LatLon}) or C{None}. @kwarg datum: Optional datum to use, otherwise use this B{C{Lcc}}'s conic.datum (L{Datum}, L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}). @kwarg height: Optional height for the point, overriding the default height (C{meter}). @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword arguments, ignored if C{B{LatLon} is None}. @return: The point (B{C{LatLon}}) or a L{LatLon4Tuple}C{(lat, lon, height, datum)} if B{C{LatLon}} is C{None}. @raise TypeError: If B{C{LatLon}} or B{C{datum}} is not ellipsoidal or not valid. ''' if LatLon: _xsubclassof(_LLEB, LatLon=LatLon) c = self.conic if datum not in (None, self.conic.datum): c = c.toDatum(datum) e = self.easting - c._E0 n = c._r0 - self.northing + c._N0 r_ = copysign0(hypot(e, n), c._n) t_ = pow(r_ / c._aF, c._1_n) x = c._xdef(t_) # XXX c._lam0 for self._iteration in range(10): # max 4 trips p, x = x, c._xdef(t_ * c._pdef(x)) if abs(x - p) < 1e-9: # XXX EPS too small? break lat = degrees90(x) lon = degrees180((atan(e / n) + c._opt3) * c._1_n + c._lam0) h = self.height if height is None else Height(height) return _LL4Tuple(lat, lon, h, c.datum, LatLon, LatLon_kwds, inst=self, name=self.name) def toRepr(self, prec=0, fmt=Fmt.SQUARE, sep=_COMMASPACE_, m=_m_, C=False, **unused): # PYCHOK expected '''Return a string representation of this L{Lcc} position. @kwarg prec: Number of (decimal) digits, unstripped (C{int}). @kwarg fmt: Enclosing backets format (C{str}). @kwarg sep: Optional separator between name:values (C{str}). @kwarg m: Optional unit of the height, default meter (C{str}). @kwarg C: Optionally, include name of conic and datum (C{bool}). @return: This Lcc as "[E:meter, N:meter, H:m, C:Conic.Datum]" (C{str}). ''' t, T = _fstrENH2(self, prec, m) if C: t += self.conic.name2, T += _C_, return _xzipairs(T, t, sep=sep, fmt=fmt) def toStr(self, prec=0, sep=_SPACE_, m=_m_): # PYCHOK expected '''Return a string representation of this L{Lcc} position. @kwarg prec: Number of (decimal) digits, unstripped (C{int}). @kwarg sep: Optional separator to join (C{str}) or C{None} to return an unjoined C{tuple} of C{str}s. @kwarg m: Optional height units, default C{meter} (C{str}). @return: This Lcc as I{"easting nothing"} in C{meter} plus I{" height"} suffixed with B{C{m}} if height is non-zero (C{str}). ''' t, _ = _fstrENH2(self, prec, m) return t if sep is None else sep.join(t) def toLcc(latlon, conic=Conics.WRF_Lb, height=None, Lcc=Lcc, name=NN, **Lcc_kwds): '''Convert an (ellipsoidal) geodetic point to a I{Lambert} location. @arg latlon: Ellipsoidal point (C{LatLon}). @kwarg conic: Optional Lambert projection to use (L{Conic}). @kwarg height: Optional height for the point, overriding the default height (C{meter}). @kwarg Lcc: Optional class to return the I{Lambert} location (L{Lcc}). @kwarg name: Optional B{C{Lcc}} name (C{str}). @kwarg Lcc_kwds: Optional, additional B{C{Lcc}} keyword arguments, ignored if B{C{Lcc}} is C{None}. @return: The I{Lambert} location (L{Lcc}) or an L{EasNor3Tuple}C{(easting, northing, height)} if C{B{Lcc} is None}. @raise TypeError: If B{C{latlon}} is not ellipsoidal. ''' _xinstanceof(_LLEB, latlon=latlon) a, b = latlon.philam c = conic.toDatum(latlon.datum) t = c._n * (b - c._lam0) - c._opt3 st, ct = sincos2(t) r = c._rdef(c._tdef(a)) e = c._E0 + r * st n = c._N0 + c._r0 - r * ct h = latlon.height if height is None else Height(height) r = EasNor3Tuple(e, n, h) if Lcc is None else \ Lcc(e, n, h=h, conic=c, **Lcc_kwds) return _xnamed(r, name or nameof(latlon)) if __name__ == '__main__': from pygeodesy.interns import _NL_, _NL_var_ # __doc__ of this file, force all into registery t = _NL_ + Conics.toRepr(all=True) print(_NL_var_.join(t.split(_NL_))) # **) MIT License # # Copyright (C) 2016-2022 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.