### Navigation

- index
- modules |
- modules |
- FNSS 0.6.0 documentation »
- Module code »

# Source code for fnss.adapters.jfed

    """Adapter for jFed

    Provides function to convert an FNSS Topology object into a jFed
    rspec file and viceversa.

    `jFed <http://jfed.iminds.be/>_` is a Java-based framework to support the
    integration of federated testbed, developed by
    `iMinds <http://www.iminds.be/>_` in the contex of the
    `Fed4FIRE <http://www.fed4fire.eu/>_` project funded by the Framework
    Programme 7 (FP7) of the European Union.
    """
    from __future__ import division
    import xml.etree.cElementTree as ET

    import networkx as nx

    from fnss import Topology, get_delays, get_capacities
    import fnss.util as util
    import fnss.units as units

    __all__ = ['to_jfed', 'from_jfed']

    def to_jfed(topology, path, testbed="wall1.ilabt.iminds.be", encoding="utf-8", prettyprint=True):
        """Convert a topology object into an RSPEC file for jFed

        Parameters
        ----------
        topology : Topology
            The topology object
        path : str
            The file to which the RSPEC will be written
        testbed : str, optional
            URI of the testbed to use
        encoding : str, optional
            The encoding of the target file
        prettyprint : bool, optional
            Indent the XML code in the output file

        Notes
        -----
        It currently supports only undirected topologies, if a topology is directed
        it is converted to undirected
        """
        if topology.is_directed():
            topology = topology.to_undirected()
        topology = nx.convert_node_labels_to_integers(topology)

        if 'capacity_unit' in topology.graph:
            capacity_norm = units.capacity_units[topology.graph['capacity_unit']]/units.capacity_units['Kbps']
        if 'delay_unit' in topology.graph:
            delay_norm = units.time_units[topology.graph['delay_unit']]/units.time_units['ms']
        delays = get_delays(topology)
        capacities = get_capacities(topology)
        # Node positions (randomly generated)
        pos = nx.random_layout(topology)
        # Create mapping between links and interface IDs
        if_names = {}
        for v in topology.edge:
            next_hops = sorted(topology.edge[v].keys())
            if_names[v] = dict((next_hops[i], i) for i in range(len(next_hops)))
        head = ET.Element('rspec')
        head.attrib["generated_by"]= "FNSS"
        head.attrib['xsi:schemaLocation'] = "http://www.geni.net/resources/rspec/3 http://www.geni.net/resources/rspec/3/request.xsd"
        head.attrib['xmlns'] = "http://www.geni.net/resources/rspec/3"
        head.attrib["xmlns:jFed"] = "http://jfed.iminds.be/rspec/ext/jfed/1"
        head.attrib["xmlns:jFedBonfire"] = "http://jfed.iminds.be/rspec/ext/jfed-bonfire/1"
        head.attrib["xmlns:delay"] = "http://www.protogeni.net/resources/rspec/ext/delay/1"
        head.attrib["xmlns:xsi"] = "http://www.w3.org/2001/XMLSchema-instance"
        # Iterate over nodes
        for v in topology.nodes_iter():
            node = ET.SubElement(head, 'node')
            node.attrib['client_id'] = "node%s" % str(v)
            node.attrib['component_manager_id'] = "urn:publicid:IDN+%s+authority+cm" % testbed
            node.attrib["exclusive"] = "true"
            sliver_type = ET.SubElement(node, 'sliver_type')
            sliver_type.attrib['name'] = topology.node[v]['sliver_type'] if 'sliver_type' in topology.node[v] else 'raw-pc'
            location = ET.SubElement(node, 'jFed:location')
            x, y = pos[v]
            location.attrib['x'] = str(1000*x)
            location.attrib['y'] = str(500*y)
            for if_name in if_names[v].values():
                interface = ET.SubElement(node, 'interface')
                interface.attrib['client_id'] = "node%s:if%s" % (str(v), str(if_name))
        # The convention in jFed is to identify links with "linkX" where X is an
        # integer but making sure that links and nodes have different integers
        link_id = topology.number_of_nodes() - 1
        for u, v in topology.edges_iter():
            link_id += 1
            link = ET.SubElement(head, 'link')
            link.attrib['client_id'] = "link%s" % str(link_id)
            component_manager =  ET.SubElement(link, 'component_manager')
            component_manager.attrib['name'] = "urn:publicid:IDN+%s+authority+cm" % testbed
            u_if = "node%s:if%s" % (str(u), str(if_names[u][v]))
            v_if = "node%s:if%s" % (str(v), str(if_names[v][u]))
            for source, dest in ((u_if, v_if), (v_if, u_if)):
                prop = ET.SubElement(link, 'property')
                prop.attrib["source_id"] = source
                prop.attrib["dest_id"] = dest
                if (u, v) in delays:
                    prop.attrib['latency'] = str(delay_norm*delays[(u, v)])
                if (u, v) in capacities:
                    prop.attrib['capacity'] = str(capacity_norm*capacities[(u, v)])
                interface_ref = ET.SubElement(link, 'interface_ref')
                interface_ref.attrib['client_id'] = source
        if prettyprint:
            util.xml_indent(head)
        ET.ElementTree(head).write(path, encoding=encoding)

    def from_jfed(path):
        """Read a jFed RSPEC file and returns an FNSS topology modelling the
        network topology of the jFed experiment specification.

        Parameters
        ----------
        path : str
            The path of the jFed RSPEC file to parse

        Returns
        -------
        topology: Topology
            The parsed topology

        Notes
        -----
        This function does not support directed topologies and unidirectional links

        It is possible in jFed to create multipoint links (links with more than 2
        endpoints). Such types of link cannot be modelled in FNSS. Therefore, any
        attempt to convert an RSPEC with such links will fail.
        """
        # This implementation could be improved by using SOAP libraries, but it
        # would require to add another dependency to the project.
        # The current implementation, although not really elegant, works fine
        tree = ET.parse(path)
        head = tree.getroot()
        xmlns = "http://www.geni.net/resources/rspec/3"
        topology = Topology()
        # Flags to indicate whether the parsed topology is annotated with
        # capacities and delays
        has_delays = False
        has_capacities = False
        # Dict mapping interface name to the node it belongs to
        if_map = {}
        # Iterate over nodes
        for node in head.findall('{%s}node' % xmlns):
            client_id = node.attrib['client_id']
            component_manager_id = node.attrib['component_manager_id']
            exclusive = bool(node.attrib['exclusive'])
            for interface in node.findall('{%s}interface' % xmlns):
                if_id = interface.attrib['client_id']
                if_map[if_id] = client_id
            topology.add_node(client_id,
                              component_manager_id=component_manager_id,
                              exclusive=exclusive)
        # Iterate over links
        for edge in head.findall('{%s}link' % xmlns):
            client_id = edge.attrib['client_id']
            component_manager = edge.find('{%s}component_manager' % xmlns).attrib['name']
            interfaces = edge.findall('{%s}interface_ref' % xmlns)
            # A link may connect more than two nodes. These links cannot be
            # represented in an FNSS Topology.
            # This statement also encompasses the potential case of one interface
            # only that should not happen if the file is correctly formatted.
            if len(interfaces) != 2:
                raise ValueError("Link %s is not a point-to-point link but a shared "
                                 "medium connecting %d interfaces. These links are "
                                 "not supported. Change your topology and try again"
                                 % (client_id, len(interfaces)))
            u = if_map[interfaces[0].attrib['client_id']]
            v = if_map[interfaces[1].attrib['client_id']]
            edge_attr = dict(component_manager=component_manager,
                             client_id=client_id)
            # There are normally two property tags per edge. We only parse one
            # because should have same attributes if links are bidirectional.
            # This function does not support unidirectional links
            prop = edge.find('{%s}property' % xmlns)
            if prop:
                if 'capacity' in prop.attrib:
                    edge_attr['capacity'] = prop.attrib['capacity']
                    has_capacities = True
                if 'latency' in prop.attrib:
                    edge_attr['delay'] = prop.attrib['latency']
                    has_delays = True
            topology.add_edge(u, v, edge_attr)
        # Set capacity and delay units
        if has_capacities:
            topology.graph['capacity_unit'] = 'kbps'
        if has_delays:
            topology.graph['delay_unit'] = 'ms'
        return topology

### Navigation

- index
- modules |
- modules |
- FNSS 0.6.0 documentation »
- Module code »