### Navigation

- index
- modules |
- modules |
- FNSS 0.6.0 documentation »
- Module code »

# Source code for fnss.netconfig.delays

    """
    Provides functions to assign and manipulate link delays.
    """
    import networkx as nx
    from fnss.units import time_units, distance_units

    __all__ = [
        'PROPAGATION_DELAY_VACUUM',
        'PROPAGATION_DELAY_FIBER',
        'set_delays_constant',
        'set_delays_geo_distance',
        'get_delays',
        'clear_delays'
               ]

    # Propagation delay of light in the vacuum
    PROPAGATION_DELAY_VACUUM = 1.0/300 # ms/Km

    # Propagation delay of light in an average optical fiber
    PROPAGATION_DELAY_FIBER = 0.005 # ms/Km

    def set_delays_constant(topology, delay=1.0, delay_unit='ms', links=None):
        """
        Assign a constant delay to all selected links

        Parameters
        ----------
        topology : Topology
            The topology on which delays are applied.
        delay : float, optional
            The constant delay to be applied to all links
        delay_unit : string, optional
            The unit of delays. Supported units are: "us" (microseconds), "ms"
            (milliseconds) and "s" (seconds)
        links : list, optional
            List of selected links on which weights are applied. If it is None,
            all links are selected

        Examples
        --------
        >>> import fnss
        >>> topology = fnss.Topology()
        >>> topology.add_path([1, 2, 4, 5, 8])
        >>> fnss.set_delays_constant(topology, 5.0, 'ms', links=[(1,2), (5,8), (4,5)])
        >>> delay = fnss.get_delays(topology)
        >>> delay[(1, 2)]
        5.0
        """
        if not delay_unit in time_units:
            raise ValueError("The delay_unit argument is not valid")
        conversion_factor = 1
        if 'delay_unit' in topology.graph and links is not None:
            # If a delay_unit is set, that means that some links have already
            # been assigned delays, so set these delay using the same unit
            # already used
            curr_delay_unit = topology.graph['delay_unit']
            if curr_delay_unit != delay_unit:
                conversion_factor = float(time_units[delay_unit]) \
                                    / time_units[curr_delay_unit]
        else:
            topology.graph['delay_unit'] = delay_unit
        edges = topology.edges_iter() if links is None else links
        for u, v in edges:
            topology.edge[u][v]['delay'] = delay * conversion_factor

    def set_delays_geo_distance(topology, specific_delay, default_delay=None,
                                delay_unit='ms', links=None):
        """
        Assign a delay to all selected links equal to the product of link length
        and specific delay. To use this function, all nodes must have a 'latitude'
        and a 'longitude' attribute. Alternatively, all links of the topology must
        have a 'length' attribute. If the length of a link cannot be determined, it
        is applied the delay equal default_delay if specified, otherwise an error
        is returned.

        Parameters
        ----------
        topology : Topology
            The topology on which delays are applied.
        specific_delay : float
            The specific delay (in ms/Km) to be applied to all links
        default_delay : float, optional
            The delay to be applied to links whose length is not known. If None, if
            the length of a link cannot be determined, an error is returned
        delay_unit : string, optional
            The unit of delays. Supported units are: "us" (microseconds), "ms"
            (milliseconds) and "s" (seconds)
        links : list, optional
            List of selected links on which weights are applied. If it is None, all
            links are selected

        Examples
        --------
        >>> import fnss
        >>> topology = fnss.parse_abilene('abilene_topo.txt')
        >>> fnss.set_delays_geo_distance(topology, specific_delay=fnss.PROPAGATION_DELAY_FIBER)
        """
        # Validate input parameters
        if not delay_unit in time_units:
            raise ValueError("The delay_unit argument is not valid")
        if not 'distance_unit' in topology.graph:
            raise ValueError("The provided topology does not have a "\
                             "distance_unit attribute")
        distance_unit = topology.graph['distance_unit']
        if distance_unit not in distance_units:
            raise ValueError("The distance_unit attribute of the provided "\
                             "topology (%s) is not valid" % distance_unit)
        edges = topology.edges() if links is None else links
        if default_delay is None:
            if any(('length' not in topology.edge[u][v] for u, v in edges)):
                raise ValueError('All links must have a length attribute')
        if 'delay_unit' in topology.graph and links is not None:
            # If a delay_unit is set, that means that some links have already
            # been assigned delays, so set these delays using the same unit
            # already used instead of the delay unit provided as argument
            curr_delay_unit = topology.graph['delay_unit']
            conv_factor = 1.0/time_units[curr_delay_unit]
        else:
            topology.graph['delay_unit'] = delay_unit
            curr_delay_unit = delay_unit # used in case of default delay assignment
            conv_factor = 1.0/time_units[delay_unit]
        # factor to convert length value in Km
        length_conv_factor = distance_units[distance_unit]
        # factor to convert default delay in target delay unit
        default_conv_factor = time_units[delay_unit] / time_units[curr_delay_unit]
        for u, v in edges:
            if 'length' in topology.edge[u][v]:
                length = topology.edge[u][v]['length'] * length_conv_factor
                delay = specific_delay * length * conv_factor
            else:
                delay = default_delay * default_conv_factor
            topology.edge[u][v]['delay'] = delay

    def get_delays(topology):
        """
        Returns all the delays.

        Parameters
        ----------
        topology : Topology
            The topology whose link delays are requested

        Returns
        -------
        delays : dict
            Dictionary of link delays keyed by link.

        Examples
        --------
        >>> import fnss
        >>> topology = fnss.Topology()
        >>> topology.add_path([1,2,3])
        >>> fnss.set_delays_constant(topology, 10, 'ms')
        >>> delay = get_delays(topology)
        >>> delay[(1,2)]
        10
        """
        return nx.get_edge_attributes(topology, 'delay')

    def clear_delays(topology):
        """
        Remove all delays from the topology.

        Parameters
        ----------
        topology : Topology

        """
        if 'delay_unit' in topology.graph:
            del topology.graph['delay_unit']
        for u, v in topology.edges_iter():
            if 'delay' in topology.edge[u][v]:
                del topology.edge[u][v]['delay']

### Navigation

- index
- modules |
- modules |
- FNSS 0.6.0 documentation »
- Module code »