# Coverage for pygeodesy/geodesicx/gxarea.py : 90%

## 228 statements 206 run 22 missing 23 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 | # -*- coding: utf-8 -*- u'''Slightly enhanced versions of I{Karney}'s Python classes U{PolygonArea<https://GeographicLib.SourceForge.io/1.50/python/ code.html#module-geographiclib.polygonarea>} and C{Accumulator}. Class L{GeodesicAreaExact} is intended to work with instances of class L{GeodesicExact} or of I{wrapped} class C{Geodesic} I{Karney}'s Python U{geographiclib <https://GeographicLib.SourceForge.io/1.50/python/index.html>} Copyright (C) Charles Karney (2012-2019) <Charles@Karney.com> and licensed under the MIT/X11 License. For more information, see U{GeographicLib<https://GeographicLib.SourceForge.io>}. ''' # make sure int/int division yields float quotient from __future__ import division from pygeodesy.basics import unsign0 from pygeodesy.interns import NAN, NN, _COMMASPACE_, \ _0_0, _2_0 from pygeodesy.karney import GeodesicError, _diff182, \ _norm180, _remainder, _3sum2 from pygeodesy.lazily import _ALL_DOCS, printf from pygeodesy.named import callername, _Dict, _NamedBase, pairs from pygeodesy.props import Property, Property_RO, property_RO # from pygeodesy.streprs import pairs # from .named from math import fmod __all__ = () __version__ = '21.05.29' class GeodesicAreaExact(_NamedBase): '''Area and perimeter of a geodesic polygon, an enhanced version of I{Karney}'s Python class U{PolygonArea <https://GeographicLib.SourceForge.io/html/python/ code.html#module-geographiclib.polygonarea>} using the more accurate surface area. @note: The name of this class C{*Exact} is a misnomer, see I{Karney}'s comments at C++ attribute U{GeodesicExact._c2 <https://GeographicLib.SourceForge.io/html/ GeodesicExact_8cpp_source.html>}. ''' _Area = None _g_gX = None # Exact or not _lat0 = _lon0 = \ _lat1 = _lon1 = NAN _mask = 0 _num = 0 _Peri = None _verbose = False _xings = 0 def __init__(self, geodesic, polyline=False, name=NN): '''New L{GeodesicAreaExact} instance. @arg geodesic: A geodesic (L{GeodesicExact}, I{wrapped} C{Geodesic} or L{GeodesicSolve}). @kwarg polyline: If C{True} compute perimeter only, otherwise area and perimeter (C{bool}). @kwarg name: Optional name (C{str}). @raise GeodesicError: Invalid B{C{geodesic}}. ''' try: # results returned as L{GDict} if not (callable(geodesic._GDictDirect) and callable(geodesic._GDictInverse)): raise TypeError except (AttributeError, TypeError): raise GeodesicError(geodesic=geodesic) self._g_gX = g = geodesic # use the class-level Caps since the values # differ between GeodesicExact and Geodesic self._mask = g.DISTANCE | g.LATITUDE | g.LONGITUDE self._Peri = _Accumulator(name='_Peri') if not polyline: # perimeter and area self._mask |= g.AREA | g.LONG_UNROLL self._Area = _Accumulator(name='_Area') if g.debug: # inherit debug as verbosity self.verbose = True if name: self.name = name def AddEdge(self, azi, s): '''Add another polygon edge. @arg azi: Azimuth at the current point (compass C{degrees}). @arg s: Length of the edge (C{meter}). ''' if self.num < 1: raise GeodesicError(num=self.num) r = self._Direct(azi, s) p = self._Peri.Add(s) if self._Area: a = self._Area.Add(r.S12) self._xings += r.xing else: a = _0_0 self._lat1 = r.lat2 self._lon1 = r.lon2 self._num += 1 if self.verbose: # PYCHOK no cover self._print(self.num, p, a, r, lat1=r.lat2, lon1=r.lon2, azi=azi, s=s) return self.num def AddPoint(self, lat, lon): '''Add another polygon point. @arg lat: Latitude of the point (C{degrees}). @arg lon: Longitude of the point (C{degrees}). ''' if self.num > 0: r = self._Inverse(self.lat1, self.lon1, lat, lon) s = r.s12 p = self._Peri.Add(s) if self._Area: a = self._Area.Add(r.S12) self._xings += r.xing else: a = _0_0 else: self._lat0 = lat self._lon0 = lon a = p = s = _0_0 r = None self._lat1 = lat self._lon1 = lon self._num += 1 if self.verbose: # PYCHOK no cover self._print(self.num, p, a, r, lat1=lat, lon1=lon, s=s) return self.num @Property_RO def area0x(self): '''Get the ellipsoid's surface area (C{meter} I{squared}), more accurate for very I{oblate} ellipsoids. ''' return self.ellipsoid.areax # not .area! area0 = area0x # for C{geographiclib} compatibility @Property_RO def _area0x_2(self): '''Get half the ellipsoid's surface area (C{meter} I{squared}). ''' return self.area0x / _2_0 def Compute(self, reverse=False, sign=True): '''Compute the accumulated perimeter and area. @kwarg reverse: If C{True}, clockwise traversal counts as a positive area instead of counter-clockwise (C{bool}). @kwarg sign: If C{True}, return a signed result for the area if the polygon is traversed in the "wrong" direction instead of returning the area for the rest of the earth. @return: 3-Tuple C{(number, perimeter (meter), area (meter*2))}. The C{perimeter} includes the length of a final edge, connecting the current to the initial point, if this polygon was initialized with C{polyline=False}. And C{area=NAN} for perimeter only, C{polyline=True}. @note: Arbitrarily complex polygons are allowed. In the case of self-intersecting polygons, the area is accumulated "algebraically". E.g., the areas of the 2 loops in a I{figure-8} polygon will partially cancel. @note: More points and edges can be added after this call. ''' n = self.num if n < 2: p = _0_0 a = NAN if self.polyline else _0_0 r = None elif self._Area: r = self._Inverse(self.lat1, self.lon1, self.lat0, self.lon0) p = self._Peri.Sum(r.s12) A = _Accumulator(self._Area.Sum(r.S12)) a = self._reduce(A, reverse, sign, r.xing) else: p = self._Peri.Sum() a = NAN r = None if self.verbose: # PYCHOK no cover self._print(n, p, a, r, lat0=self.lat0, lon0=self.lon0) return n, p, a def _Direct(self, azi, s): '''(INTERNAL) Edge helper. ''' lon1 = self.lon1 r = self._g_gX._GDictDirect(self.lat1, lon1, azi, False, s, self._mask) if self._Area: # aka transitDirect # Count crossings of prime meridian exactly as # int(ceil(lon2 / 360)) - int(ceil(lon1 / 360)) # Since we only need the parity of the result we # can use std::remquo but this is buggy with g++ # 4.8.3 and requires C++11. So instead we do: lon1 = fmod( lon1, 720) # r.lon1 lon2 = fmod(r.lon2, 720) # int(True) == 1, int(False) == 0 r.set_(xing=int(lon2 > 360 or -360 < lon2 <= 0) - int(lon1 > 360 or -360 < lon1 <= 0)) return r @Property_RO def ellipsoid(self): '''Get this area's ellipsoid (C{Ellipsoid[2]}). ''' return self._g_gX.ellipsoid @Property_RO def geodesic(self): '''Get this area's geodesic object (C{Geodesic[Exact]}). ''' return self._g_gX earth = geodesic # for C{geographiclib} compatibility def _Inverse(self, lat1, lon1, lat2, lon2): '''(INTERNAL) Point helper. ''' r = self._g_gX._GDictInverse(lat1, lon1, lat2, lon2, self._mask) if self._Area: # aka transit # count crossings of prime meridian as +1 or -1 # if in east or west direction, otherwise 0 lon1 = _norm180(lon1) lon2 = _norm180(lon2) lon12, _ = _diff182(lon1, lon2) r.set_(xing=int(lon1 <= 0 and lon2 > 0 and lon12 > 0) or -int(lon2 <= 0 and lon1 > 0 and lon12 < 0)) return r @property_RO def lat0(self): '''Get the first point's latitude (C{degrees}). ''' return self._lat0 @property_RO def lat1(self): '''Get the most recent point's latitude (C{degrees}). ''' return self._lat1 @property_RO def lon0(self): '''Get the first point's longitude (C{degrees}). ''' return self._lon0 @property_RO def lon1(self): '''Get the most recent point's longitude (C{degrees}). ''' return self._lon1 @property_RO def num(self): '''Get the current number of points (C{int}). ''' return self._num @Property_RO def polyline(self): '''Is this perimter only (C{boo}), area NAN? ''' return self._Area is None def _print(self, n, p, a, r, **kwds): # PYCHOK no cover '''(INTERNAL) Print a verbose line. ''' d = _Dict(p=p, s12=r.s12 if r else NAN, **kwds) if self._Area: d.set_(a=a, S12=r.S12 if r else NAN) t = _COMMASPACE_.join(pairs(d, prec=10)) printf('%s %s: %s (%s)', self.named2, n, t, callername(up=2)) def _reduce(self, Area, reverse, sign, xing): '''(INTERNAL) Reduce accumulated area to allowed range. ''' a0, a0_2 = self.area0x, self._area0x_2 a = Area.Remainder(a0) if ((self._xings + xing) & 1): a = Area.Add(a0_2 if a < 0 else -a0_2) # area is with the clockwise sense. If !reverse # convert to counter-clockwise convention. if not reverse: a = Area.Negate() # If sign put area in (-area0x/2, area0x/2], # otherwise put area in [0, area0x) if a > (a0 if sign else a0_2): a = Area.Add(-a0) elif a <= -(a0 if sign else a0_2): a = Area.Add( a0) return unsign0(a) def Reset(self): '''Reset this polygon to empty. ''' if self._Area: self._Area.Reset() self._Peri.Reset() self._lat0 = self._lon0 = \ self._lat1 = self._lon1 = NAN self._num = self._xings = n = 0 if self.verbose: # PYCHOK no cover printf('%s %s: (%s)', self.named2, n, self.Reset.__name__) return n Clear = Reset def TestEdge(self, azi, s, reverse=False, sign=True): '''Compute the properties for a tentative, additional edge @arg azi: Azimuth at the current the point (compass C{degrees}). @arg s: Length of the edge (C{meter}). @kwarg reverse: If C{True}, clockwise traversal counts as a positive area instead of counter-clockwise (C{bool}). @kwarg sign: If C{True}, return a signed result for the area if the polygon is traversed in the "wrong" direction instead of returning the area for the rest of the earth. @return: 3-Tuple C{(number, perimeter (meter), area (meter*2))}. @raise GeodesicError: No points. ''' n = self.num + 1 p = self._Peri.Sum(s) if self.polyline: a, r = NAN, None elif n < 2: raise GeodesicError(num=self.num) else: r = self._Direct(azi, s) a = self._Area.Sum(r.S12) x = r.xing r = self._Inverse(r.lat2, r.lon2, self.lat0, self.lon0) A = _Accumulator(a + r.S12) a = self._reduce(A, reverse, sign, x + r.xing) p += r.s12 if self.verbose: # PYCHOK no cover self._print(n, p, a, r, azi=azi, s=s) return n, p, a def TestPoint(self, lat, lon, reverse=False, sign=True): '''Compute the properties for a tentative, additional vertex @arg lat: Latitude of the point (C{degrees}). @arg lon: Longitude of the point (C{degrees}). @kwarg reverse: If C{True}, clockwise traversal counts as a positive area instead of counter-clockwise (C{bool}). @kwarg sign: If C{True}, return a signed result for the area if the polygon is traversed in the "wrong" direction instead of returning the area for the rest of the earth. @return: 3-Tuple C{(number, perimeter (meter), area (meter*2))}. ''' n = self.num + 1 if n < 2: p = _0_0 a = NAN if self.polyline else _0_0 r = None else: r = self._Inverse(self.lat1, self.lon1, lat, lon) p = self._Peri.Sum(r.s12) if self._Area: a = self._Area.Sum(r.S12) x = r.xing r = self._Inverse(lat, lon, self.lat0, self.lon0) p += r.s12 A = _Accumulator(a + r.S12) a = self._reduce(A, reverse, sign, x + r.xing) else: a, r = NAN, None if self.verbose: # PYCHOK no cover self._print(n, p, a, r, lat=lat, lon=lon) return n, p, a def toStr(self, prec=6, sep=_COMMASPACE_, **unused): # PYCHOK signature '''Return this C{GeodesicExactArea} as string. @kwarg prec: The C{float} precision, number of decimal digits (0..9). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}} values. @kwarg sep: Optional separator to join (C{str}). @return: Area items (C{str}). ''' n, p, a = self.Compute() d = dict(geodesic=self.geodesic, num=n, area=a, perimeter=p, polyline=self.polyline) return sep.join(pairs(d, prec=prec)) @Property def verbose(self): '''Get the C{verbose} option (C{bool}). ''' return self._verbose @verbose.setter # PYCHOK setter! def verbose(self, verbose): '''Set the C{verbose} option. @arg verbose: Print a message after each method invokation (C{bool}). ''' self._verbose = bool(verbose) class PolygonArea(GeodesicAreaExact): '''For C{geographiclib} compatibility, sub-class of L{GeodesicAreaExact}. ''' def __init__(self, earth, polyline=False, name=NN): '''New L{PolygonArea} instance. @arg earth: A geodesic (L{GeodesicExact}, I{wrapped} C{Geodesic} or L{GeodesicSolve}). @kwarg polyline: If C{True} perimeter only, otherwise area and perimeter (C{bool}). @kwarg name: Optional name (C{str}). @raise GeodesicError: Invalid B{C{earth}}. ''' GeodesicAreaExact.__init__(self, earth, polyline=polyline, name=name) class _Accumulator(_NamedBase): '''Like C{math.fsum}, but allowing a running sum. Original from I{Karney}'s U{geographiclib <https://PyPI.org/project/geographiclib>}C{.accumulator}, enhanced to return the current sum by most methods. ''' _n = 0 # len() _s = _t = _0_0 def __init__(self, y=0, name=NN): '''New L{_Accumulator}. ''' if isinstance(y, _Accumulator): self._s, self._t, self._n = y._s, y._t, 1 elif y: self._s, self._n = float(y), 1 if name: self.name = name def Add(self, y): '''Add a value. @return: Current C{sum}. ''' self._n += 1 self._s, self._t = _3sum2(self._s, self._t, y) return self._s # current .Sum() def Negate(self): '''Negate sum. @return: Current C{sum}. ''' self._s = s = -self._s self._t = -self._t return s # current .Sum() @property_RO def num(self): '''Get the current number of C{Add}itions (C{int}). ''' return self._n def Remainder(self, y): '''Remainder on division by B{C{y}}. @return: Current C{sum} / B{C{y}}. ''' _remainder(self._s, y) self._n = -1 return self.Add(_0_0) def Reset(self, y=0): '''Set value from argument. ''' self._n, self._s, self._t = 0, float(y), _0_0 Set = Reset def Sum(self, y=0): '''Return C{sum + B{y}}. @note: B{C{y}} is included in the returned result, but I{not} accumulated. ''' if y: s = _Accumulator(self, name='_Sum') s.Add(y) else: s = self return s._s def toStr(self, prec=6, sep=_COMMASPACE_, **unused): # PYCHOK signature '''Return this C{_Accumulator} as string. @kwarg prec: The C{float} precision, number of decimal digits (0..9). Trailing zero decimals are stripped for B{C{prec}} values of 1 and above, but kept for negative B{C{prec}} values. @kwarg sep: Optional separator to join (C{str}). @return: Accumulator (C{str}). ''' d = dict(n=self.num, s=self._s, t=self._t) return sep.join(pairs(d, prec=prec)) __all__ += _ALL_DOCS(GeodesicAreaExact, PolygonArea) # **) MIT License # # Copyright (C) 2016-2021 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE.