# Coverage for pygeodesy/lcc.py : 97%

## 231 statements 224 run 7 missing 13 excluded

Hot-keys on this page

r m x p toggle line displays

j k next/prev highlighted chunk

0 (zero) top of page

1 (one) first highlighted chunk

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18 19 20 21 22 23 24 25 26 27 28 29 30 31 32 33 34 35 36 37 38 39 40 41 42 43 44 45 46 47 48 49 50 51 52 53 54 55 56 57 58 59 60 61 62 63 64 65 66 67 68 69 70 71 72 73 74 75 76 77 78 79 80 81 82 83 84 85 86 87 88 89 90 91 92 93 94 95 96 97 98 99 100 101 102 103 104 105 106 107 108 109 110 111 112 113 114 115 116 117 118 119 120 121 122 123 124 125 126 127 128 129 130 131 132 133 134 135 136 137 138 139 140 141 142 143 144 145 146 147 148 149 150 151 152 153 154 155 156 157 158 159 160 161 162 163 164 165 166 167 168 169 170 171 172 173 174 175 176 177 178 179 180 181 182 183 184 185 186 187 188 189 190 191 192 193 194 195 196 197 198 199 200 201 202 203 204 205 206 207 208 209 210 211 212 213 214 215 216 217 218 219 220 221 222 223 224 225 226 227 228 229 230 231 232 233 234 235 236 237 238 239 240 241 242 243 244 245 246 247 248 249 250 251 252 253 254 255 256 257 258 259 260 261 262 263 264 265 266 267 268 269 270 271 272 273 274 275 276 277 278 279 280 281 282 283 284 285 286 287 288 289 290 291 292 293 294 295 296 297 298 299 300 301 302 303 304 305 306 307 308 309 310 311 312 313 314 315 316 317 318 319 320 321 322 323 324 325 326 327 328 329 330 331 332 333 334 335 336 337 338 339 340 341 342 343 344 345 346 347 348 349 350 351 352 353 354 355 356 357 358 359 360 361 362 363 364 365 366 367 368 369 370 371 372 373 374 375 376 377 378 379 380 381 382 383 384 385 386 387 388 389 390 391 392 393 394 395 396 397 398 399 400 401 402 403 404 405 406 407 408 409 410 411 412 413 414 415 416 417 418 419 420 421 422 423 424 425 426 427 428 429 430 431 432 433 434 435 436 437 438 439 440 441 442 443 444 445 446 447 448 449 450 451 452 453 454 455 456 457 458 459 460 461 462 463 464 465 466 467 468 469 470 471 472 473 474 475 476 477 478 479 480 481 482 483 484 485 486 487 488 489 490 491 492 493 494 495 496 497 498 499 500 501 502 503 504 505 506 507 508 509 510 511 512 513 514 515 516 517 518 519 520 521 522 523 524 525 526 527 528 529 530 531 532 533 534 535 536 537 538 539 540 541 542 543 544 545 546 547 548 549 550 551 552 553 554 555 556 557 558 559 560 561 562 563 564 565 566 567 568 569 570 571 572 573 574 575 576 577 578 579 580 581 582 583 584 585 586 587 588 589 590 591 592 593 594 595 596 597 598 599 600 601 602 603 604 605 606 607 608 609 610 611 612 613 614 615 616 | # -*- coding: utf-8 -*- u'''Lambert conformal conic projection for 1- or 2-Standard Parallels classes L{Conic}, L{Conics} registry, L{LCCError} and position class L{Lcc}. See U{LCC<https://WikiPedia.org/wiki/Lambert_conformal_conic_projection>}, U{Lambert Conformal Conic to Geographic Transformation Formulae <https://www.Linz.govt.NZ/data/geodetic-system/coordinate-conversion/ projection-conversions/lambert-conformal-conic-geographic>}, U{Lambert Conformal Conic Projection <https://MathWorld.Wolfram.com/LambertConformalConicProjection.html>} and John P. Snyder U{'Map Projections - A Working Manual' <https://pubs.er.USGS.gov/djvu/PP/PP_1395.pdf>}, 1987, pp 107-109. @newfield example: Example, Examples ''' from pygeodesy.basics import EPS, PI_2, property_RO, _xinstanceof, \ _xsubclassof, _xzipairs from pygeodesy.ellipsoidalBase import LatLonEllipsoidalBase as _LLEB from pygeodesy.datum import Datums, Lam_, Phi_ from pygeodesy.errors import _IsnotError, _ValueError from pygeodesy.lazily import _ALL_LAZY, _dot_ from pygeodesy.named import EasNor3Tuple, LatLon2Tuple, \ LatLon4Tuple, LatLonDatum3Tuple, \ _NamedBase, _NamedEnum, _NamedEnumItem, nameof, \ PhiLam2Tuple, _xnamed # PYCHOK indent from pygeodesy.streprs import fstr from pygeodesy.units import Easting, Height, Northing, Scalar_ from pygeodesy.utily import degrees90, degrees180, sincos2, tanPI_2_2 from math import atan, copysign, hypot, log, radians, sin, sqrt # all public constants, classes and functions __all__ = _ALL_LAZY.lcc __version__ = '20.05.05' class Conic(_NamedEnumItem): '''Lambert conformal conic projection (1- or 2-SP). ''' _auth = '' #: (INTERNAL) authorization (C{str}). _datum = None #: (INTERNAL) Datum (L{Datum}). _name = 'Conic' #: (INTERNAL) Conic (L{Conic}). _e = 0 #: (INTERNAL) Ellipsoid excentricity (C{float}). _E0 = 0 #: (INTERNAL) False easting (C{float}). _k0 = 1 #: (INTERNAL) Scale factor (C{float}). _N0 = 0 #: (INTERNAL) false northing (C{float}). _SP = 0 #: (INTERNAL) 1- or 2-SP (C{int}) _opt3 = 0 #: (INTERNAL) Optional, longitude (C{radians}). _par1 = 0 #: (INTERNAL) 1st std parallel (C{radians}). _par2 = 0 #: (INTERNAL) 2nd std parallel (C{radians}). _phi0 = 0 #: (INTERNAL) Origin lat (C{radians}). _lam0 = 0 #: (INTERNAL) Origin lon (C{radians}). _aF = 0 #: (INTERNAL) Precomputed F. _n = 0 #: (INTERNAL) Precomputed n. _n_ = 0 #: (INTERNAL) Precomputed 1 / n. _r0 = 0 #: (INTERNAL) Precomputed rho0. def __init__(self, latlon0, par1, par2=None, E0=0, N0=0, k0=1, opt3=0, name='', auth=''): '''New Lambert conformal conic projection. @arg latlon0: Origin with (ellipsoidal) datum (C{LatLon}). @arg par1: First standard parallel (C{degrees90}). @kwarg par2: Optional, second standard parallel (C{degrees90}). @kwarg E0: Optional, false easting (C{meter}). @kwarg N0: Optional, false northing (C{meter}). @kwarg k0: Optional scale factor (C{scalar}). @kwarg opt3: Optional meridian (C{degrees180}). @kwarg name: Optional name of the conic (C{str}). @kwarg auth: Optional authentication authority (C{str}). @return: A Lambert projection (L{Conic}). @raise TypeError: Non-ellipsoidal B{C{latlon0}}. @raise ValueError: Invalid B{C{par1}}, B{C{par2}}, B{C{E0}}, B{C{N0}}, B{C{k0}} or B{C{opt3}}. @example: >>> from pygeodesy import Conic, Datums, ellipsoidalNvector >>> ll0 = ellipsoidalNvector.LatLon(23, -96, datum=Datums.NAD27) >>> Snyder = Conic(ll0, 33, 45, E0=0, N0=0, name='Snyder') ''' if latlon0 is not None: _xinstanceof(_LLEB, latlon0=latlon0) self._phi0, self._lam0 = latlon0.philam self._par1 = Phi_(par1, name='par1') self._par2 = self._par1 if par2 is None else Phi_(par2, name='par2') if k0 != 1: self._k0 = Scalar_(k0, name='k0') if E0: self._E0 = Northing(E0, name='E0', falsed=True) if N0: self._N0 = Easting(N0, name='N0', falsed=True) if opt3: self._opt3 = Lam_(opt3, name='opt3') self.toDatum(latlon0.datum)._dup2(self) self._register(Conics, name) elif name: self.name = name if auth: self._auth = str(auth) @property_RO def auth(self): '''Get the authentication authority (C{str}). ''' return self._auth @property_RO def datum(self): '''Get the datum (L{Datum}). ''' return self._datum @property_RO def E0(self): '''Get the false easting (C{meter}). ''' return self._E0 @property_RO def k0(self): '''Get scale factor (C{float}). ''' return self._k0 @property_RO def lat0(self): '''Get the origin latitude (C{degrees90}). ''' return degrees90(self._phi0) @property_RO def latlon0(self): '''Get the central origin (L{LatLon2Tuple}C{(lat, lon)}). ''' return self._xnamed(LatLon2Tuple(self.lat0, self.lon0)) @property_RO def lam0(self): '''Get the central meridian (C{radians}). ''' return self._lam0 @property_RO def lon0(self): '''Get the central meridian (C{degrees180}). ''' return degrees180(self._lam0) @property_RO def N0(self): '''Get the false northing (C{meter}). ''' return self._N0 @property_RO def name2(self): '''Get the conic and datum names as "conic.datum" (C{str}). ''' return _dot_(self.name, self.datum.name) @property_RO def opt3(self): '''Get the optional meridian (C{degrees180}). ''' return degrees180(self._opt3) @property_RO def par1(self): '''Get the 1st standard parallel (C{degrees90}). ''' return degrees90(self._par1) @property_RO def par2(self): '''Get the 2nd standard parallel (C{degrees90}). ''' return degrees90(self._par2) @property_RO def phi0(self): '''Get the origin latitude (C{radians}). ''' return self._phi0 @property_RO def philam0(self): '''Get the central origin (L{PhiLam2Tuple}C{(phi, lam)}). ''' return self._xnamed(PhiLam2Tuple(self.phi0, self.lam0)) @property_RO def SP(self): '''Get the number of standard parallels (C{int}). ''' return self._SP def toDatum(self, datum): '''Convert this conic to the given datum. @arg datum: Ellipsoidal datum to use (L{Datum}). @return: Converted conic, unregistered (L{Conic}). @raise TypeError: Non-ellipsoidal B{C{datum}}. ''' E = datum.ellipsoid if not E.isEllipsoidal: raise _IsnotError('ellipsoidal', datum=datum) c = self if c._e != E.e or c._datum != datum: c = Conic(None, 0, name=self._name) self._dup2(c) c._datum = datum c._e = E.e if abs(c._par1 - c._par2) < EPS: m1 = c._mdef(c._phi0) t1 = c._tdef(c._phi0) t0 = t1 k = 1 n = sin(c._phi0) sp = 1 else: m1 = c._mdef(c._par1) m2 = c._mdef(c._par2) t1 = c._tdef(c._par1) t2 = c._tdef(c._par2) t0 = c._tdef(c._phi0) k = c._k0 n = (log(m1) - log(m2)) \ / (log(t1) - log(t2)) sp = 2 F = m1 / (n * pow(t1, n)) c._aF = k * E.a * F c._n = n c._n_ = 1 / n c._r0 = c._rdef(t0) c._SP = sp return c convertDatum = toDatum # alternate name def toStr(self, prec=8): # PYCHOK expected '''Return this conic as a string. @kwarg prec: Optional number of decimals, unstripped (C{int}). @return: Conic attributes (C{str}). ''' if self._SP == 1: return self._instr(prec, 'lat0', 'lon0', 'par1', 'E0', 'N0', 'k0', 'SP', datum=self.datum) else: return self._instr(prec, 'lat0', 'lon0', 'par1', 'par2', 'E0', 'N0', 'k0', 'SP', datum=self.datum) def _dup2(self, c): '''(INTERNAL) Copy this conic to c. @arg c: Duplicate (L{Conic}). ''' c._auth = self._auth c._datum = self._datum c._e = self._e c._E0 = self._E0 c._k0 = self._k0 c._N0 = self._N0 c._SP = self._SP c._par1 = self._par1 c._par2 = self._par2 c._phi0 = self._phi0 c._lam0 = self._lam0 c._opt3 = self._opt3 c._aF = self._aF c._n = self._n c._n_ = self._n_ c._r0 = self._r0 def _mdef(self, lat): '''(INTERNAL) Compute m(lat). ''' s, c = sincos2(lat) s *= self._e return c / sqrt(1 - s**2) def _pdef(self, lat): '''(INTERNAL) Compute p(lat). ''' s = self._e * sin(lat) return pow((1 - s) / (1 + s), self._e / 2) def _rdef(self, t): '''(INTERNAL) Compute r(t). ''' return self._aF * pow(t, self._n) def _tdef(self, lat): '''(INTERNAL) Compute t(lat). ''' return max(0, tanPI_2_2(-lat) / self._pdef(lat)) def _xdef(self, t_x): '''(INTERNAL) Compute x(t_x). ''' return PI_2 - 2 * atan(t_x) # XXX + self._phi0 Conics = _NamedEnum('Conics', Conic) #: Registered conics. Conics._assert( # <https://SpatialReference.org/ref/sr-org/...> # AsLb = Conic(_LLEB(-14.2666667, 170, datum=Datums.NAD27), 0, 0, E0=500000, N0=0, name='AsLb', auth='EPSG:2155'), # American Samoa ... SP=1 ! Be08Lb = Conic(_LLEB(50.7978150, 4.359215833, datum=Datums.GRS80), 49.833333, 51.166667, E0=649328.0, N0=665262.0, name='Be08Lb', auth='EPSG:9802'), # Belgium Be72Lb = Conic(_LLEB(90, 4.3674867, datum=Datums.NAD83), 49.8333339, 51.1666672, E0=150000.013, N0=5400088.438, name='Be72Lb', auth='EPSG:31370'), # Belgium Fr93Lb = Conic(_LLEB(46.5, 3, datum=Datums.WGS84), 49, 44, E0=700000, N0=6600000, name='Fr93Lb', auth='EPSG:2154'), # RFG93, France MaNLb = Conic(_LLEB(33.3, -5.4, datum=Datums.NTF), 31.73, 34.87, E0=500000, N0=300000, name='MaNLb'), # Marocco MxLb = Conic(_LLEB(12, -102, datum=Datums.WGS84), 17.5, 29.5, E0=2500000, N0=0, name='MxLb', auth='EPSG:2155'), # Mexico PyT_Lb = Conic(_LLEB(46.8, 2.33722917, datum=Datums.NTF), 45.89893890000052, 47.69601440000037, E0=600000, N0=200000, name='PyT_Lb', auth='Test'), # France? USA_Lb = Conic(_LLEB(23, -96, datum=Datums.WGS84), 33, 45, E0=0, N0=0, name='USA_Lb'), # Conterminous, contiguous USA? WRF_Lb = Conic(_LLEB(40, -97, datum=Datums.WGS84), 33, 45, E0=0, N0=0, name='WRF_Lb', auth='EPSG:4326') # World ) class LCCError(_ValueError): '''Lambert Conformal Conic C{LCC} or other L{Lcc} issue. ''' pass class Lcc(_NamedBase): '''Lambert conformal conic East-/Northing location. ''' _conic = None #: (INTERNAL) Lambert projection (L{Conic}). _easting = 0 #: (INTERNAL) Easting (C{float}). _height = 0 #: (INTERNAL) Height (C{meter}). _latlon = None #: (INTERNAL) latlon cache (L{LatLon2Tuple}). _northing = 0 #: (INTERNAL) Northing (C{float}). _philam = None #: (INTERNAL) philam cache (L{PhiLam2Tuple}). def __init__(self, e, n, h=0, conic=Conics.WRF_Lb, name=''): '''New L{Lcc} Lamber conformal conic position. @arg e: Easting (C{meter}). @arg n: Northing (C{meter}). @kwarg h: Optional height (C{meter}). @kwarg conic: Optional, the conic projection (L{Conic}). @kwarg name: Optional name (C{str}). @return: The Lambert location (L{Lcc}). @raise LCCError: Invalid B{C{h}} or invalid or negative B{C{e}} or B{C{n}}. @raise TypeError: If B{C{conic}} is not L{Conic}. @example: >>> lb = Lcc(448251, 5411932.0001) ''' _xinstanceof(Conic, conic=conic) self._conic = conic self._easting = Easting(e, falsed=conic.E0 > 0, Error=LCCError) self._northing = Northing(n, falsed=conic.N0 > 0, Error=LCCError) if h: self._height = Height(h, name='h', Error=LCCError) if name: self.name = name @property_RO def conic(self): '''Get the conic projection (L{Conic}). ''' return self._conic @property_RO def easting(self): '''Get the easting (C{meter}). ''' return self._easting @property_RO def height(self): '''Get the height (C{meter}). ''' return self._height @property_RO def latlon(self): '''Get the lat- and longitude in C{degrees} (L{LatLon2Tuple}). ''' if self._latlon is None: r = self.toLatLon(LatLon=None, datum=None) self._latlon = LatLon2Tuple(r.lat, r.lon) return self._xnamed(self._latlon) @property_RO def northing(self): '''Get the northing (C{meter}). ''' return self._northing @property_RO def philam(self): '''Get the lat- and longitude in C{radians} (L{PhiLam2Tuple}). ''' if self._philam is None: self._philam = PhiLam2Tuple(radians(self.latlon.lat), radians(self.latlon.lon)) return self._xnamed(self._philam) def to3lld(self, datum=None): # PYCHOK no cover '''DEPRECATED, use method C{toLatLon}. @kwarg datum: Optional datum to use, otherwise use this B{C{Lcc}}'s conic.datum (C{Datum}). @return: A L{LatLonDatum3Tuple}C{(lat, lon, datum)}. @raise TypeError: If B{C{datum}} is not ellipsoidal. ''' if datum in (None, self.conic.datum): r = LatLonDatum3Tuple(self.latlon.lat, self.latlon.lon, self.conic.datum) else: r = self.toLatLon(LatLon=None, datum=datum) r = LatLonDatum3Tuple(r.lat, r.lon, r.datum) return self._xnamed(r) def toLatLon(self, LatLon=None, datum=None, height=None): '''Convert this L{Lcc} to an (ellipsoidal) geodetic point. @kwarg LatLon: Optional, ellipsoidal class to return the geodetic point (C{LatLon}) or C{None}. @kwarg datum: Optional datum to use, otherwise use this B{C{Lcc}}'s conic.datum (C{Datum}). @kwarg height: Optional height for the point, overriding the default height (C{meter}). @return: The point (B{C{LatLon}}) or a L{LatLon4Tuple}C{(lat, lon, height, datum)} if B{C{LatLon}} is C{None}. @raise TypeError: If B{C{LatLon}} or B{C{datum}} is not ellipsoidal. ''' if LatLon: _xsubclassof(_LLEB, LatLon=LatLon) c = self.conic if datum: c = c.toDatum(datum) e = self.easting - c._E0 n = c._r0 - self.northing + c._N0 r_ = copysign(hypot(e, n), c._n) t_ = pow(r_ / c._aF, c._n_) x = c._xdef(t_) # XXX c._lam0 while True: p, x = x, c._xdef(t_ * c._pdef(x)) if abs(x - p) < 1e-9: # XXX EPS too small? break lat = degrees90(x) lon = degrees180((atan(e / n) + c._opt3) * c._n_ + c._lam0) h = self.height if height is None else height d = c.datum r = LatLon4Tuple(lat, lon, h, d) if LatLon is None else \ LatLon(lat, lon, height=h, datum=d) return self._xnamed(r) def toRepr(self, prec=0, fmt='[%s]', sep=', ', m='m', C=False, **unused): # PYCHOK expected '''Return a string representation of this L{Lcc} position. @kwarg prec: Optional number of decimals, unstripped (C{int}). @kwarg fmt: Optional, enclosing backets format (C{str}). @kwarg sep: Optional separator between name:values (C{str}). @kwarg m: Optional unit of the height, default meter (C{str}). @kwarg C: Optionally, include name of conic and datum (C{bool}). @return: This Lcc as "[E:meter, N:meter, H:m, C:Conic.Datum]" (C{str}). ''' t = self.toStr(prec=prec, sep=None, m=m) k = 'ENH'[:len(t)] if C: k += 'C' t += [self.conic.name2] return _xzipairs(k, t, sep=sep, fmt=fmt) def toStr(self, prec=0, sep=' ', m='m'): # PYCHOK expected '''Return a string representation of this L{Lcc} position. @kwarg prec: Optional number of decimal, unstripped (C{int}). @kwarg sep: Optional separator to join (C{str}) or C{None} to return an unjoined C{tuple} of C{str}s. @kwarg m: Optional height units, default C{meter} (C{str}). @return: This Lcc as "easting nothing" C{str} in C{meter} plus " height" and 'm' if heigth is non-zero (C{str}). @example: >>> lb = Lcc(448251, 5411932.0001) >>> lb.toStr(4) # 448251.0 5411932.0001 >>> lb.toStr(sep=', ') # 448251, 5411932 ''' t = [fstr(self._easting, prec=prec), fstr(self._northing, prec=prec)] if self._height: t += ['%+.2f%s' % (self._height, m)] return tuple(t) if sep is None else sep.join(t) def toLcc(latlon, conic=Conics.WRF_Lb, height=None, Lcc=Lcc, name='', **Lcc_kwds): '''Convert an (ellipsoidal) geodetic point to a I{Lambert} location. @arg latlon: Ellipsoidal point (C{LatLon}). @kwarg conic: Optional Lambert projection to use (L{Conic}). @kwarg height: Optional height for the point, overriding the default height (C{meter}). @kwarg Lcc: Optional class to return the I{Lambert} location (L{Lcc}). @kwarg name: Optional B{C{Lcc}} name (C{str}). @kwarg Lcc_kwds: Optional, additional B{C{Lcc}} keyword arguments, ignored if B{C{Lcc=None}}. @return: The I{Lambert} location (L{Lcc}) or an L{EasNor3Tuple}C{(easting, northing, height)} if B{C{Lcc}} is C{None}. @raise TypeError: If B{C{latlon}} is not ellipsoidal. ''' _xinstanceof(_LLEB, latlon=latlon) a, b = latlon.philam c = conic.toDatum(latlon.datum) t = c._n * (b - c._lam0) - c._opt3 st, ct = sincos2(t) r = c._rdef(c._tdef(a)) e = c._E0 + r * st n = c._N0 + c._r0 - r * ct h = latlon.height if height is None else height r = EasNor3Tuple(e, n, h) if Lcc is None else \ Lcc(e, n, h=h, conic=c, **Lcc_kwds) return _xnamed(r, name or nameof(latlon)) if __name__ == '__main__': # print all for c in (Conics,): c = '\n' + repr(c) print('\n# '.join(c.split('\n'))) # **) MIT License # # Copyright (C) 2016-2020 -- mrJean1 at Gmail -- All Rights Reserved. # # Permission is hereby granted, free of charge, to any person obtaining a # copy of this software and associated documentation files (the "Software"), # to deal in the Software without restriction, including without limitation # the rights to use, copy, modify, merge, publish, distribute, sublicense, # and/or sell copies of the Software, and to permit persons to whom the # Software is furnished to do so, subject to the following conditions: # # The above copyright notice and this permission notice shall be included # in all copies or substantial portions of the Software. # # THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS # OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, # FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL # THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR # OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, # ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR # OTHER DEALINGS IN THE SOFTWARE. # % python -m pygeodesy.lcc # Conics.Be08Lb: Conic(name='Be08Lb', lat0=50.797815, lon0=4.35921583, par1=49.833333, par2=51.166667, E0=649328, N0=665262, k0=1, SP=2, datum=(name='GRS80', ellipsoid=Ellipsoids.GRS80, transform=Transforms.WGS84), # Conics.Be72Lb: Conic(name='Be72Lb', lat0=90, lon0=4.3674867, par1=49.8333339, par2=51.1666672, E0=150000.013, N0=5400088.438, k0=1, SP=2, datum=(name='NAD83', ellipsoid=Ellipsoids.GRS80, transform=Transforms.NAD83), # Conics.Fr93Lb: Conic(name='Fr93Lb', lat0=46.5, lon0=3, par1=49, par2=44, E0=700000, N0=6600000, k0=1, SP=2, datum=(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), # Conics.MaNLb: Conic(name='MaNLb', lat0=33.3, lon0=-5.4, par1=31.73, par2=34.87, E0=500000, N0=300000, k0=1, SP=2, datum=(name='NTF', ellipsoid=Ellipsoids.Clarke1880IGN, transform=Transforms.NTF), # Conics.MxLb: Conic(name='MxLb', lat0=12, lon0=-102, par1=17.5, par2=29.5, E0=2500000, N0=0, k0=1, SP=2, datum=(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), # Conics.PyT_Lb: Conic(name='PyT_Lb', lat0=46.8, lon0=2.33722917, par1=45.8989389, par2=47.6960144, E0=600000, N0=200000, k0=1, SP=2, datum=(name='NTF', ellipsoid=Ellipsoids.Clarke1880IGN, transform=Transforms.NTF), # Conics.USA_Lb: Conic(name='USA_Lb', lat0=23, lon0=-96, par1=33, par2=45, E0=0, N0=0, k0=1, SP=2, datum=(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84), # Conics.WRF_Lb: Conic(name='WRF_Lb', lat0=40, lon0=-97, par1=33, par2=45, E0=0, N0=0, k0=1, SP=2, datum=(name='WGS84', ellipsoid=Ellipsoids.WGS84, transform=Transforms.WGS84),