Package pygeodesy :: Module ltp |
[frames] | no frames]

# Module ltp

Local tangent plane (LTP) and local cartesian coordinates.

Local cartesian and local tangent plane classes LocalCartesian and Ltp, LocalError and Frustum.

See Also: Local tangent plane coordinates and class LocalCartesian, transcribed from Charles Karney's C++ classLocalCartesian.

Version: 21.04.22

Classes
| LocalError A LocalCartesian or Ltp related issue.
| LocalCartesian Conversion between geodetic `(lat, lon, height)` and local cartesian `(x, y, z)` coordinates with geodetic origin `(lat0, lon0, height0)`, transcribed from Karney's C++ class LocalCartesian.
| Ltp A local tangent plan LTP, a sub-class of `LocalCartesian` with configurable ECEF converter and without optional rotation matrix.
| Frustum A rectangular pyramid, typically representing a camera's field of view (fov) and the intersection with (or projection to) a local tangent plane.

Variables
| __all__ = `_ALL_LAZY.ltp`