Package pygeodesy :: Module elevations |
[frames] | no frames]

# Module elevations

Functions to obtain elevations and geoid heights thru web services, for (lat, lon) locations, currently limited to the Conterminous US (CONUS).

macOS: If an `SSLCertVerificationError` occurs, especially this "[SSL: CERTIFICATE_VERIFY_FAILED] certificate verify failed: self "signed certificate in certificate chain ...", review this post for a remedy. From a Terminal window run: `"/Applications/Python X.Y/Install Certificates.command"`

Version: 18.09.14

Functions
elevation2(lat, lon, timeout=2.0) Get the geoid elevation at an `NAD83` to `NAVD88` location. |
geoidHeight2(lat, lon, model=0, timeout=2.0) Get the `NAVD88` geoid height at an `NAD83` location. |

Function Details

### elevation2(lat, lon, timeout=2.0) |
Get the geoid elevation at an `NAD83` to `NAVD88` location. Parameters: `lat` - Latitude (degrees). `lon` - Longitude (degrees). `timeout` - Optional, query timeout (seconds). Returns: 2-Tuple (elevation, data_source) in (meter, string) or (None, <error>). Note: The returned elevation is None if lat or lon is invalid or outside the `Conterminous US (CONUS)`, if the query timed out or if conversion failed. The <error> is the HTTP-, IO-, SSL-, Type-, URL- or ValueError as string. See Also: USGS National Map, the FAQ and USGS10mElev.py.

### geoidHeight2(lat, lon, model=0, timeout=2.0) |
Get the `NAVD88` geoid height at an `NAD83` location. Parameters: `lat` - Latitude (degrees). `lon` - Longitude (degrees). `model` - Optional, geoid model ID (int). `timeout` - Optional, query timeout (seconds). Returns: 2-Tuple (height, model_name) in (meter, string) or (None, <error>). Note: The returned height is CNone if lat or lon is invalid or outside the `Conterminous US (CONUS)`, if the model was invalid, if the query timed out or if conversion failed. The <error> is the HTTP-, IO-, SSL-, Type-, URL- or ValueError as string. See Also: NOAA National Geodetic Survery and Geoid