Package pygeodesy :: Module ltpTuples :: Class Ned |
[frames] | no frames]

# Class Ned

      object --+
               |
    named._Named --+
                   |
    named._NamedBase --+
                       |
                      Ned

Known Subclasses:
  - ellipsoidalNvector.Ned

Local `North-Eeast-Down` (NED) location in a local tangent plane.

See Also: Enu and Ltp.

Instance Methods
__init__(self, ned, east=0.0, down=0.0, ltp=None, name='') New Ned vector. |
to3ned(self) DEPRECATED, use property ned4. |
toRepr(self, prec=None, fmt='[%s]', sep=', ', **unused) Return a string representation of this NED. |
toStr(self, prec=3, fmt='[%s]', sep=', ') Return a string representation of this NED. |
toVector3d(self) DEPRECATED, use property xyz. |
toXyz(self, Xyz=None, **Xyz_kwds) Get the local X, Y, Z (XYZ) components. |
Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others` Inherited from `named._Named`: `_DOT_`, `attrs`, `classof`, `copy`, `rename`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
| aer4 Get the `(azimuth, elevation, slantrange, ltp)` components (Aer4Tuple).
| azimuth Get the Azimuth, bearing from North (`degrees360`).
| bearing DEPRECATED, use azimuth.
| down Get the Down component (`meter`).
| east Get the East component (`meter`).
| elevation Get the Elevation, tilt above horizon (`degrees90`).
| groundrange Get the ground range, distance (`meter`).
| length DEPRECATED, use `slantrange`.
| ltp Get the local tangent plane (Ltp).
| ned DEPRECATED, use property `ned4`.
| ned4 Get the `(north, east, down, ltp)` components (Ned4Tuple).
| north Get the North component (`meter`).
| slantrange Get the slant Range, distance (`meter`).
| up Get the Up component (`meter`).
| x Get the X component (`meter`).
| xyz Get the local `(X, Y, Z)` coordinates (Vector3Tuple`(x, y, z)`).
| xyz4 Get the `(x, y, z, ltp)` components (Xyz4Tuple).
| xyzLocal Get this NED as an XyzLocal.
| y Get the Y component (`meter`).
| z Get the Z component (`meter`).
Inherited from `named._Named`: `classname`, `classnaming`, `name`, `named`, `named2`, `named3`, `named4` Inherited from `object`: `__class__`

Method Details

### __init__ (self, ned, east=0.0, down=0.0, ltp=None, name='') (Constructor) |
New Ned vector. Arguments: `ned` - Scalar north component (`meter`) or local NED (Ned, Ned4Tuple). `east` - Scalar east component (`meter`) if scalar `ned`. `down` - Scalar down component, normal to inside surface of the ellipsoid or sphere (`meter`) if scalar `ned`. `ltp` - The local tangent plane, (geodetic) origin (Ltp, LocalCartesian). `name` - Optional name (`str`). Raises: `TypeError` - Invalid `ltp`. `UnitError` - Invalid `north`, `east` or `down`. Overrides: object.__init__

### to3ned (self) |
DEPRECATED, use property ned4. Decorators: `@deprecated_method`

### toRepr (self, prec=None, fmt='[%s]', sep=', ', **unused) |
Return a string representation of this NED. Arguments: `prec` - Optional number of decimals, unstripped (`int`). `fmt` - Optional enclosing backets format (`str`). `sep` - Optional separator between items (`str`). Returns: This NED as "[N:meter, E:meter, D:meter]" (`str`). Overrides: named._Named.toRepr

### toStr (self, prec=3, fmt='[%s]', sep=', ') |
Return a string representation of this NED. Arguments: `prec` - Optional number of decimals, unstripped (`int`). `fmt` - Optional enclosing backets format (`str`). `sep` - Optional separator between NEDs (`str`). Returns: This NED as "[meter, meter, meter]" (`str`). Raises: `AssertionError` - Always, see function notOverloaded. Overrides: named._Named.toStr

### toVector3d (self) |
DEPRECATED, use property xyz. Decorators: `@deprecated_method`

### toXyz (self, Xyz=None, **Xyz_kwds) |
Get the local X, Y, Z (XYZ) components. Arguments: `Xyz` - Class to return XYZ (XyzLocal, Enu, Ned, Aer) or `None`. `Xyz_kwds` - Optional, additional `Xyz` keyword arguments, ignored if `Xyz=None`. Returns: XYZ as an `Xyz` instance or if `Xyz=None`, an Xyz4Tuple`(x, y, z, ltp)`. Raises: `TypeError` - Invalid `Xyz`.

Property Details

### aer4 Get the `(azimuth, elevation, slantrange, ltp)` components (Aer4Tuple). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### azimuth Get the Azimuth, bearing from North (`degrees360`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### bearing DEPRECATED, use azimuth. Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### down Get the Down component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### east Get the East component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### elevation Get the Elevation, tilt above horizon (`degrees90`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### groundrange Get the ground range, distance (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### length DEPRECATED, use `slantrange`. Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### ltp Get the local tangent plane (Ltp). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### ned DEPRECATED, use property `ned4`. Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### ned4 Get the `(north, east, down, ltp)` components (Ned4Tuple). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### north Get the North component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### slantrange Get the slant Range, distance (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### up Get the Up component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### x Get the X component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyz Get the local `(X, Y, Z)` coordinates (Vector3Tuple`(x, y, z)`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyz4 Get the `(x, y, z, ltp)` components (Xyz4Tuple). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyzLocal Get this NED as an XyzLocal. Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### y Get the Y component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### z Get the Z component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)