mwavepy.transmissionLine.coax | index /usr/local/lib/python2.6/dist-packages/mwavepy/transmissionLine/coax.py

`contains coaxial cable transmission line class`

Classes
`` |  | mwavepy.transmissionLine.genericTEM.GenericTEM(__builtin__.object) Coax
class Coax(mwavepy.transmissionLine.genericTEM.GenericTEM)
`` |  | Method resolution order: Coax mwavepy.transmissionLine.genericTEM.GenericTEM __builtin__.object Methods defined here: __init__(self, innerRadius, outerRadius, surfaceResistance=0, relative_permativity=1, relative_permeability=1) Methods inherited from mwavepy.transmissionLine.genericTEM.GenericTEM: characteristic_impedance(self, f) `The characteristic impedance at a given angular frequency. Z0(w) = sqrt(Z'(w)/Y'(w)) takes: f: frequency returns: Z0: characteristic impedance ohms` distributed_admittance(self, f) `distributed Admittance, Y'(w) = G' + jwC' takes: f: frequency [Hz]` distributed_impedance(self, f) `distributed Impedance, Z'(w) = R' + jwI' takes: f: frequency [Hz]` electrical_length(self, f, d, deg=False) propagation_constant(self, f) `the propagation constant gamma(w) = sqrt(Z'(w)*Y'(w)) takes: f: frequency [Hz] returns: gamma: possibly complex propagation constant, [jrad/m+]` Data descriptors inherited from mwavepy.transmissionLine.genericTEM.GenericTEM: __dict__ `dictionary for instance variables (if defined)` __weakref__ `list of weak references to the object (if defined)`