1

2# -*- coding: utf-8 -*-

3

4 u'''Cassini-Soldner (CSS) projection.

5

6 Classes L{CassiniSoldner}, L{Css} and L{CSSError} requiring I{Charles Karney}'s

7 U{geographiclib <https://PyPI.org/project/geographiclib>} Python package to be

8 installed.

9'''

10

11 from pygeodesy.basics import islistuple, neg, _xinstanceof, _xsubclassof

12 from pygeodesy.constants import _umod_360, _0_0, _0_5, _90_0

13 from pygeodesy.datums import _ellipsoidal_datum, _WGS84

14 from pygeodesy.ellipsoidalBase import LatLonEllipsoidalBase as _LLEB

15 from pygeodesy.errors import _ValueError, _xdatum, _xellipsoidal, \

16 _xattr, _xkwds

17 from pygeodesy.interns import NN, _azimuth_, _COMMASPACE_, _easting_, \

18 _lat_, _lon_, _m_, _name_, _northing_, \

19 _reciprocal_, _SPACE_

20 from pygeodesy.interns import _C_ # PYCHOK used!

21 from pygeodesy.karney import _atan2d, _copysign, _diff182, _norm2, \

22 _norm180, _signBit, _sincos2d, fabs

23 from pygeodesy.lazily import _ALL_LAZY, _ALL_MODS as _MODS

24 from pygeodesy.named import _NamedBase, _NamedTuple, nameof

25 from pygeodesy.namedTuples import EasNor2Tuple, EasNor3Tuple, \

26 LatLon2Tuple, LatLon4Tuple, _LL4Tuple

27 from pygeodesy.props import deprecated_Property_RO, Property, \

28 Property_RO, _update_all

29 from pygeodesy.streprs import Fmt, _fstrENH2, _fstrLL0, _xzipairs

30 from pygeodesy.units import Bearing, Degrees, Easting, Height, _heigHt, \

31 Lat_, Lon_, Northing, Scalar

32

33# from math import fabs # from .karney

34

35__all__ = _ALL_LAZY.css

36__version__ = '23.12.03'

37

38

39 def _CS0(cs0):

40 '''(INTERNAL) Get/set default projection.

41 '''

42 if cs0 is None:

43 cs0 = Css._CS0

44 if cs0 is None:

45 Css._CS0 = cs0 = CassiniSoldner(_0_0, _0_0, name='Default')

46 else:

47 _xinstanceof(CassiniSoldner, cs0=cs0)

48 return cs0

49

50

51 class CSSError(_ValueError):

52 '''Cassini-Soldner (CSS) conversion or other L{Css} issue.

53 '''

54 pass

55

56

57 class CassiniSoldner(_NamedBase):

58 '''Cassini-Soldner projection, a Python version of I{Karney}'s C++ class U{CassiniSoldner

59 <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1CassiniSoldner.html>}.

60 '''

61 _cb0 = _0_0

62 _datum = _WGS84 # L{Datum}

63 _geodesic = None

64 _latlon0 = ()

65 _meridian = None

66 _sb0 = _0_0

67

68 def __init__(self, lat0, lon0, datum=_WGS84, name=NN):

69 '''New L{CassiniSoldner} projection.

70

71 @arg lat0: Latitude of center point (C{degrees90}).

72 @arg lon0: Longitude of center point (C{degrees180}).

73 @kwarg datum: Optional datum or ellipsoid (L{Datum},

74 L{Ellipsoid}, L{Ellipsoid2} or L{a_f2Tuple}).

75 @kwarg name: Optional name (C{str}).

76

77 @raise CSSError: Invalid B{C{lat}} or B{C{lon}}.

78 '''

79 if datum not in (None, self._datum):

80 self._datum = _xellipsoidal(datum=_ellipsoidal_datum(datum, name=name))

81 if name:

82 self.name = name

83

84 self.reset(lat0, lon0)

85

86 @Property

87 def datum(self):

88 '''Get the datum (L{Datum}).

89 '''

90 return self._datum

91

92 @datum.setter # PYCHOK setter!

93 def datum(self, datum):

94 '''Set the datum or ellipsoid (L{Datum}, L{Ellipsoid}, L{Ellipsoid2}

95 or L{a_f2Tuple}) or C{None} for the default.

96 '''

97 d = CassiniSoldner._datum if datum is None else \

98 _xellipsoidal(datum=_ellipsoidal_datum(datum, name=self.name))

99 if self._datum != d:

100 self._datum = d

101 self.geodesic = None if self._geodesic is None else self.isExact

102

103 def _datumatch(self, latlon):

104 '''Check for matching datum ellipsoids.

105

106 @raise CSSError: Ellipsoid mismatch of B{C{latlon}} and this projection.

107 '''

108 d = _xattr(latlon, datum=None)

109 if d:

110 _xdatum(self.datum, d, Error=CSSError)

111

112 @Property_RO

113 def equatoradius(self):

114 '''Get the ellipsoid's equatorial radius, semi-axis (C{meter}).

115 '''

116 return self.geodesic.a

117

118 a = equatoradius

119

120 @Property_RO

121 def flattening(self):

122 '''Get the ellipsoid's flattening (C{scalar}).

123 '''

124 return self.geodesic.f

125

126 f = flattening

127

128 def forward(self, lat, lon, name=NN):

129 '''Convert an (ellipsoidal) geodetic location to Cassini-Soldner

130 easting and northing.

131

132 @arg lat: Latitude of the location (C{degrees90}).

133 @arg lon: Longitude of the location (C{degrees180}).

134 @kwarg name: Name inlieu of this projection's name (C{str}).

135

136 @return: An L{EasNor2Tuple}C{(easting, northing)}.

137

138 @see: Methods L{CassiniSoldner.forward4}, L{CassiniSoldner.reverse}

139 and L{CassiniSoldner.reverse4}.

140

141 @raise CSSError: Invalid B{C{lat}} or B{C{lon}}.

142 '''

143 t = self.forward6(lat, lon, name=name)

144 return EasNor2Tuple(t.easting, t.northing, name=t.name)

145

146 def forward4(self, lat, lon, name=NN):

147 '''Convert an (ellipsoidal) geodetic location to Cassini-Soldner

148 easting and northing.

149

150 @arg lat: Latitude of the location (C{degrees90}).

151 @arg lon: Longitude of the location (C{degrees180}).

152 @kwarg name: Name inlieu of this projection's name (C{str}).

153

154 @return: An L{EasNorAziRk4Tuple}C{(easting, northing,

155 azimuth, reciprocal)}.

156

157 @see: Method L{CassiniSoldner.forward}, L{CassiniSoldner.forward6},

158 L{CassiniSoldner.reverse} and L{CassiniSoldner.reverse4}.

159

160 @raise CSSError: Invalid B{C{lat}} or B{C{lon}}.

161 '''

162 t = self.forward6(lat, lon, name=name)

163 return EasNorAziRk4Tuple(t.easting, t.northing,

164 t.azimuth, t.reciprocal, name=t.name)

165

166 def forward6(self, lat, lon, name=NN):

167 '''Convert an (ellipsoidal) geodetic location to Cassini-Soldner

168 easting and northing.

169

170 @arg lat: Latitude of the location (C{degrees90}).

171 @arg lon: Longitude of the location (C{degrees180}).

172 @kwarg name: Name inlieu of this projection's name (C{str}).

173

174 @return: An L{EasNorAziRkEqu6Tuple}C{(easting, northing,

175 azimuth, reciprocal, equatorarc, equatorazimuth)}.

176

177 @see: Method L{CassiniSoldner.forward}, L{CassiniSoldner.forward4},

178 L{CassiniSoldner.reverse} and L{CassiniSoldner.reverse4}.

179

180 @raise CSSError: Invalid B{C{lat}} or B{C{lon}}.

181 '''

182 g = self.geodesic

183

184 lat = Lat_(lat, Error=CSSError)

185 d, _ = _diff182(self.lon0, Lon_(lon, Error=CSSError)) # _2sum

186 D = fabs(d)

187

188 r = g.Inverse(lat, -D, lat, D)

189 z1, a = r.azi1, (r.a12 * _0_5)

190 z2, e = r.azi2, (r.s12 * _0_5)

191 if e == 0: # PYCHOK no cover

192 z = _diff182(z1, z2)[0] * _0_5 # _2sum

193 c = _copysign(_90_0, 90 - D) # -90 if D > 90 else 90

194 z1, z2 = c - z, c + z

195 if _signBit(d):

196 a, e, z2 = neg(a), neg(e), z1

197

198 z = _norm180(z2) # azimuth of easting direction

199 p = g.Line(lat, d, z, g.DISTANCE | g.GEODESICSCALE | g.LINE_OFF)

200 # reciprocal of azimuthal northing scale

201 rk = p.ArcPosition(neg(a), g.GEODESICSCALE).M21

202 # rk = p._GenPosition(True, -a, g.DISTANCE)[7]

203

204 s, c = _sincos2d(p.azi0) # aka equatorazimuth

205 sb1 = _copysign(c, lat)

206 cb1 = _copysign(s, 90 - D) # -abs(s) if D > 90 else abs(s)

207 d = _atan2d(sb1 * self._cb0 - cb1 * self._sb0,

208 cb1 * self._cb0 + sb1 * self._sb0)

209 n = self._meridian.ArcPosition(d, g.DISTANCE).s12

210 # n = self._meridian._GenPosition(True, d, g.DISTANCE)[4]

211 return EasNorAziRkEqu6Tuple(e, n, z, rk, p.a1, p.azi0,

212 name=name or self.name)

213

214 @Property

215 def geodesic(self):

216 '''Get this projection's I{wrapped} U{geodesic.Geodesic

217 <https://GeographicLib.SourceForge.io/Python/doc/code.html>}, provided

218 I{Karney}'s U{geographiclib<https://PyPI.org/project/geographiclib>}

219 package is installed, otherwise an I{exact} L{GeodesicExact} instance.

220 '''

221 g = self._geodesic

222 if g is None:

223 E = self.datum.ellipsoid

224 try:

225 g = E.geodesicw

226 except ImportError:

227 g = E.geodesicx

228 self._geodesic = g

229 return g

230

231 @geodesic.setter # PYCHOK setter!

232 def geodesic(self, exact):

233 '''Set this projection's geodesic (C{bool}) to L{GeodesicExact}

234 or I{wrapped Karney}'s or C{None} for the default.

235

236 @raise ImportError: Package U{geographiclib<https://PyPI.org/

237 project/geographiclib>} not installed or

238 not found and C{B{exact}=False}.

239 '''

240 E = self.datum.ellipsoid

241 self._geodesic = None if exact is None else (

242 E.geodesicx if exact else E.geodesicw)

243 self.reset(*self.latlon0)

244

245 @Property_RO

246 def isExact(self):

247 '''Return C{True} if this projection's geodesic is L{GeodesicExact}.

248 '''

249 return isinstance(self.geodesic, _MODS.geodesicx.GeodesicExact)

250

251 @Property_RO

252 def lat0(self):

253 '''Get the center latitude (C{degrees90}).

254 '''

255 return self.latlon0.lat

256

257 @property

258 def latlon0(self):

259 '''Get the center lat- and longitude (L{LatLon2Tuple}C{(lat, lon)})

260 in (C{degrees90}, (C{degrees180}).

261 '''

262 return self._latlon0

263

264 @latlon0.setter # PYCHOK setter!

265 def latlon0(self, latlon0):

266 '''Set the center lat- and longitude (ellipsoidal C{LatLon},

267 L{LatLon2Tuple}, L{LatLon4Tuple} or a C{tuple} or C{list}

268 with the C{lat}- and C{lon}gitude in C{degrees}).

269

270 @raise CSSError: Invalid B{C{latlon0}} or ellipsoid mismatch

271 of B{C{latlon0}} and this projection.

272 '''

273 if islistuple(latlon0, 2):

274 lat0, lon0 = latlon0[:2]

275 else:

276 try:

277 lat0, lon0 = latlon0.lat, latlon0.lon

278 self._datumatch(latlon0)

279 except (AttributeError, TypeError, ValueError) as x:

280 raise CSSError(latlon0=latlon0, cause=x)

281 self.reset(lat0, lon0)

282

283 @Property_RO

284 def lon0(self):

285 '''Get the center longitude (C{degrees180}).

286 '''

287 return self.latlon0.lon

288

289 @deprecated_Property_RO

290 def majoradius(self): # PYCHOK no cover

291 '''DEPRECATED, use property C{equatoradius}.'''

292 return self.equatoradius

293

294 def reset(self, lat0, lon0):

295 '''Set or reset the center point of this Cassini-Soldner projection.

296

297 @arg lat0: Center point latitude (C{degrees90}).

298 @arg lon0: Center point longitude (C{degrees180}).

299

300 @raise CSSError: Invalid B{C{lat0}} or B{C{lon0}}.

301 '''

302 _update_all(self)

303

304 g = self.geodesic

305 self._meridian = m = g.Line(Lat_(lat0=lat0, Error=CSSError),

306 Lon_(lon0=lon0, Error=CSSError), _0_0,

307 g.STANDARD | g.DISTANCE_IN | g.LINE_OFF)

308 self._latlon0 = LatLon2Tuple(m.lat1, m.lon1)

309 s, c = _sincos2d(m.lat1) # == self.lat0 == self.LatitudeOrigin()

310 self._sb0, self._cb0 = _norm2(s * g.f1, c)

311

312 def reverse(self, easting, northing, name=NN, LatLon=None, **LatLon_kwds):

313 '''Convert a Cassini-Soldner location to (ellipsoidal) geodetic

314 lat- and longitude.

315

316 @arg easting: Easting of the location (C{meter}).

317 @arg northing: Northing of the location (C{meter}).

318 @kwarg name: Name inlieu of this projection's name (C{str}).

319 @kwarg LatLon: Optional, ellipsoidal class to return the

320 geodetic location as (C{LatLon}) or C{None}.

321 @kwarg LatLon_kwds: Optional (C{LatLon}) keyword arguments,

322 ignored if C{B{LatLon} is None}.

323

324 @return: Geodetic location B{C{LatLon}} or if B{C{LatLon}}

325 is C{None}, a L{LatLon2Tuple}C{(lat, lon)}.

326

327 @raise CSSError: Ellipsoidal mismatch of B{C{LatLon}} and this projection.

328

329 @raise TypeError: Invalid B{C{LatLon}} or B{C{LatLon_kwds}}.

330

331 @see: Method L{CassiniSoldner.reverse4}, L{CassiniSoldner.forward}.

332 L{CassiniSoldner.forward4} and L{CassiniSoldner.forward6}.

333 '''

334 r = self.reverse4(easting, northing, name=name)

335 if LatLon is None:

336 r = LatLon2Tuple(r.lat, r.lon, name=r.name) # PYCHOK expected

337 else:

338 _xsubclassof(_LLEB, LatLon=LatLon)

339 kwds = _xkwds(LatLon_kwds, datum=self.datum, name=r.name)

340 r = LatLon(r.lat, r.lon, **kwds) # PYCHOK expected

341 self._datumatch(r)

342 return r

343

344 def reverse4(self, easting, northing, name=NN):

345 '''Convert a Cassini-Soldner location to (ellipsoidal) geodetic

346 lat- and longitude.

347

348 @arg easting: Easting of the location (C{meter}).

349 @arg northing: Northing of the location (C{meter}).

350 @kwarg name: Name inlieu of this projection's name (C{str}).

351

352 @return: A L{LatLonAziRk4Tuple}C{(lat, lon, azimuth, reciprocal)}.

353

354 @see: Method L{CassiniSoldner.reverse}, L{CassiniSoldner.forward}

355 and L{CassiniSoldner.forward4}.

356 '''

357 g = self.geodesic

358 n = self._meridian.Position(northing)

359 r = g.Direct(n.lat2, n.lon2, n.azi2 + _90_0, easting, outmask=g.STANDARD | g.GEODESICSCALE)

360 z = _umod_360(r.azi2) # -180 <= r.azi2 < 180 ... 0 <= z < 360

361 # include z azimuth of easting direction and rk reciprocal

362 # of azimuthal northing scale (see C++ member Direct() 5/6

363 # <https://GeographicLib.SourceForge.io/C++/doc/classGeographicLib_1_1Geodesic.html>)

364 return LatLonAziRk4Tuple(r.lat2, r.lon2, z, r.M12, name=name or self.name)

365

366 toLatLon = reverse # XXX not reverse4

367

368 def toRepr(self, prec=6, **unused): # PYCHOK expected

369 '''Return a string representation of this projection.

370

371 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

372

373 @return: This projection as C{"<classname>(lat0, lon0, ...)"}

374 (C{str}).

375 '''

376 return _fstrLL0(self, prec, True)

377

378 def toStr(self, prec=6, sep=_SPACE_, **unused): # PYCHOK expected

379 '''Return a string representation of this projection.

380

381 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

382 @kwarg sep: Separator to join (C{str}).

383

384 @return: This projection as C{"lat0 lon0"} (C{str}).

385 '''

386 t = _fstrLL0(self, prec, False)

387 return t if sep is None else sep.join(t)

388

389

390 class Css(_NamedBase):

391 '''Cassini-Soldner East-/Northing location.

392 '''

393 _CS0 = None # default projection (L{CassiniSoldner})

394 _cs0 = None # projection (L{CassiniSoldner})

395 _easting = _0_0 # easting (C{float})

396 _height = 0 # height (C{meter})

397 _northing = _0_0 # northing (C{float})

398

399 def __init__(self, e, n, h=0, cs0=None, name=NN):

400 '''New L{Css} Cassini-Soldner position.

401

402 @arg e: Easting (C{meter}).

403 @arg n: Northing (C{meter}).

404 @kwarg h: Optional height (C{meter}).

405 @kwarg cs0: Optional, the Cassini-Soldner projection

406 (L{CassiniSoldner}).

407 @kwarg name: Optional name (C{str}).

408

409 @return: The Cassini-Soldner location (L{Css}).

410

411 @raise CSSError: If B{C{e}} or B{C{n}} is invalid.

412

413 @raise TypeError: If B{C{cs0}} is not L{CassiniSoldner}.

414

415 @raise ValueError: Invalid B{C{h}}.

416 '''

417 self._cs0 = _CS0(cs0)

418 self._easting = Easting(e, Error=CSSError)

419 self._northing = Northing(n, Error=CSSError)

420 if h:

421 self._height = Height(h=h)

422 if name:

423 self.name = name

424

425 @Property_RO

426 def azi(self):

427 '''Get the azimuth of easting direction (C{degrees}).

428 '''

429 return self.reverse4.azimuth

430

431 azimuth = azi

432

433 @Property

434 def cs0(self):

435 '''Get the projection (L{CassiniSoldner}).

436 '''

437 return self._cs0 or Css._CS0

438

439 @cs0.setter # PYCHOK setter!

440 def cs0(self, cs0):

441 '''Set the I{Cassini-Soldner} projection (L{CassiniSoldner}).

442

443 @raise TypeError: Invalid B{C{cs0}}.

444 '''

445 cs0 = _CS0(cs0)

446 if cs0 != self._cs0:

447 _update_all(self)

448 self._cs0 = cs0

449

450# def dup(self, name=NN, **e_n_h_cs0): # PYCHOK signature

451# '''Duplicate this position with some attributes modified.

452#

453# @kwarg e_n_h_cs0: Use keyword argument C{B{e}=...}, C{B{n}=...},

454# C{B{h}=...} and/or C{B{cs0}=...} to override

455# the current C{easting}, C{northing} C{height}

456# or C{cs0} projectio, respectively.

457# '''

458# def _args_kwds(e=None, n=None, **kwds):

459# return (e, n), kwds

460#

461# kwds = _xkwds(e_n_h_cs0, e=self.easting, n=self.northing,

462# h=self.height, cs0=self.cs0,

463# name=name or self.name)

464# args, kwds = _args_kwds(**kwds)

465# return self.__class__(*args, **kwds) # .classof

466

467 @Property_RO

468 def easting(self):

469 '''Get the easting (C{meter}).

470 '''

471 return self._easting

472

473 @Property_RO

474 def height(self):

475 '''Get the height (C{meter}).

476 '''

477 return self._height

478

479 @Property_RO

480 def latlon(self):

481 '''Get the lat- and longitude (L{LatLon2Tuple}).

482 '''

483 r = self.reverse4

484 return LatLon2Tuple(r.lat, r.lon, name=self.name)

485

486 @Property_RO

487 def northing(self):

488 '''Get the northing (C{meter}).

489 '''

490 return self._northing

491

492 @Property_RO

493 def reverse4(self):

494 '''Get the lat, lon, azimuth and reciprocal (L{LatLonAziRk4Tuple}).

495 '''

496 return self.cs0.reverse4(self.easting, self.northing, name=self.name)

497

498 @Property_RO

499 def rk(self):

500 '''Get the reciprocal of azimuthal northing scale (C{scalar}).

501 '''

502 return self.reverse4.reciprocal

503

504 reciprocal = rk

505

506 def toLatLon(self, LatLon=None, height=None, **LatLon_kwds):

507 '''Convert this L{Css} to an (ellipsoidal) geodetic point.

508

509 @kwarg LatLon: Optional, ellipsoidal class to return the

510 geodetic point (C{LatLon}) or C{None}.

511 @kwarg height: Optional height for the point, overriding the

512 default height (C{meter}).

513 @kwarg LatLon_kwds: Optional, additional B{C{LatLon}} keyword

514 arguments, ignored if C{B{LatLon} is None}.

515

516 @return: The geodetic point (B{C{LatLon}}) or if B{C{LatLon}}

517 is C{None}, a L{LatLon4Tuple}C{(lat, lon, height,

518 datum)}.

519

520 @raise TypeError: If B{C{LatLon}} or B{C{datum}} is not

521 ellipsoidal or invalid B{C{height}} or

522 B{C{LatLon_kwds}}.

523 '''

524 if LatLon:

525 _xsubclassof(_LLEB, LatLon=LatLon)

526

527 lat, lon = self.latlon

528 h = _heigHt(self, height)

529 return _LL4Tuple(lat, lon, h, self.cs0.datum, LatLon, LatLon_kwds,

530 inst=self, name=self.name)

531

532 def toRepr(self, prec=6, fmt=Fmt.SQUARE, sep=_COMMASPACE_, m=_m_, C=False): # PYCHOK expected

533 '''Return a string representation of this L{Css} position.

534

535 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

536 @kwarg fmt: Enclosing backets format (C{str}).

537 @kwarg sep: Optional separator between name:values (C{str}).

538 @kwarg m: Optional unit of the height, default meter (C{str}).

539 @kwarg C: Optionally, include name of projection (C{bool}).

540

541 @return: This position as C{"[E:meter, N:meter, H:m, name:'',

542 C:Conic.Datum]"} (C{str}).

543 '''

544 t, T = _fstrENH2(self, prec, m)

545 if self.name:

546 t += repr(self.name),

547 T += _name_,

548 if C:

549 t += self.cs0.toRepr(prec=prec),

550 T += _C_,

551 return _xzipairs(T, t, sep=sep, fmt=fmt)

552

553 def toStr(self, prec=6, sep=_SPACE_, m=_m_): # PYCHOK expected

554 '''Return a string representation of this L{Css} position.

555

556 @kwarg prec: Number of (decimal) digits, unstripped (C{int}).

557 @kwarg sep: Optional separator to join (C{str}) or C{None}

558 to return an unjoined C{tuple} of C{str}s.

559 @kwarg m: Height units, default C{meter} (C{str}).

560

561 @return: This position as C{"easting nothing"} C{str} in

562 C{meter} plus C{" height"} and C{'m'} if height

563 is non-zero (C{str}).

564 '''

565 t, _ = _fstrENH2(self, prec, m)

566 return t if sep is None else sep.join(t)

567

568

569 class EasNorAziRk4Tuple(_NamedTuple):

570 '''4-Tuple C{(easting, northing, azimuth, reciprocal)} for the

571 Cassini-Soldner location with C{easting} and C{northing} in

572 C{meters} and the C{azimuth} of easting direction and

573 C{reciprocal} of azimuthal northing scale, both in C{degrees}.

574 '''

575 _Names_ = (_easting_, _northing_, _azimuth_, _reciprocal_)

576 _Units_ = ( Easting, Northing, Bearing, Scalar)

577

578

579 class EasNorAziRkEqu6Tuple(_NamedTuple):

580 '''6-Tuple C{(easting, northing, azimuth, reciprocal, equatorarc,

581 equatorazimuth)} for the Cassini-Soldner location with

582 C{easting} and C{northing} in C{meters} and the C{azimuth} of

583 easting direction, C{reciprocal} of azimuthal northing scale,

584 C{equatorarc} and C{equatorazimuth}, all in C{degrees}.

585 '''

586 _Names_ = EasNorAziRk4Tuple._Names_ + ('equatorarc', 'equatorazimuth')

587 _Units_ = EasNorAziRk4Tuple._Units_ + ( Degrees, Bearing)

588

589

590 class LatLonAziRk4Tuple(_NamedTuple):

591 '''4-Tuple C{(lat, lon, azimuth, reciprocal)}, all in C{degrees}

592 where C{azimuth} is the azimuth of easting direction and

593 C{reciprocal} the reciprocal of azimuthal northing scale.

594 '''

595 _Names_ = (_lat_, _lon_, _azimuth_, _reciprocal_)

596 _Units_ = ( Lat_, Lon_, Bearing, Scalar)

597

598

599 def toCss(latlon, cs0=None, height=None, Css=Css, name=NN):

600 '''Convert an (ellipsoidal) geodetic point to a Cassini-Soldner

601 location.

602

603 @arg latlon: Ellipsoidal point (C{LatLon} or L{LatLon4Tuple}).

604 @kwarg cs0: Optional, the Cassini-Soldner projection to use

605 (L{CassiniSoldner}).

606 @kwarg height: Optional height for the point, overriding the

607 default height (C{meter}).

608 @kwarg Css: Optional class to return the location (L{Css}) or C{None}.

609 @kwarg name: Optional B{C{Css}} name (C{str}).

610

611 @return: The Cassini-Soldner location (B{C{Css}}) or an

612 L{EasNor3Tuple}C{(easting, northing, height)}

613 if B{C{Css}} is C{None}.

614

615 @raise CSSError: Ellipsoidal mismatch of B{C{latlon}} and B{C{cs0}}.

616

617 @raise ImportError: Package U{geographiclib<https://PyPI.org/

618 project/geographiclib>} not installed or

619 not found.

620

621 @raise TypeError: If B{C{latlon}} is not ellipsoidal.

622 '''

623 _xinstanceof(_LLEB, LatLon4Tuple, latlon=latlon)

624

625 cs = _CS0(cs0)

626 cs._datumatch(latlon)

627

628 c = cs.forward4(latlon.lat, latlon.lon)

629 h = _heigHt(latlon, height)

630 n = name or nameof(latlon)

631

632 if Css is None:

633 r = EasNor3Tuple(c.easting, c.northing, h, name=n)

634 else:

635 r = Css(c.easting, c.northing, h=h, cs0=cs, name=n)

636 r._latlon = LatLon2Tuple(latlon.lat, latlon.lon, name=n)

637 r._azi, r._rk = c.azimuth, c.reciprocal

638 return r

639

640# **) MIT License

641#

642# Copyright (C) 2016-2024 -- mrJean1 at Gmail -- All Rights Reserved.

643#

644# Permission is hereby granted, free of charge, to any person obtaining a

645# copy of this software and associated documentation files (the "Software"),

646# to deal in the Software without restriction, including without limitation

647# the rights to use, copy, modify, merge, publish, distribute, sublicense,

648# and/or sell copies of the Software, and to permit persons to whom the

649# Software is furnished to do so, subject to the following conditions:

650#

651# The above copyright notice and this permission notice shall be included

652# in all copies or substantial portions of the Software.

653#

654# THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS

655# OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,

656# FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL

657# THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR

658# OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,

659# ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR

660# OTHER DEALINGS IN THE SOFTWARE.