Package pygeodesy :: Module namedTuples |
[frames] | no frames]

# Module namedTuples

Named tuples.

Tuples returned by `pygeodesy` functions and class methods are all instances of some `Named...Tuple` class, all sub-classes of `_NamedTuple` defined in `pygeodesy.named`.

Version: 21.12.28

Classes
| Bearing2Tuple 2-Tuple `(initial, final)` bearings, both in compass `degrees360`.
| Bounds2Tuple 2-Tuple `(latlonSW, latlonNE)` with the bounds' lower-left and upper-right corner as `LatLon` instance.
| Bounds4Tuple 4-Tuple `(latS, lonW, latN, lonE)` with the bounds' lower-left `(LatS, LowW)` and upper-right `(latN, lonE)` corner lat- and longitudes.
| Destination2Tuple 2-Tuple `(destination, final)`, `destination` in `LatLon` and `final` bearing in compass `degrees360`.
| Destination3Tuple 3-Tuple `(lat, lon, final)`, destination `lat`, `lon` in `degrees90` respectively `degrees180` and `final` bearing in compass `degrees360`.
| Distance2Tuple 2-Tuple `(distance, initial)`, `distance` in `meter` and `initial` bearing in compass `degrees360`.
| Distance3Tuple 3-Tuple `(distance, initial, final)`, `distance` in `meter` and `initial` and `final` bearing, both in compass `degrees360`.
| Distance4Tuple 4-Tuple `(distance2, delta_lat, delta_lon, unroll_lon2)` with the distance in `degrees squared`, the latitudinal `delta_lat = lat2 - lat1`, the wrapped, unrolled and adjusted longitudinal `delta_lon = lon2 - lon1` and `unroll_lon2`, the unrolled or original `lon2`.
| EasNor2Tuple 2-Tuple `(easting, northing)`, both in `meter`, conventionally.
| EasNor3Tuple 3-Tuple `(easting, northing, height)`, all in `meter`, conventionally.
| Intersection3Tuple 3-Tuple `(point, outside1, outside2)` of an intersection `point` and `outside1`, the position of the `point`, `-1` if before the start, `+1` if after the end and `0` if on or between the start and end point of the first line.
| LatLon2Tuple 2-Tuple `(lat, lon)` in `degrees90` and `degrees180`.
| LatLon3Tuple 3-Tuple `(lat, lon, height)` in `degrees90`, `degrees180` and `meter`, conventionally.
| LatLon4Tuple 4-Tuple `(lat, lon, height, datum)` in `degrees90`, `degrees180`, `meter` and Datum.
| LatLonDatum3Tuple 3-Tuple `(lat, lon, datum)` in `degrees90`, `degrees180` and Datum.
| LatLonDatum5Tuple 5-Tuple `(lat, lon, datum, convergence, scale)` in `degrees90`, `degrees180`, Datum, `degrees` and `float`.
| LatLonPrec3Tuple 3-Tuple `(lat, lon, precision)` in `degrees`, `degrees` and `int`.
| LatLonPrec5Tuple 5-Tuple `(lat, lon, precision, height, radius)` in `degrees`, `degrees`, `int` and `height` or `radius` in `meter` (or `None` if missing).
| NearestOn2Tuple 2-Tuple `(closest, fraction)` of the `closest` point on and `fraction` along a line (segment) between two points.
| NearestOn3Tuple 3-Tuple `(closest, distance, angle)` of the `closest` point on the polygon, either a `LatLon` instance or a LatLon3Tuple`(lat, lon, height)` and the `distance` and `angle` to the `closest` point are in `meter` respectively compass `degrees360`.
| NearestOn5Tuple 5-Tuple `(lat, lon, distance, angle, height)` all in `degrees`, except `height`.
| NearestOn6Tuple 6-Tuple `(closest, distance, fi, j, start, end)` with the `closest` point, the `distance` in `meter`, conventionally and the `start` and `end` point of the path or polygon edge.
| NearestOn8Tuple 8-Tuple `(closest, distance, fi, j, start, end, initial, final)`, like NearestOn6Tuple but extended with the `initial` and the `final` bearing at the reference respectively the `closest` point, both in compass `degrees`.
| PhiLam2Tuple 2-Tuple `(phi, lam)` with latitude `phi` in `radians[PI_2]` and longitude `lam` in `radians[PI]`.
| PhiLam3Tuple 3-Tuple `(phi, lam, height)` with latitude `phi` in `radians[PI_2]`, longitude `lam` in `radians[PI]` and `height` in `meter`.
| PhiLam4Tuple 4-Tuple `(phi, lam, height, datum)` with latitude `phi` in `radians[PI_2]`, longitude `lam` in `radians[PI]`, `height` in `meter` and Datum.
| Point3Tuple 3-Tuple `(x, y, ll)` in `meter`, `meter` and `LatLon`.
| Points2Tuple 2-Tuple `(number, points)` with the `number` of points and -possible reduced- `list` or `tuple` of `points`.
| Triangle7Tuple 7-Tuple `(A, a, B, b, C, c, area)` with interior angles `A`, `B` and `C` in `degrees`, spherical sides `a`, `b` and `c` in `meter` and the `area` of a spherical triangle in square `meter`.
| Triangle8Tuple 8-Tuple `(A, a, B, b, C, c, D, E)` with interior angles `A`, `B` and `C`, spherical sides `a`, `b` and `c`, spherical deficit `D` and spherical excess `E` of a spherical triangle, all in `radians`.
| Trilaterate5Tuple 5-Tuple `(min, minPoint, max, maxPoint, n)` with `min` and `max` in `meter`, the corresponding trilaterated `minPoint` and `maxPoint` as `LatLon` and the number `n`.
| UtmUps2Tuple 2-Tuple `(zone, hemipole)` as `int` and `str`, where `zone` is `1..60` for UTM or `0` for UPS and `hemipole` `'N'|'S'` is the UTM hemisphere or the UPS pole.
| UtmUps5Tuple 5-Tuple `(zone, hemipole, easting, northing, band)` as `int`, `str`, `meter`, `meter` and `band` letter, where `zone` is `1..60` for UTM or `0` for UPS, `hemipole` `'N'|'S'` is the UTM hemisphere or the UPS pole and `band` is `""` or the longitudinal UTM band `'C'|'D'|..|'W'|'X'` or polar UPS band `'A'|'B'|'Y'|'Z'`.
| UtmUps8Tuple 8-Tuple `(zone, hemipole, easting, northing, band, datum, convergence, scale)` as `int`, `str`, `meter`, `meter`, `band` letter, `Datum`, `degrees` and `scalar`, where `zone` is `1..60` for UTM or `0` for UPS, `hemipole` `'N'|'S'` is the UTM hemisphere or the UPS pole and `band` is `""` or the longitudinal UTM band `'C'|'D'|..|'W'|'X'` or polar UPS band `'A'|'B'|'Y'|'Z'`.
| UtmUpsLatLon5Tuple 5-Tuple `(zone, band, hemipole, lat, lon)` as `int`, `str`, `str`, `degrees90` and `degrees180`, where `zone` is `1..60` for UTM or `0` for UPS, `band` is `""` or the longitudinal UTM band `'C'|'D'|..|'W'|'X'` or polar UPS band `'A'|'B'|'Y'|'Z'` and `hemipole` `'N'|'S'` is the UTM hemisphere or the UPS pole.
| Vector2Tuple 2-Tuple `(x, y)` of (geocentric) components, both in `meter` or `units`.
| Vector3Tuple 3-Tuple `(x, y, z)` of (geocentric) components, all in `meter` or `units`.
| Vector4Tuple 4-Tuple `(x, y, z, h)` of (geocentric) components, all in `meter` or `units`.

Variables
| __all__ = `_ALL_LAZY.namedTuples`