Package pygeodesy :: Module ltpTuples :: Class Aer |
[frames] | no frames]

# Class Aer

      object --+
               |
    named._Named --+
                   |
    named._NamedBase --+
                       |
                      Aer

Local `Azimuth-Elevation-Range` (AER) in a local tangent plane.

Instance Methods
__init__(self, aer, elevation=0.0, slantrange=0.0, ltp=None, name='') New Aer. |
toRepr(self, prec=None, fmt='[%s]', sep=', ', **unused) Return a string representation of this AER as azimuth (bearing), elevation and slant range. |
toStr(self, prec=3, fmt='[%s]', sep=', ') Return a string representation of this ENU/NED/AER. |
toXyz(self, Xyz=None, **Xyz_kwds) Get the local X, Y, Z (XYZ) components. |
Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others` Inherited from `named._Named`: `_DOT_`, `attrs`, `classof`, `copy`, `rename`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
| aer4 Get the `(azimuth, elevation, slantrange, ltp)` components (Aer4Tuple).
| azimuth Get the Azimuth, bearing from North (`degrees360`).
| down Get the Down component (`meter`).
| east Get the East component (`meter`).
| elevation Get the Elevation, tilt above horizon (`degrees90`).
| groundrange Get the ground range, distance (`meter`).
| ltp Get the local tangent plane (Ltp).
| north Get the North component (`meter`).
| slantrange Get the slant Range, distance (`meter`).
| up Get the Up component (`meter`).
| x Get the X component (`meter`).
| xyz Get the local `(X, Y, Z)` coordinates (Vector3Tuple`(x, y, z)`).
| xyz4 Get the `(x, y, z, ltp)` components (Xyz4Tuple).
| xyzLocal Get this AER as an XyzLocal.
| y Get the Y component (`meter`).
| z Get the Z component (`meter`).
Inherited from `named._Named`: `classname`, `classnaming`, `name`, `named`, `named2`, `named3`, `named4` Inherited from `object`: `__class__`

Method Details

### __init__ (self, aer, elevation=0.0, slantrange=0.0, ltp=None, name='') (Constructor) |
New Aer. Arguments: `aer` - Scalar azimuth, bearing from North (`degrees360`) or local (Aer, Aer4Tuple). `elevation` - Scalar angle above horizon, above `ltp` (`degrees90`) if scalar `aer`. `slantrange` - Scalar distance (`meter`) if scalar `aer`. `ltp` - The local tangent plane, (geodetic) origin (Ltp, LocalCartesian). `name` - Optional name (`str`). Raises: `TypeError` - Invalid `ltp`. `UnitError` - Invalid `azimuth`, `elevation` or or `slantrange`. Overrides: object.__init__

### toRepr (self, prec=None, fmt='[%s]', sep=', ', **unused) |
Return a string representation of this AER as azimuth (bearing), elevation and slant range. Arguments: `prec` - Optional number of decimals, unstripped (`int`). `fmt` - Optional enclosing backets format (`str`). `sep` - Optional separator between AERs (`str`). Returns: This AER as "[A:degrees360, E:degrees90, R:meter]" (`str`). Overrides: named._Named.toRepr

### toStr (self, prec=3, fmt='[%s]', sep=', ') |
Return a string representation of this ENU/NED/AER. Arguments: `prec` - Optional number of decimals, unstripped (`int`). `fmt` - Optional enclosing backets format (`str`). `sep` - Optional separator between NEDs (`str`). Returns: This AER as "[degrees360, degrees90, meter]" (`str`). Raises: `AssertionError` - Always, see function notOverloaded. Overrides: named._Named.toStr

### toXyz (self, Xyz=None, **Xyz_kwds) |
Get the local X, Y, Z (XYZ) components. Arguments: `Xyz` - Class to return XYZ (XyzLocal, Enu, Ned, Aer) or `None`. `Xyz_kwds` - Optional, additional `Xyz` keyword arguments, ignored if `Xyz=None`. Returns: XYZ as an `Xyz` instance or if `Xyz=None`, an Xyz4Tuple`(x, y, z, ltp)`. Raises: `TypeError` - Invalid `Xyz`.

Property Details

### aer4 Get the `(azimuth, elevation, slantrange, ltp)` components (Aer4Tuple). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### azimuth Get the Azimuth, bearing from North (`degrees360`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### down Get the Down component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### east Get the East component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### elevation Get the Elevation, tilt above horizon (`degrees90`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### groundrange Get the ground range, distance (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### ltp Get the local tangent plane (Ltp). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### north Get the North component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### slantrange Get the slant Range, distance (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### up Get the Up component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### x Get the X component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyz Get the local `(X, Y, Z)` coordinates (Vector3Tuple`(x, y, z)`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyz4 Get the `(x, y, z, ltp)` components (Xyz4Tuple). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### xyzLocal Get this AER as an XyzLocal. Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### y Get the Y component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)

### z Get the Z component (`meter`). Get method: _fget(inst) Set method: _fset_error(inst, val) - Throws an `AttributeError`, always. Delete Method: _fdel(inst)