Package pygeodesy :: Module lcc :: Class Conic |
[frames] | no frames]

# Class Conic

      object --+
               |
    named._Named --+
                   |
    named._NamedBase --+
                       |
    named._NamedEnumItem --+
                           |
                          Conic

Lambert conformal conic projection (1- or 2-SP).

Instance Methods
__init__(self, latlon0, par1, par2=None, E0=0, N0=0, k0=1, opt3=0, name=`'````'`, auth=`'````'`) New Lambert conformal conic projection. |
copy(self) Copy this conic. |
toDatum(self, datum) Convert this conic to the given datum. |
convertDatum(self, datum) Convert this conic to the given datum. |
toStr(self, prec=8) Return this conic as a string. |
Inherited from `named._NamedEnumItem`: `__ne__`, `unregister` Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others`, `toStr2` Inherited from `named._Named`: `__copy__`, `classof` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Class Variables
| _n_ = `0` (INTERNAL) Precomputed 1 / n.

Properties
| auth Get the authentication authority (`str`).
| datum Get the datum (Datum).
| E0 Get the false easting (`meter`).
| k0 Get scale factor (`float`).
| lat0 Get the origin latitude (`degrees90`).
| lon0 Get the central meridian (`degrees180`).
| N0 Get the false northing (`meter`).
| name2 Get the conic and datum names as "conic.datum" (`str`).
| par1 Get the 1st standard parallel (`degrees90`).
| par2 Get the 2nd standard parallel (`degrees90`).
| opt3 Get the optional meridian (`degrees180`).
| SP Get the number of standard parallels (`int`).
Inherited from `named._NamedEnumItem`: `name` Inherited from `named._Named`: `classname`, `classnaming`, `named`, `named2` Inherited from `object`: `__class__`

Method Details

### __init__(self, latlon0, par1, par2=None, E0=0, N0=0, k0=1, opt3=0, name=`'````'`, auth=`'````'`) (Constructor) |
New Lambert conformal conic projection. Parameters: `latlon0` - Origin with (ellipsoidal) datum (`LatLon`). `par1` - First standard parallel (`degrees90`). `par2` - Optional, second standard parallel (`degrees90`). `E0` - Optional, false easting (`meter`). `N0` - Optional, false northing (`meter`). `k0` - Optional scale factor (`scalar`). `opt3` - Optional meridian (`degrees180`). `name` - Optional name of the conic (`str`). `auth` - Optional authentication authority (`str`). Returns: A Lambert projection (Conic). Raises: `TypeError` - Non-ellipsoidal `latlon0`. Overrides: object.__init__ Example:
    >>> from pygeodesy import Conic, Datums, ellipsoidalNvector
    >>> ll0 = ellipsoidalNvector.LatLon(23, -96, datum=Datums.NAD27)
    >>> Snyder = Conic(ll0, 33, 45, E0=0, N0=0, name='Snyder')

### copy(self) |
Copy this conic. Returns: The copy, unregistered (Conic or subclass thereof). Overrides: named._Named.copy

### toDatum(self, datum) |
Convert this conic to the given datum. Parameters: `datum` - Ellipsoidal datum to use (Datum). Returns: Converted conic, unregistered (Conic). Raises: `TypeError` - Non-ellipsoidal `datum`.

### convertDatum(self, datum) |
Convert this conic to the given datum. Parameters: `datum` - Ellipsoidal datum to use (Datum). Returns: Converted conic, unregistered (Conic). Raises: `TypeError` - Non-ellipsoidal `datum`.

### toStr(self, prec=8) |
Return this conic as a string. Parameters: `prec` - Optional number of decimals, unstripped (`int`). Returns: Conic attributes (`str`). Overrides: named._Named.toStr

Property Details

### auth Get the authentication authority (`str`). Get Method: auth(self) - Get the authentication authority (`str`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### datum Get the datum (Datum). Get Method: datum(self) - Get the datum (Datum). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### E0 Get the false easting (`meter`). Get Method: E0(self) - Get the false easting (`meter`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### k0 Get scale factor (`float`). Get Method: k0(self) - Get scale factor (`float`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### lat0 Get the origin latitude (`degrees90`). Get Method: lat0(self) - Get the origin latitude (`degrees90`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### lon0 Get the central meridian (`degrees180`). Get Method: lon0(self) - Get the central meridian (`degrees180`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### N0 Get the false northing (`meter`). Get Method: N0(self) - Get the false northing (`meter`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### name2 Get the conic and datum names as "conic.datum" (`str`). Get Method: name2(self) - Get the conic and datum names as "conic.datum" (`str`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### par1 Get the 1st standard parallel (`degrees90`). Get Method: par1(self) - Get the 1st standard parallel (`degrees90`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### par2 Get the 2nd standard parallel (`degrees90`). Get Method: par2(self) - Get the 2nd standard parallel (`degrees90`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### opt3 Get the optional meridian (`degrees180`). Get Method: opt3(self) - Get the optional meridian (`degrees180`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.

### SP Get the number of standard parallels (`int`). Get Method: SP(self) - Get the number of standard parallels (`int`). Set Method: Read_Only(self, ignored) - Throws an `AttributeError`, always.