### Navigation

- index
- modules |
- FabIO v0.1.4 documentation »
- Module code »

# Source code for fabio.pixiimage

    """
    Author: Jon Wright, ESRF.
    """
    # Get ready for python3:
    from __future__ import with_statement, print_function

    __authors__ = ["Jon Wright", "Jérôme Kieffer"]
    __contact__ = "wright@esrf.fr"
    __license__ = "GPLv3+"
    __copyright__ = "European Synchrotron Radiation Facility, Grenoble, France"
    __version__ = "29 Oct 2013"

    import numpy
    import sys
    import os
    from .fabioimage import fabioimage

    class pixiimage(fabioimage):
        _need_a_seek_to_read = True

        def _readheader(self, infile):
            infile.seek(0)
            self.header = {}
            byt = infile.read(4)
            framesize = numpy.fromstring(byt, numpy.int32)
            if framesize == 243722:
                # life is good
                width = 476
                height = 512
                offset = 24
                self.header['framesize'] = framesize
                self.header['width'] = width
                self.header['height'] = height
                self.header['offset'] = offset
            else:
                print("Pixiimage, bad framesize: %s" % framesize)
                raise

        def read(self, fname, frame=None):
            if frame is None:
                frame = 0
            self.header = {}
            self.resetvals()
            infile = self._open(fname, "rb")
            self.sequencefilename = fname
            self._readheader(infile)
            self.nframes = os.path.getsize(fname) / 487448
            self._readframe(infile, frame)
            infile.close()
            return self

        def _makeframename(self):
            self.filename = "%s$%04d" % (self.sequencefilename,
                                         self.currentframe)

        def _readframe(self, filepointer, img_num):
            if (img_num > self.nframes or img_num < 0):
                raise Exception("Bad image number")
            imgstart = self.header['offset'] + img_num * (512 * 476 * 2 + 24)
            filepointer.seek(imgstart, 0)
            self.data = numpy.fromstring(filepointer.read(512 * 476 * 2),
                                          numpy.uint16)
            self.data.shape = self.header['height'], self.header['width']
            self.dim2, self.dim1 = self.data.shape
            self.currentframe = int(img_num)
            self._makeframename()

        def write(self, fname, force_type=numpy.uint16):
            raise Exception("Write is not implemented")

        def getframe(self, num):
            """
            Returns a frame as a new fabioimage object
            """
            if num < 0 or num > self.nframes:
                raise Exception("Requested frame number is out of range")
            # Do a deep copy of the header to make a new one
            newheader = {}
            for k in self.header.keys():
                newheader[k] = self.header[k]
            frame = pixiimage(header=newheader)
            frame.nframes = self.nframes
            frame.sequencefilename = self.sequencefilename
            infile = frame._open(self.sequencefilename, "rb")
            frame._readframe(infile, num)
            infile.close()
            return frame

        def next(self):
            """
            Get the next image in a series as a fabio image
            """
            if self.currentframe < (self.nframes - 1) and self.nframes > 1:
                return self.getframe(self.currentframe + 1)
            else:
                newobj = pixiimage()
                newobj.read(next_filename(
                    self.sequencefilename))
                return newobj

        def previous(self):
            """
            Get the previous image in a series as a fabio image
            """
            if self.currentframe > 0:
                return self.getframe(self.currentframe - 1)
            else:
                newobj = pixiimage()
                newobj.read(previous_filename(
                    self.sequencefilename))
                return newobj

    def demo(fname):
        i = pixiimage()
        i.read(fname)
        import pylab
        pylab.imshow(numpy.log(i.data))
        print("%s\t%s\t%s\ts" % (i.filename, i.data.max(), i.data.min(), i.data.mean()))
        pylab.title(i.filename)
        pylab.show()
        while 1:
            i = i.next()
            pylab.imshow(numpy.log(i.data))
            pylab.title(i.filename)
            pylab.show()
            raw_input()

    if __name__ == "__main__":
        import sys
        demo(sys.argv[1])

### Navigation

- index
- modules |
- FabIO v0.1.4 documentation »
- Module code »