Package pygeodesy :: Module ltp :: Class ChLVe |
[frames] | no frames]

# Class ChLVe

              object --+
                       |
                   _ChLV --+
                           |
      object --+           |
               |           |
    named._Named --+       |
                   |       |
    named._NamedBase --+   |
                       |   |
          LocalCartesian --+
                           |
                          ChLVe

Conversion between WGS84 geodetic and Swiss projection coordinates using the Ellipsoidal approximate formulas, pp 10-11 and Bolliger, J. pp 148-151 (also GGGS).

Note: Methods ChLVe.forward and ChLVe.reverse have an additional keyword argument `gamma=False` to approximate the meridian convergence. If `gamma=True` a 2-tuple `(t, gamma)` is returned with `t` the usual result (`ChLV9Tuple`) and `gamma`, the meridian convergence (decimal `degrees`). To convert `gamma` to `grades` or `gons`, use function pygeodesy.degrees2grades.

See Also: Older references.

Instance Methods
__init__(self, name=`'``Bern``'`) New Approximate WGS84-Swiss ChLVe converter, centered at Bern, Ch. |
forward(self, latlonh, lon=None, height=0, M=None, name='', gamma=False) Convert WGS84 geodetic to Swiss projection coordinates. |
reverse(self, enh_, n=None, h_=0, M=None, name='', gamma=False) Convert Swiss projection to WGS84 geodetic coordinates. |
Inherited from `LocalCartesian`: `__eq__`, `reset`, `toStr` Inherited from `named._NamedBase`: `__repr__`, `__str__`, `others`, `toRepr` Inherited from `named._Named`: `__imatmul__`, `__matmul__`, `__rmatmul__`, `attrs`, `classof`, `copy`, `dup`, `methodname`, `rename`, `toStr2` Inherited from `object`: `__delattr__`, `__format__`, `__getattribute__`, `__hash__`, `__new__`, `__reduce__`, `__reduce_ex__`, `__setattr__`, `__sizeof__`, `__subclasshook__`

Properties
Inherited from `LocalCartesian`: `M`, `datum`, `ecef`, `height0`, `lat0`, `latlonheight0`, `lon0` Inherited from `named._Named`: `classname`, `classnaming`, `iteration`, `name`, `named`, `named2`, `named3`, `named4`, `sizeof` Inherited from `object`: `__class__`

Method Details

### __init__ (self, name=`'``Bern``'`) (Constructor) |
New Approximate WGS84-Swiss ChLVe converter, centered at Bern, Ch. Arguments: `name` - Optional name (`str`), overriding `Bern.name`. Raises: `LocalError` - If `latlonh0` not `LatLon`, LatLon4Tuple, Ltp or Ecef9Tuple or `latlonh0`, `lon0` or `height0` invalid, non-`scalar`. `TypeError` - Invalid `ecef` or not EcefKarney. Overrides: object.__init__

### forward (self, latlonh, lon=None, height=0, M=None, name='', gamma=False) |
Convert WGS84 geodetic to Swiss projection coordinates. Arguments: `latlonh` - Either a `LatLon`, Ltp or `scalar` (geodetic) latitude (`degrees`). `lon` - Optional, `scalar` (geodetic) longitude for `scalar` `latlonh` (`degrees`). `height` - Optional, height, vertically above (or below) the surface of the ellipsoid (`meter`) for `scalar` `latlonh` and `lon`. `M` - If `True`, return the concatenated rotation EcefMatrix iff available for `ChLV` only, `None` otherwise (`bool`). `name` - Optional name (`str`). Returns: A ChLV9Tuple`(Y, X, h_, lat, lon, height, ltp, ecef, M)` with the unfalsed Swiss Y, X coordinates, Swiss h_ height, the given geodetic `lat`, `lon` and `height`, this `ChLV*` instance and `ecef` (Ecef9Tuple) at Bern, Ch and rotation matrix `M`. The returned `ltp` is this `ChLV`, `ChLVa` or `ChLVe` instance. Raises: `LocalError` - Invalid or non-`scalar` `latlonh`, `lon` or `height`. Overrides: LocalCartesian.forward (inherited documentation)

### reverse (self, enh_, n=None, h_=0, M=None, name='', gamma=False) |
Convert Swiss projection to WGS84 geodetic coordinates. Arguments: `enh_` - A Swiss projection (ChLV9Tuple) or the `scalar`, falsed Swiss E_LV95 or y_LV03 easting (`meter`). `n` - Falsed Swiss N_LV85 or x_LV03 northing for `scalar` `enh_` and `h_` (`meter`). `h_` - Swiss h' height for `scalar` `enh_` and `n` (`meter`). `M` - If `True`, return the concatenated rotation EcefMatrix iff available for `ChLV` only, `None` otherwise (`bool`). `name` - Optional name (`str`). Returns: A ChLV9Tuple`(Y, X, h_, lat, lon, height, ltp, ecef, M)` with the unfalsed Swiss Y, X coordinates, Swiss h_ height, the given geodetic `lat`, `lon` and `height`, this `ChLV*` instance and `ecef` (Ecef9Tuple) at Bern, Ch and rotation matrix `M`. The returned `ltp` is this `ChLV`, `ChLVa` or `ChLVe` instance. Raises: `LocalError` - Invalid or non-`scalar` `enh_`, `n` or `h_`. Overrides: LocalCartesian.reverse (inherited documentation)