Package pygeodesy :: Module elevations |
[frames] | no frames]

# Module elevations

Functions to obtain elevations and geoid heights thru web services, for (lat, lon) locations, currently limited to the Conterminous US (CONUS), see also module geoids, module heights classes and USGS10mElev.py.

macOS: If an `SSLCertVerificationError` occurs, especially this "[SSL: CERTIFICATE_VERIFY_FAILED] certificate verify failed: self "signed certificate in certificate chain ...", review this post for a remedy. From a Terminal window run: `"/Applications/Python X.Y/Install Certificates.command"`

Version: 19.11.05

Functions
elevation2(lat, lon, timeout=2.0) Get the geoid elevation at an `NAD83` to `NAVD88` location. |
geoidHeight2(lat, lon, model=0, timeout=2.0) Get the `NAVD88` geoid height at an `NAD83` location. |

Variables
| __all__ = `_ALL_LAZY.elevations`

Function Details

### elevation2(lat, lon, timeout=2.0) |
Get the geoid elevation at an `NAD83` to `NAVD88` location. Parameters: `lat` - Latitude (`degrees`). `lon` - Longitude (`degrees`). `timeout` - Optional, query timeout (seconds). Returns: An Elevation2Tuple`(elevation, data_source)` or (`None, error`) in case of errors. Note: The returned `elevation` is `None` if `lat` or `lon` is invalid or outside the `Conterminous US (CONUS)`, if conversion failed or if the query timed out. The `error` is the `HTTP-, IO-, SSL-, Type-, URL-` or `ValueError` as a string (`str`). See Also: USGS National Map, the FAQ, geoid.py, module geoids, classes GeoidG2012B, GeoidKarney and GeoidPGM.

### geoidHeight2(lat, lon, model=0, timeout=2.0) |
Get the `NAVD88` geoid height at an `NAD83` location. Parameters: `lat` - Latitude (`degrees`). `lon` - Longitude (`degrees`). `model` - Optional, geoid model ID (`int`). `timeout` - Optional, query timeout (seconds). Returns: An GeoidHeight2Tuple`(height, model_name)` or `(None, error`) in case of errors. Note: The returned `height` is `None` if `lat` or `lon` is invalid or outside the `Conterminous US (CONUS)`, if the `model` was invalid, if conversion failed or if the query timed out. The `error` is the `HTTP-, IO-, SSL-, Type-, URL-` or `ValueError` as a string (`str`). See Also: NOAA National Geodetic Survey, Geoid, USGS10mElev.py, module geoids, classes GeoidG2012B, GeoidKarney and GeoidPGM.